(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 25)
    (no_connects 1)
    (area 106.045 45.085 170.18 86.995)
    (thickness 1.6)
    (drawings 9)
    (tracks 79)
    (zones 0)
    (modules 15)
    (nets 25)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(Q1-Pad1)")
  (net 2 "Net-(U1-Pad3)")
  (net 3 "Net-(R3-Pad2)")
  (net 4 "Net-(R2-Pad2)")
  (net 5 "Net-(U2-Pad1)")
  (net 6 "Net-(U2-Pad4)")
  (net 7 "Net-(R4-Pad1)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 DC_ISO)
  (net 10 GND_ISO)
  (net 11 ARD_GND)
  (net 12 ARD_PWM)
  (net 13 ARD_PWR_LVL)
  (net 14 ARD_TEMP)
  (net 15 DC_GND)
  (net 16 DC_IN)
  (net 17 "Net-(U1-Pad2)")
  (net 18 "Net-(U1-Pad6)")
  (net 19 "Net-(U1-Pad8)")
  (net 20 "Net-(U3-Pad1)")
  (net 21 "Net-(U3-Pad4)")
  (net 22 "Net-(U3-Pad5)")
  (net 23 "Net-(U3-Pad8)")
  (net 24 "Net-(J3-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_PWR_LVL)
    (add_net ARD_TEMP)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net DC_ISO)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad8)")
  )

  (net_class Power ""
    (clearance 0.2)
    (trace_width 3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND_ISO)
    (add_net "Net-(J3-Pad1)")
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 592C7871) (tstamp 592C208A)
    (at 116.205 76.835 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R1 (at -1.905 -1.27 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_PWM))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592C750E) (tstamp 592C64CC)
    (at 137.16 77.47 90)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592AD9EF)
    (fp_text reference U3 (at 7.62 -2.54 90) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (ICL7667)" (at 2.54 -2.54 90) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U3-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(R3-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND_ISO))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U3-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U3-Pad5)"))
    (pad 6 thru_hole circle (at 7.62 5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 DC_ISO))
    (pad 7 thru_hole circle (at 7.62 2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(R4-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U3-Pad8)"))
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 592C8523) (tstamp 592C18AC)
    (at 128.27 60.96 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C1 (at -0.635 -3.81 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22uF (at 1 3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.65 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.55) (end 1 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.55) (end 1.04 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0.98) (end 1.04 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.549) (end 1.08 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 0.98) (end 1.08 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.548) (end 1.12 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 0.98) (end 1.12 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.546) (end 1.16 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 0.98) (end 1.16 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.543) (end 1.2 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 0.98) (end 1.2 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.539) (end 1.24 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.98) (end 1.24 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.535) (end 1.28 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.98) (end 1.28 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.531) (end 1.32 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.98) (end 1.32 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.525) (end 1.36 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.98) (end 1.36 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.519) (end 1.4 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.98) (end 1.4 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.513) (end 1.44 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.98) (end 1.44 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -2.506) (end 1.48 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.98) (end 1.48 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -2.498) (end 1.52 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.98) (end 1.52 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -2.489) (end 1.56 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.98) (end 1.56 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -2.48) (end 1.6 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.98) (end 1.6 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -2.47) (end 1.64 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.98) (end 1.64 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -2.46) (end 1.68 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.98) (end 1.68 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -2.448) (end 1.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.98) (end 1.721 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -2.436) (end 1.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.98) (end 1.761 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -2.424) (end 1.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.98) (end 1.801 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -2.41) (end 1.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.98) (end 1.841 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -2.396) (end 1.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.98) (end 1.881 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -2.382) (end 1.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.98) (end 1.921 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -2.366) (end 1.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.98) (end 1.961 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -2.35) (end 2.001 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.98) (end 2.001 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -2.333) (end 2.041 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.98) (end 2.041 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -2.315) (end 2.081 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.98) (end 2.081 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -2.296) (end 2.121 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.98) (end 2.121 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -2.276) (end 2.161 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.98) (end 2.161 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -2.256) (end 2.201 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.98) (end 2.201 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -2.234) (end 2.241 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.98) (end 2.241 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -2.212) (end 2.281 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.98) (end 2.281 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -2.189) (end 2.321 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.98) (end 2.321 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -2.165) (end 2.361 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.98) (end 2.361 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -2.14) (end 2.401 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.98) (end 2.401 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -2.113) (end 2.441 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.98) (end 2.441 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -2.086) (end 2.481 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.98) (end 2.481 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -2.058) (end 2.521 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.98) (end 2.521 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -2.028) (end 2.561 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.98) (end 2.561 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.997) (end 2.601 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.98) (end 2.601 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.965) (end 2.641 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.98) (end 2.641 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.932) (end 2.681 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.98) (end 2.681 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.897) (end 2.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.98) (end 2.721 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.861) (end 2.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.98) (end 2.761 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.823) (end 2.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 0.98) (end 2.801 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -1.783) (end 2.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 0.98) (end 2.841 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -1.742) (end 2.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 0.98) (end 2.881 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -1.699) (end 2.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 0.98) (end 2.921 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -1.654) (end 2.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 0.98) (end 2.961 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -1.606) (end 3.001 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -1.556) (end 3.041 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -1.504) (end 3.081 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.121 -1.448) (end 3.121 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.161 -1.39) (end 3.161 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.201 -1.327) (end 3.201 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.241 -1.261) (end 3.241 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.281 -1.189) (end 3.281 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.321 -1.112) (end 3.321 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.361 -1.028) (end 3.361 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.401 -0.934) (end 3.401 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.441 -0.829) (end 3.441 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.481 -0.707) (end 3.481 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.521 -0.559) (end 3.521 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.561 -0.354) (end 3.561 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.85) (end -1.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 2.85) (end 3.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end 3.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end -1.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1 0) (end -1.397436 -0.98) (angle 135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.397436 0.98) (angle -135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.397436 -0.98) (angle 44.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 DC_ISO))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 592C6D5E) (tstamp 592C18B2)
    (at 151.13 69.215 270)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (path /592ACBF5)
    (fp_text reference C2 (at -2.54 2.54 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220nF (at 7.5 4.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 7.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.5 -3.5) (end -1.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 3.5) (end 16.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 16.5 3.5) (end 16.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 16.5 -3.5) (end -1.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.56 -3.56) (end 16.56 -3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.56 3.56) (end 16.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.56 -3.56) (end -1.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.56 -3.56) (end 16.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -3.85) (end -1.85 3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 3.85) (end 16.85 3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.85 3.85) (end 16.85 -3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.85 -3.85) (end -1.85 -3.85) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 DC_ISO))
    (pad 2 thru_hole circle (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:TO254P470X990X1910-3P (layer F.Cu) (tedit 592C8530) (tstamp 592C18C5)
    (at 147.32 63.5 90)
    (descr "TO220, Molded, 3-Lead, Jedec Variation AB")
    (tags Transistor)
    (path /592BF9D4)
    (fp_text reference Q1 (at 6.985 -4.445 90) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value RFP12N10L (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -2.76 -3.15) (end 7.84 -3.15) (layer Dwgs.User) (width 0.05))
    (fp_line (start 7.84 -3.15) (end 7.84 2.05) (layer Dwgs.User) (width 0.05))
    (fp_line (start 7.84 2.05) (end -2.76 2.05) (layer Dwgs.User) (width 0.05))
    (fp_line (start -2.76 2.05) (end -2.76 -3.15) (layer Dwgs.User) (width 0.05))
    (fp_line (start -2.51 -2.9) (end 7.59 -2.9) (layer Dwgs.User) (width 0.1))
    (fp_line (start 7.59 -2.9) (end 7.59 1.8) (layer Dwgs.User) (width 0.1))
    (fp_line (start 7.59 1.8) (end -2.51 1.8) (layer Dwgs.User) (width 0.1))
    (fp_line (start -2.51 1.8) (end -2.51 -2.9) (layer Dwgs.User) (width 0.1))
    (fp_line (start -2.51 -1.63) (end -1.24 -2.9) (layer Dwgs.User) (width 0.1))
    (fp_line (start 7.59 1.8) (end 7.59 -2.9) (layer F.SilkS) (width 0.2))
    (fp_line (start 7.59 -2.9) (end -2.51 -2.9) (layer F.SilkS) (width 0.2))
    (fp_line (start -2.51 -2.9) (end -2.51 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.92 1.92) (drill 1.28) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.92 1.92) (drill 1.28) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J3-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.92 1.92) (drill 1.28) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND_ISO))
  )

  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 592C652C) (tstamp 592C18D1)
    (at 131.445 81.28 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (path /592AC85B)
    (fp_text reference R2 (at 15.24 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330 (at 6.35 2.66 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.85 -1.6) (end 1.85 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1.85 1.6) (end 10.85 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 10.85 1.6) (end 10.85 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 10.85 -1.6) (end 1.85 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.85 0) (layer F.Fab) (width 0.1))
    (fp_line (start 12.7 0) (end 10.85 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.79 -1.66) (end 1.79 1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.79 1.66) (end 10.91 1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.91 1.66) (end 10.91 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.91 -1.66) (end 1.79 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.79 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.72 0) (end 10.91 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.95) (end -1.05 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.95) (end 13.75 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.75 1.95) (end 13.75 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.75 -1.95) (end -1.05 -1.95) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 DC_ISO))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 592C6582) (tstamp 592C18D7)
    (at 133.985 81.28)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACAE5)
    (fp_text reference R3 (at -2.54 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4K7 (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 DC_ISO))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(R3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 592C8527) (tstamp 592C18DD)
    (at 133.35 60.325)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACDEB)
    (fp_text reference R4 (at -1.905 -0.635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4K7 (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 GND_ISO))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 592C7874) (tstamp 592C18E3)
    (at 140.97 64.135 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACE76)
    (fp_text reference R5 (at 9.525 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470 (at 3.81 1.86 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(R4-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592C8707) (tstamp 592C18FB)
    (at 121.92 57.785 270)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592C6117)
    (fp_text reference U1 (at 5.715 10.795 360) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (NME1212DC)" (at 0 0 270) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 15 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 DC_ISO))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND_ISO))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad8)"))
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592C77BA) (tstamp 592C1913)
    (at 121.285 76.835 90)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592ADB99)
    (fp_text reference U2 (at 5.08 10.16 90) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (6N317)" (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 ARD_GND))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 7.62 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND_ISO))
    (pad 6 thru_hole circle (at 7.62 5.08 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(R3-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(R2-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(R2-Pad2)"))
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0410_04x1.25mm_Straight (layer F.Cu) (tedit 592C8386) (tstamp 592C64AE)
    (at 111.125 71.755 270)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0410")
    (tags "connector molex picoblade")
    (path /592C94BD)
    (fp_text reference J1 (at 6.35 -1.905 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 1.875 -3.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2 -2.55) (end -2 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 1.6) (end 5.75 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 1.6) (end 5.75 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -2.55) (end -2 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -2.075) (end -1.5 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.125) (end 5.25 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start 5.25 1.125) (end 5.25 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start 5.25 -2.075) (end -1.5 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -2.225) (end -1.65 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 1.275) (end 5.4 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.4 1.275) (end 5.4 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.4 -2.225) (end -1.65 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.875 0.725) (end -1.1 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0.725) (end -1.1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.8) (end -1.1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.8) (end -1.1 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.675) (end 1.875 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.875 0.725) (end 4.85 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 0.725) (end 4.85 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 0) (end 5.05 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 0) (end 5.05 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.8) (end 4.85 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 -0.8) (end 4.85 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 -1.675) (end 1.875 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -1.9 0.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -0.9 1.525) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 1.875 -1.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 ARD_GND))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 ARD_PWM))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 ARD_PWR_LVL))
    (pad 4 thru_hole circle (at 3.75 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 ARD_TEMP))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410_04x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer F.Cu) (tedit 592C7857) (tstamp 592C64B4)
    (at 109.855 58.42 270)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (path /592C95DB)
    (fp_text reference J2 (at -2.54 1.27 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0.625 -3.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2 -2.55) (end -2 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 1.6) (end 3.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 1.6) (end 3.25 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 -2.55) (end -2 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -2.075) (end -1.5 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.125) (end 2.75 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 1.125) (end 2.75 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -2.075) (end -1.5 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -2.225) (end -1.65 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 1.275) (end 2.9 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 1.275) (end 2.9 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -2.225) (end -1.65 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.625 0.725) (end -1.1 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0.725) (end -1.1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.8) (end -1.1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.8) (end -1.1 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.675) (end 0.625 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.625 0.725) (end 2.35 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0.725) (end 2.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0) (end 2.55 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.55 0) (end 2.55 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.55 -0.8) (end 2.35 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 -0.8) (end 2.35 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 -1.675) (end 0.625 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -1.9 0.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -0.9 1.525) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0.625 -1.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 16 DC_IN))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 15 DC_GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 592CA092)
    (at 164.465 69.215)
    (path /592CA485)
    (fp_text reference J3 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DrainLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 592CA097)
    (at 165.1 57.785)
    (path /592CA834)
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SourceLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 10 GND_ISO))
  )

  (gr_arc (start 107.315 55.245) (end 106.68 55.245) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.315 85.725) (end 107.315 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 85.725) (end 168.275 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 55.245) (end 167.64 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 54.61) (end 167.64 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.275 85.725) (end 168.275 55.245) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.315 86.36) (end 167.64 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.68 55.245) (end 106.68 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.315 54.61) (end 166.37 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 140.97 64.135) (end 146.685 64.135) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 146.685 64.135) (end 147.32 63.5) (width 0.25) (layer F.Cu) (net 1) (tstamp 592C8BF7))
  (segment (start 126.365 69.215) (end 128.27 71.12) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 128.27 71.12) (end 133.35 71.12) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F5E))
  (segment (start 141.605 81.28) (end 141.605 80.645) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 141.605 80.645) (end 139.7 78.74) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F59))
  (segment (start 139.7 76.2) (end 139.7 77.47) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F61))
  (segment (start 134.62 71.12) (end 139.7 76.2) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F60))
  (segment (start 133.35 71.12) (end 134.62 71.12) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F5F))
  (segment (start 139.7 78.74) (end 139.7 77.47) (width 0.25) (layer F.Cu) (net 3) (tstamp 592C8F5A))
  (segment (start 121.285 69.215) (end 123.825 69.215) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 118.745 81.28) (end 112.395 81.28) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 119.38 67.31) (end 121.285 69.215) (width 0.25) (layer F.Cu) (net 4) (tstamp 592C8B81))
  (segment (start 111.125 67.31) (end 119.38 67.31) (width 0.25) (layer F.Cu) (net 4) (tstamp 592C8B7F))
  (segment (start 109.22 69.215) (end 111.125 67.31) (width 0.25) (layer F.Cu) (net 4) (tstamp 592C8B7D))
  (segment (start 109.22 77.47) (end 109.22 69.215) (width 0.25) (layer F.Cu) (net 4) (tstamp 592C8B7B))
  (segment (start 112.395 81.28) (end 109.22 77.47) (width 0.25) (layer F.Cu) (net 4) (tstamp 592C8B79))
  (segment (start 133.35 64.135) (end 133.985 64.135) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 133.985 64.135) (end 139.7 69.85) (width 0.25) (layer F.Cu) (net 7) (tstamp 592C8CA0))
  (segment (start 133.35 60.325) (end 133.35 64.135) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 116.205 69.215) (end 118.745 69.215) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 118.745 69.215) (end 126.365 76.835) (width 0.25) (layer F.Cu) (net 8) (tstamp 592C8B5C))
  (segment (start 128.27 60.96) (end 128.27 62.865) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 136.525 71.12) (end 140.97 71.12) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8F83))
  (segment (start 128.27 62.865) (end 136.525 71.12) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8F81))
  (segment (start 131.445 82.55) (end 132.08 83.185) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 132.08 83.185) (end 142.875 83.185) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8DEE))
  (segment (start 142.875 83.185) (end 143.51 82.55) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8DEF))
  (segment (start 143.51 82.55) (end 143.51 80.645) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8DF0))
  (segment (start 143.51 80.645) (end 140.97 78.105) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8DF1))
  (segment (start 140.97 78.105) (end 140.97 71.12) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8DF3))
  (segment (start 131.445 81.28) (end 133.985 81.28) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 131.445 81.28) (end 131.445 82.55) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 111.76 65.405) (end 114.3 65.405) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CD1))
  (segment (start 108.585 69.215) (end 111.76 65.405) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CCF))
  (segment (start 108.585 77.47) (end 108.585 69.215) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CCD))
  (segment (start 113.03 83.185) (end 108.585 77.47) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CCB))
  (segment (start 130.81 83.185) (end 113.03 83.185) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CCA))
  (segment (start 131.445 82.55) (end 130.81 83.185) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CC8))
  (segment (start 128.27 60.96) (end 128.27 61.595) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 140.97 71.12) (end 142.24 69.85) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8CAC))
  (segment (start 142.24 69.85) (end 142.24 69.215) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 149.86 67.945) (end 151.13 69.215) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8C24))
  (segment (start 143.51 67.945) (end 149.86 67.945) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8C22))
  (segment (start 142.24 69.215) (end 143.51 67.945) (width 0.25) (layer F.Cu) (net 9) (tstamp 592C8C21))
  (segment (start 165.1 57.785) (end 149.225 57.785) (width 3) (layer F.Cu) (net 10) (status 400000))
  (segment (start 139.7 66.04) (end 140.335 66.675) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C19))
  (segment (start 140.97 60.325) (end 140.97 60.96) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 140.97 60.96) (end 139.7 62.23) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C16))
  (segment (start 139.7 62.23) (end 139.7 66.04) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C17))
  (segment (start 140.97 60.325) (end 145.415 60.325) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 145.415 60.325) (end 147.32 58.42) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8BA6))
  (segment (start 126.27 60.96) (end 126.27 59.15) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 127 58.42) (end 147.32 58.42) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B92))
  (segment (start 126.27 59.15) (end 127 58.42) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B90))
  (segment (start 126.27 60.96) (end 126.27 66.58) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 126.27 66.58) (end 126.365 66.675) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B8D))
  (segment (start 119.38 65.405) (end 119.38 66.04) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 126.365 66.675) (end 128.905 69.215) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B89))
  (segment (start 120.015 66.675) (end 126.365 66.675) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B88))
  (segment (start 119.38 66.04) (end 120.015 66.675) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8B87))
  (segment (start 142.24 77.47) (end 142.875 77.47) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 149.62 84.215) (end 151.13 84.215) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8DE3))
  (segment (start 142.875 77.47) (end 149.62 84.215) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8DE2))
  (segment (start 140.335 66.675) (end 154.94 66.675) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C1A))
  (segment (start 155.575 79.77) (end 151.13 84.215) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C1D))
  (segment (start 155.575 67.31) (end 155.575 79.77) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C1C))
  (segment (start 154.94 66.675) (end 155.575 67.31) (width 0.25) (layer F.Cu) (net 10) (tstamp 592C8C1B))
  (segment (start 111.125 71.755) (end 118.745 71.755) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 118.745 71.755) (end 123.825 76.835) (width 0.25) (layer F.Cu) (net 11) (tstamp 592C8EFF))
  (segment (start 111.125 73.005) (end 112.375 73.005) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 112.375 73.005) (end 116.205 76.835) (width 0.25) (layer F.Cu) (net 12) (tstamp 592C8F03))
  (segment (start 109.855 59.67) (end 120.035 59.67) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 120.035 59.67) (end 121.92 57.785) (width 0.25) (layer F.Cu) (net 15) (tstamp 592C8B50))
  (segment (start 109.855 58.42) (end 113.665 58.42) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 113.665 58.42) (end 114.3 57.785) (width 0.25) (layer F.Cu) (net 16) (tstamp 592C8B4D))
  (segment (start 164.465 69.215) (end 163.195 69.215) (width 0.75) (layer F.Cu) (net 24))
  (segment (start 163.195 69.215) (end 150.495 61.595) (width 3) (layer F.Cu) (net 24) (tstamp 592CA19E))
  (segment (start 150.495 61.595) (end 147.32 60.96) (width 0.75) (layer F.Cu) (net 24) (tstamp 592CA1A1))

)
