(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 137)
    (no_connects 107)
    (area 31.674999 45.644999 138.505001 113.105001)
    (thickness 1.6)
    (drawings 15)
    (tracks 126)
    (zones 0)
    (modules 68)
    (nets 34)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.4)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 1)
    (uvia_drill 0.5)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 Earth)
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(C7-Pad2)")
  (net 5 "Net-(C10-Pad1)")
  (net 6 "Net-(C11-Pad2)")
  (net 7 "Net-(C13-Pad1)")
  (net 8 "Net-(C15-Pad2)")
  (net 9 "Net-(IC1-Pad2)")
  (net 10 "Net-(IC2-Pad2)")
  (net 11 "Net-(IC3-Pad2)")
  (net 12 "Net-(IC4-Pad2)")
  (net 13 DC_IN)
  (net 14 DC_GND)
  (net 15 ARD_TEMP)
  (net 16 ARD_GND)
  (net 17 "Net-(R2-Pad2)")
  (net 18 "Net-(R4-Pad2)")
  (net 19 "Net-(R6-Pad2)")
  (net 20 "Net-(R8-Pad2)")
  (net 21 "Net-(C20-Pad1)")
  (net 22 "Net-(C17-Pad1)")
  (net 23 "Net-(C19-Pad1)")
  (net 24 "Net-(C21-Pad1)")
  (net 25 "Net-(C23-Pad1)")
  (net 26 "Net-(R3-Pad1)")
  (net 27 "Net-(R5-Pad1)")
  (net 28 "Net-(R7-Pad1)")
  (net 29 "Net-(R9-Pad1)")
  (net 30 ARD_PWM_A)
  (net 31 ARD_PWM_B)
  (net 32 ARD_PWM_C)
  (net 33 ARD_PWM_D)

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 1)
    (uvia_drill 0.5)
    (add_net ARD_GND)
    (add_net ARD_PWM_A)
    (add_net ARD_PWM_B)
    (add_net ARD_PWM_C)
    (add_net ARD_PWM_D)
    (add_net ARD_TEMP)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net Earth)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC2-Pad2)")
    (add_net "Net-(IC3-Pad2)")
    (add_net "Net-(IC4-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 59A7ED15) (tstamp 59A7F116)
    (at 53.34 107.95)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 59A7ED1B) (tstamp 59A7F102)
    (at 124.46 107.95)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 59A7ED10) (tstamp 59A7F0FC)
    (at 121.92 45.72)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E9D7)
    (at 123.19 60.96)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A71299/59A6D3E0)
    (fp_text reference C10 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EF40)
    (at 96.52 81.28)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A712A3/59A6D3EA)
    (fp_text reference U7 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value NME1212DC (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 14 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 13 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C13-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R9-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EE9E)
    (at 55.88 81.28)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A7109E/59A6D3EA)
    (fp_text reference U3 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value NME1212DC (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 14 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 13 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C20-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R5-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EEEF)
    (at 93.98 50.8)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A71299/59A6D3EA)
    (fp_text reference U5 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value NME1212DC (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 14 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 13 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C10-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(R7-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EC7B)
    (at 107.95 92.71)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A712A3/59498139)
    (fp_text reference IC4 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value TC4422AVPA (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC4-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C15-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C15-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C23-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EC0D)
    (at 67.31 92.71)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A7109E/59498139)
    (fp_text reference IC2 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value TC4422AVPA (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC2-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C7-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C7-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C19-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EC44)
    (at 105.41 60.96)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59A71299/59498139)
    (fp_text reference IC3 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value TC4422AVPA (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC3-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C11-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C11-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C21-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EBD6)
    (at 67.31 66.04)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59498AA5/59498139)
    (fp_text reference IC1 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value TC4422AVPA (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C17-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 59A6EE4D)
    (at 55.88 55.88)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /59498AA5/59A6D3EA)
    (fp_text reference U1 (at 3.81 -2.286) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value NME1212DC (at 3.556 9.906) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start 0.508 8.7122) (end 0.508 -1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -1.1938) (end 7.112 -1.1938) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 3.048) (end 0.508 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 2.032) (end -0.4826 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 2.032) (end -0.4826 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 3.048) (end 0.508 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 1.5748) (end 7.112 0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 4.1148) (end 7.112 3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 6.0452) (end 0.508 6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 3.5052) (end 0.508 4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer F.SilkS) (width 0.1524))
    (fp_line (start 7.112 6.6548) (end 7.112 6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 1.0922) (end 0.508 1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start 0.508 0.508) (end 0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 -0.508) (end -0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 -0.508) (end -0.4826 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 0.508) (end 0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 5.588) (end 0.508 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 4.572) (end -0.4826 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 4.572) (end -0.4826 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 5.588) (end 0.508 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.128) (end 0.508 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 7.112) (end -0.4826 7.1374) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 7.1374) (end -0.4826 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.4826 8.128) (end 0.508 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 7.112) (end 7.112 8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.128) (end 8.1026 8.1026) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 8.1026) (end 8.1026 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 7.112) (end 7.112 7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 4.572) (end 7.112 5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 5.588) (end 8.1026 5.5626) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 5.5626) (end 8.1026 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 4.572) (end 7.112 4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 2.032) (end 7.112 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 3.048) (end 8.1026 3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 3.048) (end 8.1026 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 2.032) (end 7.112 2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 -0.508) (end 7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 0.508) (end 8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 0.508) (end 8.1026 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 8.1026 -0.508) (end 7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.508 8.7122) (end 7.112 8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 7.112 8.7122) (end 7.112 -1.0922) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 14 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 13 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R3-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6E764)
    (at 78.78 66.04)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59498AA5/59A6D3D9)
    (fp_text reference C1 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E777)
    (at 85.09 66.04)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59498AA5/59A6D3E0)
    (fp_text reference C2 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E78A)
    (at 78.78 73.66)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59498AA5/5949814D)
    (fp_text reference C3 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6E80F)
    (at 85.13 73.66)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59498AA5/59498146)
    (fp_text reference C4 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6E894)
    (at 78.78 92.71)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A7109E/59A6D3D9)
    (fp_text reference C5 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E8A7)
    (at 85.13 92.71)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A7109E/59A6D3E0)
    (fp_text reference C6 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E8BA)
    (at 78.78 100.33)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A7109E/5949814D)
    (fp_text reference C7 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6E93F)
    (at 85.13 100.33)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A7109E/59498146)
    (fp_text reference C8 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6E9C4)
    (at 116.84 60.96)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A71299/59A6D3D9)
    (fp_text reference C9 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6E9EA)
    (at 116.84 68.58)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A71299/5949814D)
    (fp_text reference C11 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6EA6F)
    (at 123.19 68.58)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A71299/59498146)
    (fp_text reference C12 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6EAF4)
    (at 120.69 92.71)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A712A3/59A6D3D9)
    (fp_text reference C13 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6EB07)
    (at 127.04 92.71)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A712A3/59A6D3E0)
    (fp_text reference C14 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59A6EB1A)
    (at 120.69 100.33)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A712A3/5949814D)
    (fp_text reference C15 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59A6EB9F)
    (at 127.04 100.33)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59A712A3/59498146)
    (fp_text reference C16 (at 1.25 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 59A6EC93)
    (at 44.6024 55.499 270)
    (tags RJ45)
    (path /59526541)
    (fp_text reference J1 (at 4.7 11.18 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 ARD_TEMP))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59A6ECBC)
    (at 42.037 80.518 180)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /599EAAF2)
    (fp_text reference J2 (at 1.25 -3.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Temperature Probe" (at 1.25 4.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59A6ECE5)
    (at 74.97 57.15)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59498AA5/595237FD)
    (fp_text reference J3 (at 1.25 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Drive Signal" (at 1.25 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59A6ED0E)
    (at 77.51 83.82)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59A7109E/595237FD)
    (fp_text reference J4 (at 1.25 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Drive Signal" (at 1.25 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59A6ED37)
    (at 113.07 52.07)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59A71299/595237FD)
    (fp_text reference J5 (at 1.25 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Drive Signal" (at 1.25 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59A6ED60)
    (at 115.61 83.82)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59A712A3/595237FD)
    (fp_text reference J6 (at 1.25 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Drive Signal" (at 1.25 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A6ED76)
    (at 34.29 73.66)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /599EAAF9)
    (fp_text reference R1 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 ARD_TEMP))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 DC_GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A6ED8C)
    (at 52.07 73.66 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59498AA5/59A6DA9F)
    (fp_text reference R2 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 180 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 ARD_PWM_A))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A6EDB4)
    (at 52.07 100.33 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A7109E/59A6DA9F)
    (fp_text reference R4 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 180 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 ARD_PWM_B))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A6EE04)
    (at 92.71 100.33 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A712A3/59A6DA9F)
    (fp_text reference R8 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 180 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 ARD_PWM_D))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 59A7E8CF)
    (at 44.6024 88.9 270)
    (tags RJ45)
    (path /59A7EBD8)
    (fp_text reference J7 (at 4.7 11.18 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 ARD_PWM_A))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 ARD_PWM_B))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 ARD_PWM_C))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 ARD_PWM_D))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 59A7ED08) (tstamp 59A7F0E0)
    (at 53.34 50.8)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF669F)
    (at 86.995 57.785)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59498AA5/59EF0ED7)
    (fp_text reference C17 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF66B2)
    (at 66.715 36.195)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59498AA5/59EF1DD4)
    (fp_text reference C18 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF66C5)
    (at 82.59 106.68)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A7109E/59EF0ED7)
    (fp_text reference C19 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF66D8)
    (at 86.995 83.82)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A7109E/59EF1DD4)
    (fp_text reference C20 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF66EB)
    (at 129.54 68.58)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A71299/59EF0ED7)
    (fp_text reference C21 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF66FE)
    (at 129.54 60.96)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A71299/59EF1DD4)
    (fp_text reference C22 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF6711)
    (at 129.58 83.82)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A712A3/59EF0ED7)
    (fp_text reference C23 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B) (tstamp 59EF6724)
    (at 123.23 83.82)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59A712A3/59EF1DD4)
    (fp_text reference C24 (at 1.25 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -0.770693 -1.18) (angle 119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.770693 1.18) (angle -119.4) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.270693 -1.18) (angle 60.6) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF678A)
    (at 75.565 34.29)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59498AA5/59EF0FC7)
    (fp_text reference R10 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF67A0)
    (at 68.58 48.26)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59498AA5/59EF1A58)
    (fp_text reference R11 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF67B6)
    (at 59.69 106.68)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A7109E/59EF0FC7)
    (fp_text reference R12 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(IC2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF67CC)
    (at 88.9 106.68)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A7109E/59EF1A58)
    (fp_text reference R13 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF67E2)
    (at 113.03 74.93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A71299/59EF0FC7)
    (fp_text reference R14 (at 3.81 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C21-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(IC3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF67F8)
    (at 116.84 74.93)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A71299/59EF1A58)
    (fp_text reference R15 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C11-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF680E)
    (at 101.6 106.68)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A712A3/59EF0FC7)
    (fp_text reference R16 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C23-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59EF6824)
    (at 134.62 101.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A712A3/59EF1A58)
    (fp_text reference R17 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C15-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59C78D6B) (tstamp 59EF683E)
    (at 56.515 69.85)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /59498AA5/59A6DAA6)
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value H11N1M (at 3.81 7.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 6.41) (end 6.46 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 6.41) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59C78D6B) (tstamp 59EF6858)
    (at 56.515 94.615)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /59A7109E/59A6DAA6)
    (fp_text reference U4 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value H11N1M (at 3.81 7.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 6.41) (end 6.46 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 6.41) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R4-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(IC2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59C78D6B) (tstamp 59EF6872)
    (at 94.615 64.135)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /59A71299/59A6DAA6)
    (fp_text reference U6 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value H11N1M (at 3.81 7.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 6.41) (end 6.46 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 6.41) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(IC3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59C78D6B) (tstamp 59EF688C)
    (at 97.155 95.25)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /59A712A3/59A6DAA6)
    (fp_text reference U8 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value H11N1M (at 3.81 7.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 6.41) (end 6.46 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 6.41) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC4-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59F0538A)
    (at 68.58 54.61 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59498AA5/59A6DAAD)
    (fp_text reference R3 (at 3.81 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3K (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59F053A0)
    (at 69.85 81.28 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A7109E/59A6DAAD)
    (fp_text reference R5 (at 3.81 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3K (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59F053B6)
    (at 106.68 50.8 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A71299/59A6DAAD)
    (fp_text reference R7 (at 3.81 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3K (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59F053CC)
    (at 109.22 81.28 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A712A3/59A6DAAD)
    (fp_text reference R9 (at 3.81 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3K (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59F05D37)
    (at 101.6 74.93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A71299/59A6DA9F)
    (fp_text reference R6 (at 3.81 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 180 (at 3.81 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 ARD_PWM_C))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5921392F) (tstamp 59F0CB1D)
    (at 81.28 52.07)
    (descr "D, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "D T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (path /59498AA5/59EF0E59)
    (fp_text reference D1 (at 2.54 -2.36) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Zener (at 2.54 2.36) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.94 -1.3) (end 0.94 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.94 1.3) (end 4.14 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.94 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.14 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.88 -1.18) (end 0.88 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 -1.36) (end 4.2 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 -1.36) (end 4.2 -1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.18) (end 0.88 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.36) (end 4.2 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 1.36) (end 4.2 1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.42 -1.36) (end 1.42 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -1.65) (end -1.25 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.65) (end 6.35 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.65) (end 6.35 -1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.65) (end -1.25 -1.65) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5921392F) (tstamp 59F0CB36)
    (at 72.39 106.68)
    (descr "D, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "D T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (path /59A7109E/59EF0E59)
    (fp_text reference D2 (at 2.54 -2.36) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Zener (at 2.54 2.36) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.94 -1.3) (end 0.94 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.94 1.3) (end 4.14 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.94 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.14 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.88 -1.18) (end 0.88 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 -1.36) (end 4.2 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 -1.36) (end 4.2 -1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.18) (end 0.88 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.36) (end 4.2 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 1.36) (end 4.2 1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.42 -1.36) (end 1.42 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -1.65) (end -1.25 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.65) (end 6.35 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.65) (end 6.35 -1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.65) (end -1.25 -1.65) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5921392F) (tstamp 59F0CB4F)
    (at 123.19 53.34)
    (descr "D, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "D T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (path /59A71299/59EF0E59)
    (fp_text reference D3 (at 2.54 -2.36) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Zener (at 2.54 2.36) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.94 -1.3) (end 0.94 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.94 1.3) (end 4.14 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.94 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.14 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.88 -1.18) (end 0.88 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 -1.36) (end 4.2 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 -1.36) (end 4.2 -1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.18) (end 0.88 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.36) (end 4.2 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 1.36) (end 4.2 1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.42 -1.36) (end 1.42 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -1.65) (end -1.25 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.65) (end 6.35 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.65) (end 6.35 -1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.65) (end -1.25 -1.65) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(C21-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5921392F) (tstamp 59F0CB68)
    (at 113.03 106.68)
    (descr "D, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "D T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (path /59A712A3/59EF0E59)
    (fp_text reference D4 (at 2.54 -2.36) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Zener (at 2.54 2.36) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.94 -1.3) (end 0.94 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.94 1.3) (end 4.14 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 1.3) (end 4.14 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.14 -1.3) (end 0.94 -1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.94 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.14 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.42 -1.3) (end 1.42 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start 0.88 -1.18) (end 0.88 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 -1.36) (end 4.2 -1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 -1.36) (end 4.2 -1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.18) (end 0.88 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 1.36) (end 4.2 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.2 1.36) (end 4.2 1.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.42 -1.36) (end 1.42 1.36) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -1.65) (end -1.25 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 1.65) (end 6.35 1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.65) (end 6.35 -1.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.65) (end -1.25 -1.65) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(C23-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 31.75 113.03) (end 138.43 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 31.75 105.41) (end 31.75 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 31.75 45.72) (end 31.75 50.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 45.72) (end 31.75 45.72) (layer Edge.Cuts) (width 0.15))
  (dimension 67.31 (width 0.3) (layer Dwgs.User)
    (gr_text "67.310 mm" (at 192.27932 71.177509 90) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 187.11932 37.522509) (xy 193.62932 37.522509)))
    (feature2 (pts (xy 187.11932 104.832509) (xy 193.62932 104.832509)))
    (crossbar (pts (xy 190.92932 104.832509) (xy 190.92932 37.522509)))
    (arrow1a (pts (xy 190.92932 37.522509) (xy 191.515741 38.649013)))
    (arrow1b (pts (xy 190.92932 37.522509) (xy 190.342899 38.649013)))
    (arrow2a (pts (xy 190.92932 104.832509) (xy 191.515741 103.706005)))
    (arrow2b (pts (xy 190.92932 104.832509) (xy 190.342899 103.706005)))
  )
  (dimension 100.33 (width 0.3) (layer Dwgs.User)
    (gr_text "100.330 mm" (at 83.79204 19.789583) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 133.95704 24.949583) (xy 133.95704 18.439583)))
    (feature2 (pts (xy 33.62704 24.949583) (xy 33.62704 18.439583)))
    (crossbar (pts (xy 33.62704 21.139583) (xy 133.95704 21.139583)))
    (arrow1a (pts (xy 133.95704 21.139583) (xy 132.830536 21.726004)))
    (arrow1b (pts (xy 133.95704 21.139583) (xy 132.830536 20.553162)))
    (arrow2a (pts (xy 33.62704 21.139583) (xy 34.753544 21.726004)))
    (arrow2b (pts (xy 33.62704 21.139583) (xy 34.753544 20.553162)))
  )
  (gr_text "© Enertechnos Ltd. 2017" (at 163.83 116.205) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (gr_text "Module Rev1" (at 179.054555 39.634405 90) (layer B.Cu)
    (effects (font (size 1 1) (thickness 0.25)) (justify mirror))
  )
  (gr_text "Module Rev1" (at 177.428955 39.634405 90) (layer F.Cu)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_line (start 138.43 45.72) (end 138.43 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 31.75 105.41) (end 31.75 50.8) (layer Edge.Cuts) (width 0.15))
  (gr_text "Switch 4" (at 109.22 78.74) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Switch 2" (at 68.58 78.74) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Switch 3" (at 106.68 48.26) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Switch 1" (at 68.58 53.34) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )

  (segment (start 124.46 74.93) (end 125.73 76.2) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 125.73 76.2) (end 125.73 83.82) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 132.04 60.96) (end 132.08 60.96) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 132.08 60.96) (end 132.08 68.58) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 132.08 68.58) (end 132.04 68.58) (width 1) (layer F.Cu) (net 2) (tstamp 59F0EDA2) (status 80000))
  (segment (start 125.69 68.58) (end 125.73 68.58) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 125.73 68.58) (end 125.73 71.12) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 125.73 71.12) (end 124.46 72.39) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 124.46 72.39) (end 124.46 74.93) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 116.84 68.58) (end 116.84 67.31) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 116.84 67.31) (end 118.11 66.04) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 118.11 66.04) (end 125.73 66.04) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 125.73 66.04) (end 125.73 68.58) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 125.73 68.58) (end 125.69 68.58) (width 1) (layer F.Cu) (net 2) (tstamp 59F0B2CA) (status 80000))
  (segment (start 125.69 68.58) (end 125.73 68.58) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 125.73 68.58) (end 127 67.31) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 127 67.31) (end 127 66.04) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 127 66.04) (end 132.08 66.04) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 132.08 66.04) (end 132.08 68.58) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 132.08 68.58) (end 132.04 68.58) (width 1) (layer B.Cu) (net 2) (tstamp 59F0AA7E) (status 80000))
  (segment (start 125.69 60.96) (end 125.73 60.96) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 125.73 60.96) (end 127 59.69) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 127 59.69) (end 127 58.42) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 127 58.42) (end 132.08 58.42) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 132.08 58.42) (end 132.08 60.96) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 132.08 60.96) (end 132.04 60.96) (width 1) (layer F.Cu) (net 2) (tstamp 59F099E7) (status 80000))
  (segment (start 125.69 60.96) (end 125.73 60.96) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 125.73 60.96) (end 125.73 63.5) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 125.73 63.5) (end 120.65 63.5) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 120.65 63.5) (end 120.65 62.23) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 120.65 62.23) (end 119.38 60.96) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 119.38 60.96) (end 119.34 60.96) (width 1) (layer B.Cu) (net 2) (tstamp 59F0919B) (status 80000))
  (segment (start 105.41 68.58) (end 104.14 68.58) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 104.14 68.58) (end 104.14 67.31) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 104.14 67.31) (end 102.87 67.31) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 102.87 67.31) (end 102.235 66.675) (width 1) (layer F.Cu) (net 2) (tstamp 59F0894D) (status 80000))
  (segment (start 113.03 68.58) (end 105.41 68.58) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 113.03 68.58) (end 116.84 68.58) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 119.34 60.96) (end 119.38 60.96) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 119.38 60.96) (end 119.38 58.42) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 119.38 58.42) (end 115.57 54.61) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 115.57 54.61) (end 115.57 52.07) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 129.54 60.96) (end 128.27 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 128.27 62.23) (end 128.27 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 128.27 63.5) (end 124.46 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.46 63.5) (end 124.46 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.46 62.23) (end 123.19 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 123.19 62.23) (end 123.19 60.96) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 123.19 60.96) (end 121.92 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 121.92 62.23) (end 121.92 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 121.92 63.5) (end 118.11 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 118.11 63.5) (end 116.84 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 116.84 62.23) (end 116.84 60.96) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 119.34 68.58) (end 119.38 68.58) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 119.38 68.58) (end 119.38 71.12) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 119.38 71.12) (end 116.84 73.66) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 116.84 73.66) (end 116.84 74.93) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 119.34 68.58) (end 123.19 68.58) (width 1) (layer B.Cu) (net 6) (status 80000))
  (segment (start 119.34 68.58) (end 119.38 68.58) (width 1) (layer B.Cu) (net 6) (status 80000))
  (segment (start 119.38 68.58) (end 119.38 66.04) (width 1) (layer B.Cu) (net 6) (status 80000))
  (segment (start 119.38 66.04) (end 113.03 66.04) (width 1) (layer B.Cu) (net 6) (status 80000))
  (segment (start 113.03 66.04) (end 113.03 63.5) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 113.03 63.5) (end 111.76 63.5) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 111.76 63.5) (end 110.49 62.23) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 110.49 62.23) (end 110.49 59.69) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 110.49 59.69) (end 113.03 57.15) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 113.03 57.15) (end 113.03 52.07) (width 1) (layer F.Cu) (net 6) (status 80000))
  (segment (start 113.03 52.07) (end 113.07 52.07) (width 1) (layer F.Cu) (net 6) (tstamp 59F08101) (status 80000))
  (segment (start 102.235 69.215) (end 102.87 69.85) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 102.87 69.85) (end 102.87 72.39) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 102.87 72.39) (end 105.41 74.93) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 105.41 63.5) (end 106.68 63.5) (width 1) (layer F.Cu) (net 11) (status 80000))
  (segment (start 106.68 63.5) (end 107.95 64.77) (width 1) (layer F.Cu) (net 11) (status 80000))
  (segment (start 107.95 64.77) (end 107.95 71.12) (width 1) (layer F.Cu) (net 11) (status 80000))
  (segment (start 107.95 71.12) (end 102.87 71.12) (width 1) (layer F.Cu) (net 11) (status 80000))
  (segment (start 102.87 71.12) (end 102.87 69.85) (width 1) (layer F.Cu) (net 11) (status 80000))
  (segment (start 102.87 69.85) (end 102.235 69.215) (width 1) (layer F.Cu) (net 11) (tstamp 59F0894F) (status 80000))
  (segment (start 96.52 88.9) (end 95.25 88.9) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 95.25 88.9) (end 91.44 85.09) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 91.44 85.09) (end 91.44 71.12) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 91.44 71.12) (end 92.71 69.85) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 92.71 69.85) (end 92.71 62.23) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 92.71 62.23) (end 93.98 60.96) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 93.98 60.96) (end 93.98 58.42) (width 1) (layer F.Cu) (net 13) (status 80000))
  (segment (start 96.52 81.28) (end 99.06 78.74) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 99.06 78.74) (end 99.06 62.23) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 99.06 62.23) (end 96.52 59.69) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 96.52 59.69) (end 96.52 52.07) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 96.52 52.07) (end 95.25 50.8) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 95.25 50.8) (end 93.98 50.8) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 94.615 64.135) (end 95.25 64.77) (width 1) (layer F.Cu) (net 19) (status 80000))
  (segment (start 95.25 64.77) (end 96.52 64.77) (width 1) (layer F.Cu) (net 19) (status 80000))
  (segment (start 96.52 64.77) (end 96.52 71.12) (width 1) (layer F.Cu) (net 19) (status 80000))
  (segment (start 96.52 71.12) (end 93.98 73.66) (width 1) (layer F.Cu) (net 19) (status 80000))
  (segment (start 93.98 73.66) (end 93.98 74.93) (width 1) (layer F.Cu) (net 19) (status 80000))
  (segment (start 123.19 53.34) (end 125.73 55.88) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 125.73 55.88) (end 134.62 55.88) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 134.62 55.88) (end 134.62 71.12) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 134.62 71.12) (end 130.81 71.12) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 130.81 71.12) (end 129.54 69.85) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 129.54 69.85) (end 129.54 68.58) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 113.03 74.93) (end 116.84 71.12) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 116.84 71.12) (end 133.35 71.12) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 133.35 71.12) (end 134.62 69.85) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 134.62 69.85) (end 134.62 59.69) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 134.62 59.69) (end 133.35 58.42) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 133.35 58.42) (end 113.03 58.42) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 113.03 58.42) (end 113.03 60.96) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 105.41 60.96) (end 104.14 60.96) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 104.14 60.96) (end 102.87 62.23) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 102.87 62.23) (end 102.87 64.77) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 102.87 64.77) (end 102.235 64.135) (width 1) (layer F.Cu) (net 24) (tstamp 59F0894E) (status 80000))
  (segment (start 113.03 60.96) (end 105.41 60.96) (width 1) (layer B.Cu) (net 24) (status 80000))
  (segment (start 105.41 60.96) (end 106.68 59.69) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 106.68 59.69) (end 106.68 58.42) (width 1) (layer F.Cu) (net 24) (status 80000))
  (segment (start 106.68 50.8) (end 104.14 53.34) (width 1) (layer B.Cu) (net 28) (status 80000))
  (segment (start 104.14 53.34) (end 101.6 53.34) (width 1) (layer B.Cu) (net 28) (status 80000))
  (segment (start 44.6024 93.98) (end 43.18 93.98) (width 1) (layer F.Cu) (net 32) (status 80000))
  (segment (start 43.18 93.98) (end 41.91 92.71) (width 1) (layer F.Cu) (net 32) (status 80000))
  (segment (start 41.91 92.71) (end 41.91 86.36) (width 1) (layer F.Cu) (net 32) (status 80000))
  (segment (start 41.91 86.36) (end 48.26 80.01) (width 1) (layer F.Cu) (net 32) (status 80000))
  (via (at 48.26 80.01) (size 1.5) (layers F.Cu B.Cu) (net 32) (status 80000))
  (segment (start 48.26 80.01) (end 50.8 77.47) (width 1) (layer B.Cu) (net 32) (status 80000))
  (segment (start 50.8 77.47) (end 96.52 77.47) (width 1) (layer B.Cu) (net 32) (status 80000))
  (segment (start 96.52 77.47) (end 99.06 74.93) (width 1) (layer B.Cu) (net 32) (status 80000))
  (segment (start 99.06 74.93) (end 101.6 74.93) (width 1) (layer B.Cu) (net 32) (status 80000))

)
