(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 26)
    (no_connects 3)
    (area 109.347619 85.014999 195.965239 125.961905)
    (thickness 1.6)
    (drawings 12)
    (tracks 69)
    (zones 0)
    (modules 15)
    (nets 17)
  )

  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory SVG/))
  )

  (net 0 "")
  (net 1 GND_ISO)
  (net 2 ARD_GND)
  (net 3 VCC_ISO)
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 ARD_PWM)
  (net 7 VCC)
  (net 8 "Net-(J4-Pad1)")
  (net 9 ARD_TEMP)
  (net 10 "Net-(R2-Pad2)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 GND)
  (net 13 "Net-(U2-Pad3)")
  (net 14 "Net-(U2-Pad6)")
  (net 15 "Net-(U3-Pad2)")
  (net 16 ARD_SRC_V)

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class Control ""
    (clearance 1)
    (trace_width 1)
    (via_dia 1.6)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GND_ISO)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad2)")
    (add_net VCC)
    (add_net VCC_ISO)
  )

  (net_class Power ""
    (clearance 1)
    (trace_width 3)
    (via_dia 4)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J4-Pad1)")
  )

  (net_class Signal ""
    (clearance 0.8)
    (trace_width 0.8)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_SRC_V)
    (add_net ARD_TEMP)
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5920C257) (tstamp 5935471D)
    (at 132.3 93.6 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /592EA608)
    (fp_text reference C1 (at 2.5 -3.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 3.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC_ISO))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module RS:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592AD99B) (tstamp 5935477B)
    (at 118.8 94.2)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592EC206)
    (fp_text reference U1 (at 0 0) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value NME1212DC (at 0 0) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND_ISO))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC_ISO))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  )

  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 59354723)
    (at 140.5 91.9 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C2 (at 1.25 -4.21 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 4.21 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.1 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.2) (end 1.25 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.2) (end 1.29 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.2) (end 1.33 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.198) (end 1.37 3.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.197) (end 1.41 3.197) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.194) (end 1.45 3.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.192) (end 1.49 3.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.188) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 3.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.185) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 3.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.18) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 3.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.176) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 3.176) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.17) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 3.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.165) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 3.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.158) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 3.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.152) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.144) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 3.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.137) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 3.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.128) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 3.128) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.119) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 3.119) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.11) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.1) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.09) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.079) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 3.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.067) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 3.067) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.055) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.042) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 3.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.029) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 3.029) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.015) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 3.015) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.001) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 3.001) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.986) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.97) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.954) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.937) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.919) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.919) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.901) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.901) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.882) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.863) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.843) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.843) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.822) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.822) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.8) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.778) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 2.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.755) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 2.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.731) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 2.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.706) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 2.706) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.681) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.654) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 2.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.627) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 2.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.599) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 2.599) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.57) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 2.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.54) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.51) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 2.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.478) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 2.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.445) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 2.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.411) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 2.411) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.375) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 2.375) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.339) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 2.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.301) (end 3.491 2.301) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.262) (end 3.531 2.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.222) (end 3.571 2.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.18) (end 3.611 2.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.137) (end 3.651 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.092) (end 3.691 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.045) (end 3.731 2.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -1.997) (end 3.771 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.946) (end 3.811 1.946) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.894) (end 3.851 1.894) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.839) (end 3.891 1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.781) (end 3.931 1.781) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.721) (end 3.971 1.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.658) (end 4.011 1.658) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.591) (end 4.051 1.591) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.52) (end 4.091 1.52) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.445) (end 4.131 1.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.364) (end 4.171 1.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.278) (end 4.211 1.278) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.184) (end 4.251 1.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.081) (end 4.291 1.081) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -0.966) (end 4.331 0.966) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.834) (end 4.371 0.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.676) (end 4.411 0.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.468) (end 4.451 0.468) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -3.5) (end -2.25 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 3.5) (end 4.75 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 3.5) (end 4.75 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.5) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.838236 -0.98) (angle 144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.838236 0.98) (angle -144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 4.338236 -0.98) (angle 35.2) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC_ISO))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5920C257) (tstamp 59354729)
    (at 143.3 98)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /592ACBF5)
    (fp_text reference C3 (at 2.5 -3.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 3.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC_ISO))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 5935472F)
    (at 147.5 117.4 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /592ED18A)
    (fp_text reference C4 (at 1.25 -4.21 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 4.21 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.1 0 540) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.2) (end 1.25 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.2) (end 1.29 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.2) (end 1.33 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.198) (end 1.37 3.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.197) (end 1.41 3.197) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.194) (end 1.45 3.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.192) (end 1.49 3.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.188) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 3.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.185) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 3.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.18) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 3.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.176) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 3.176) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.17) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 3.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.165) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 3.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.158) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 3.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.152) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.144) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 3.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.137) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 3.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.128) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 3.128) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.119) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 3.119) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.11) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.1) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.09) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.079) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 3.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.067) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 3.067) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.055) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.042) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 3.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.029) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 3.029) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.015) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 3.015) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.001) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 3.001) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.986) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.97) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.954) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.937) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.919) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.919) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.901) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.901) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.882) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.863) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.843) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.843) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.822) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.822) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.8) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.778) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 2.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.755) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 2.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.731) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 2.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.706) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 2.706) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.681) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.654) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 2.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.627) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 2.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.599) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 2.599) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.57) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 2.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.54) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.51) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 2.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.478) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 2.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.445) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 2.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.411) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 2.411) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.375) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 2.375) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.339) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 2.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.301) (end 3.491 2.301) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.262) (end 3.531 2.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.222) (end 3.571 2.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.18) (end 3.611 2.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.137) (end 3.651 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.092) (end 3.691 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.045) (end 3.731 2.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -1.997) (end 3.771 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.946) (end 3.811 1.946) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.894) (end 3.851 1.894) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.839) (end 3.891 1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.781) (end 3.931 1.781) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.721) (end 3.971 1.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.658) (end 4.011 1.658) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.591) (end 4.051 1.591) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.52) (end 4.091 1.52) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.445) (end 4.131 1.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.364) (end 4.171 1.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.278) (end 4.211 1.278) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.184) (end 4.251 1.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.081) (end 4.291 1.081) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -0.966) (end 4.331 0.966) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.834) (end 4.371 0.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.676) (end 4.411 0.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.468) (end 4.451 0.468) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -3.5) (end -2.25 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 3.5) (end 4.75 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 3.5) (end 4.75 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.5) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.838236 -0.98) (angle 144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.838236 0.98) (angle -144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 4.338236 -0.98) (angle 35.2) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 59354750)
    (at 188.5 95.9)
    (path /592CA485)
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DrainLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 59354755)
    (at 189.1 114)
    (path /592CA834)
    (fp_text reference J5 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SourceLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59354763)
    (at 136.6 115.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /5935695A)
    (fp_text reference R1 (at 3.81 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 ARD_TEMP))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59354769)
    (at 113.7 116 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R2 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 5935476F)
    (at 130.8 103.6 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ED01B)
    (fp_text reference R3 (at 2.54 -1.86 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4K7 (at 2.54 1.86 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 -0.8) (end 0.74 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.74 0.8) (end 4.34 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 0.8) (end 4.34 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 -0.8) (end 0.74 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.74 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.34 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.68 -0.86) (end 4.4 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.68 0.86) (end 4.4 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 6.05 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.15) (end 6.05 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC_ISO))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 58CC8E33) (tstamp 59354785)
    (at 118.5 106.5)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /592E7A66)
    (fp_text reference U2 (at 3.81 -2.39) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4N35 (at 3.81 7.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 6.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 6.47) (end 6.58 6.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 6.47) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 ARD_PWM))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad3)"))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad6)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:TC4422AVPA (layer F.Cu) (tedit 592E9A52) (tstamp 593547BC)
    (at 143.1 111.6)
    (descr DIP254P762X432-8)
    (tags "Integrated Circuit")
    (path /592E820A)
    (fp_text reference U3 (at -3.81 -9.906) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value TC4422AVPA (at -4.064 2.286) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -7.112 1.0922) (end -7.112 -8.7122) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -8.8138) (end -0.508 -8.8138) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -4.572) (end -7.112 -4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -5.588) (end -8.1026 -4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -5.588) (end -8.1026 -5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -4.572) (end -7.112 -5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -6.0452) (end -0.508 -6.6548) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.508 -3.5052) (end -0.508 -4.1148) (layer F.SilkS) (width 0.1524))
    (fp_line (start -7.112 -1.5748) (end -7.112 -0.9652) (layer F.SilkS) (width 0.1524))
    (fp_line (start -7.112 -4.1148) (end -7.112 -3.5052) (layer F.SilkS) (width 0.1524))
    (fp_line (start -7.112 1.0922) (end -0.508 1.0922) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.508 -0.9652) (end -0.508 -1.5748) (layer F.SilkS) (width 0.1524))
    (fp_line (start -7.112 -6.5278) (end -7.112 -6.0452) (layer F.SilkS) (width 0.1524))
    (fp_line (start -7.112 -7.112) (end -7.112 -8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -8.128) (end -8.1026 -8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -8.128) (end -8.1026 -7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -7.112) (end -7.112 -7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -2.032) (end -7.112 -3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -3.048) (end -8.1026 -3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -3.048) (end -8.1026 -2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -2.032) (end -7.112 -2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 0.508) (end -7.112 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 -0.508) (end -8.1026 -0.4826) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 -0.4826) (end -8.1026 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -8.1026 0.508) (end -7.112 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -0.508) (end -0.508 0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 0.508) (end 0.4826 0.4826) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 0.4826) (end 0.4826 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -0.508) (end -0.508 -0.508) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -3.048) (end -0.508 -2.032) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -2.032) (end 0.4826 -2.0574) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -2.0574) (end 0.4826 -3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -3.048) (end -0.508 -3.048) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -5.588) (end -0.508 -4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -4.572) (end 0.4826 -4.572) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -4.572) (end 0.4826 -5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -5.588) (end -0.508 -5.588) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -8.128) (end -0.508 -7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 -7.112) (end 0.4826 -7.112) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -7.112) (end 0.4826 -8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start 0.4826 -8.128) (end -0.508 -8.128) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -7.112 1.0922) (end -0.508 1.0922) (layer Dwgs.User) (width 0.1524))
    (fp_line (start -0.508 1.0922) (end -0.508 -8.7122) (layer Dwgs.User) (width 0.1524))
    (pad 1 thru_hole rect (at -7.62 -7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC_ISO))
    (pad 2 thru_hole circle (at -7.62 -5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U3-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at -7.62 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND_ISO))
    (pad 5 thru_hole circle (at 0 0 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND_ISO))
    (pad 6 thru_hole circle (at 0 -2.54 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)"))
    (pad 7 thru_hole circle (at 0 -5.08 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)"))
    (pad 8 thru_hole circle (at 0 -7.62 90) (size 1.4859 1.4859) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC_ISO))
  )

  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446) (tstamp 59354B6B)
    (at 134.2 120.2 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (path /59355101)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TEMP_PROBE (at 0 4.87 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 3.87) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD5446) (tstamp 59354B73)
    (at 121.12 120.2 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (path /592C94BD)
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ARD_CONN (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 8.95) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ARD_PWM))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 ARD_SRC_V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 ARD_TEMP))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446) (tstamp 59354B79)
    (at 113.8 99.2 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (path /592C95DB)
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DC_CONN (at 0 4.87 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 3.87) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (gr_arc (start 190.5 87.63) (end 190.5 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 121.92) (end 193.04 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190.5 121.92) (end 193.04 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 121.92) (end 113.03 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 87.63) (end 110.49 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 85.09) (end 190.5 85.09) (angle 90) (layer Edge.Cuts) (width 0.15) (tstamp 592EF4C2))
  (gr_line (start 113.03 124.46) (end 190.5 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 87.63) (end 110.49 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 114.1 88.4) (end 114.1 86.9) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 189.7 88.4) (end 188.2 88.4) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 189.6 121) (end 188.1 121) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 113.8 121.2) (end 113.8 119.7) (layer Edge.Cuts) (width 0.15))

  (segment (start 143.1 111.6) (end 143.1 117.300002) (width 1) (layer B.Cu) (net 1))
  (segment (start 143.1 117.300002) (end 145.699998 119.9) (width 1) (layer B.Cu) (net 1))
  (segment (start 145.699998 119.9) (end 146.36863 119.9) (width 1) (layer B.Cu) (net 1))
  (segment (start 146.36863 119.9) (end 147.5 119.9) (width 1) (layer B.Cu) (net 1))
  (segment (start 126.12 111.58) (end 124.98863 111.58) (width 1) (layer B.Cu) (net 1))
  (segment (start 123.819999 110.411369) (end 123.819999 104.420001) (width 1) (layer B.Cu) (net 1))
  (segment (start 124.98863 111.58) (end 123.819999 110.411369) (width 1) (layer B.Cu) (net 1))
  (segment (start 123.819999 104.420001) (end 125.870001 102.369999) (width 1) (layer B.Cu) (net 1))
  (segment (start 125.870001 102.369999) (end 126.42 101.82) (width 1) (layer B.Cu) (net 1))
  (segment (start 140.5 89.4) (end 142.300002 89.4) (width 1) (layer B.Cu) (net 1))
  (segment (start 142.300002 89.4) (end 148.3 95.399998) (width 1) (layer B.Cu) (net 1))
  (segment (start 148.3 95.399998) (end 148.3 96.86863) (width 1) (layer B.Cu) (net 1))
  (segment (start 148.3 96.86863) (end 148.3 98) (width 1) (layer B.Cu) (net 1))
  (segment (start 132.3 88.6) (end 139.7 88.6) (width 1) (layer B.Cu) (net 1))
  (segment (start 139.7 88.6) (end 140.5 89.4) (width 1) (layer B.Cu) (net 1))
  (segment (start 132.3 88.6) (end 129.1 88.6) (width 1) (layer B.Cu) (net 1))
  (segment (start 129.1 88.6) (end 124.369999 93.330001) (width 1) (layer B.Cu) (net 1))
  (segment (start 124.369999 93.330001) (end 124.369999 100.547816) (width 1) (layer B.Cu) (net 1))
  (segment (start 124.369999 100.547816) (end 125.642183 101.82) (width 1) (layer B.Cu) (net 1))
  (segment (start 125.642183 101.82) (end 126.42 101.82) (width 1) (layer B.Cu) (net 1))
  (segment (start 127.25137 111.58) (end 126.12 111.58) (width 1) (layer B.Cu) (net 1))
  (segment (start 135.48 111.6) (end 143.1 111.6) (width 1) (layer B.Cu) (net 1))
  (segment (start 126.12 111.58) (end 135.46 111.58) (width 1) (layer B.Cu) (net 1))
  (segment (start 135.46 111.58) (end 135.48 111.6) (width 1) (layer B.Cu) (net 1))
  (segment (start 113.7 116) (end 113.7 117.13137) (width 0.8) (layer B.Cu) (net 2))
  (segment (start 113.7 117.13137) (end 118.818631 122.250001) (width 0.8) (layer B.Cu) (net 2))
  (segment (start 118.818631 122.250001) (end 122.81208 122.250001) (width 0.8) (layer B.Cu) (net 2))
  (segment (start 122.81208 122.250001) (end 123.66 121.402081) (width 0.8) (layer B.Cu) (net 2))
  (segment (start 123.66 121.402081) (end 123.66 120.2) (width 0.8) (layer B.Cu) (net 2))
  (segment (start 132.3 93.6) (end 138.8 93.6) (width 1) (layer B.Cu) (net 3))
  (segment (start 138.8 93.6) (end 140.5 91.9) (width 1) (layer B.Cu) (net 3))
  (segment (start 126.42 96.74) (end 129.16 96.74) (width 1) (layer B.Cu) (net 3))
  (segment (start 129.16 96.74) (end 132.3 93.6) (width 1) (layer B.Cu) (net 3))
  (segment (start 126.42 96.74) (end 127.197817 96.74) (width 1) (layer B.Cu) (net 3))
  (segment (start 127.197817 96.74) (end 130.8 100.342183) (width 1) (layer B.Cu) (net 3))
  (segment (start 130.8 100.342183) (end 130.8 102.610051) (width 1) (layer B.Cu) (net 3))
  (segment (start 130.8 102.610051) (end 130.8 103.6) (width 1) (layer B.Cu) (net 3))
  (segment (start 143.1 103.98) (end 143.1 98.2) (width 1) (layer B.Cu) (net 3))
  (segment (start 143.1 98.2) (end 143.3 98) (width 1) (layer B.Cu) (net 3))
  (segment (start 135.48 103.98) (end 143.1 103.98) (width 1) (layer B.Cu) (net 3))
  (segment (start 130.8 103.6) (end 135.1 103.6) (width 1) (layer B.Cu) (net 3))
  (segment (start 135.1 103.6) (end 135.48 103.98) (width 1) (layer B.Cu) (net 3))
  (segment (start 143.1 109.06) (end 144.150689 109.06) (width 1) (layer B.Cu) (net 4))
  (segment (start 144.150689 109.06) (end 147.5 112.409311) (width 1) (layer B.Cu) (net 4))
  (segment (start 147.5 112.409311) (end 147.5 115.6) (width 1) (layer B.Cu) (net 4))
  (segment (start 147.5 115.6) (end 147.5 117.4) (width 1) (layer B.Cu) (net 4))
  (segment (start 136.74 120.2) (end 136.74 115.64) (width 1) (layer B.Cu) (net 5))
  (segment (start 136.74 115.64) (end 136.6 115.5) (width 1) (layer B.Cu) (net 5))
  (segment (start 121.12 120.2) (end 121.12 107.52) (width 0.8) (layer B.Cu) (net 6))
  (segment (start 121.12 107.52) (end 120.1 106.5) (width 0.8) (layer B.Cu) (net 6))
  (segment (start 120.1 106.5) (end 118.5 106.5) (width 0.8) (layer B.Cu) (net 6))
  (segment (start 113.8 99.2) (end 113.792 99.187) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 113.792 99.187) (end 116.459 101.854) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 116.459 101.854) (end 118.745 101.854) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 118.745 101.854) (end 118.8 101.82) (width 1) (layer B.Cu) (net 7) (tstamp 59356227) (status 80000))
  (segment (start 128.74 120.2) (end 128.74 115.74) (width 0.8) (layer B.Cu) (net 9))
  (segment (start 128.74 115.74) (end 128.98 115.5) (width 0.8) (layer B.Cu) (net 9))
  (segment (start 113.7 108.38) (end 113.665 108.331) (width 1) (layer B.Cu) (net 10) (status 80000))
  (segment (start 113.665 108.331) (end 114.427 109.093) (width 1) (layer B.Cu) (net 10) (status 80000))
  (segment (start 114.427 109.093) (end 118.491 109.093) (width 1) (layer B.Cu) (net 10) (status 80000))
  (segment (start 118.491 109.093) (end 118.5 109.04) (width 1) (layer B.Cu) (net 10) (tstamp 59356428) (status 80000))
  (segment (start 130.8 108.68) (end 126.48 108.68) (width 1) (layer B.Cu) (net 11))
  (segment (start 126.48 108.68) (end 126.12 109.04) (width 1) (layer B.Cu) (net 11))
  (segment (start 135.48 109.06) (end 131.18 109.06) (width 1) (layer B.Cu) (net 11))
  (segment (start 131.18 109.06) (end 130.8 108.68) (width 1) (layer B.Cu) (net 11))
  (segment (start 113.8 96.66) (end 113.792 96.647) (width 1) (layer B.Cu) (net 12) (status 80000))
  (segment (start 113.792 96.647) (end 116.205 94.234) (width 1) (layer B.Cu) (net 12) (status 80000))
  (segment (start 116.205 94.234) (end 118.745 94.234) (width 1) (layer B.Cu) (net 12) (status 80000))
  (segment (start 118.745 94.234) (end 118.8 94.2) (width 1) (layer B.Cu) (net 12) (tstamp 59356226) (status 80000))

)
