(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/BreakoutBoard/BreakoutBoard.sch)
    (date "29/08/2017 14:26:27")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source BreakoutBoard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J2)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EEF12))
    (comp (ref J4)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EF0F4))
    (comp (ref J3)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EF1B1))
    (comp (ref J5)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EF28B))
    (comp (ref J1)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EE011))
    (comp (ref P2)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EFF88))
    (comp (ref P1)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F28C2))
    (comp (ref P3)
      (value Analog)
      (footprint Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F5771))
    (comp (ref P5)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F76EC))
    (comp (ref P4)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F7708))
    (comp (ref P6)
      (value Analog)
      (footprint Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F771D))
    (comp (ref J6)
      (value ARD_GROUND)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F9F17))
    (comp (ref J7)
      (value CONTROL_DC)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599FA2FA)))
  (libparts
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_02X06)
      (description "Connector, double row, 02x06, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))))
    (libpart (lib conn) (part CONN_02X08)
      (description "Connector, double row, 02x08, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name "Net-(P5-Pad2)")
      (node (ref P5) (pin 2)))
    (net (code 2) (name "Net-(P5-Pad10)")
      (node (ref P5) (pin 10)))
    (net (code 3) (name "Net-(P5-Pad9)")
      (node (ref P5) (pin 9)))
    (net (code 4) (name "Net-(P5-Pad8)")
      (node (ref P5) (pin 8)))
    (net (code 5) (name "Net-(P5-Pad7)")
      (node (ref P5) (pin 7)))
    (net (code 6) (name "Net-(P5-Pad6)")
      (node (ref P5) (pin 6)))
    (net (code 7) (name "Net-(P5-Pad5)")
      (node (ref P5) (pin 5)))
    (net (code 8) (name "Net-(P5-Pad4)")
      (node (ref P5) (pin 4)))
    (net (code 9) (name "Net-(P5-Pad3)")
      (node (ref P5) (pin 3)))
    (net (code 10) (name "Net-(P5-Pad11)")
      (node (ref P5) (pin 11)))
    (net (code 11) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 30) (name "Net-(P5-Pad16)")
      (node (ref P5) (pin 16)))
    (net (code 31) (name "Net-(P5-Pad15)")
      (node (ref P5) (pin 15)))
    (net (code 32) (name "Net-(P5-Pad14)")
      (node (ref P5) (pin 14)))
    (net (code 33) (name "Net-(P5-Pad13)")
      (node (ref P5) (pin 13)))
    (net (code 34) (name "Net-(P5-Pad12)")
      (node (ref P5) (pin 12)))
    (net (code 36) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 44) (name "Net-(P3-Pad2)")
      (node (ref P3) (pin 2)))
    (net (code 52) (name "Net-(P3-Pad10)")
      (node (ref P3) (pin 10)))
    (net (code 59) (name "Net-(P3-Pad12)")
      (node (ref P3) (pin 12)))
    (net (code 60) (name "Net-(P3-Pad11)")
      (node (ref P3) (pin 11)))
    (net (code 62) (name "Net-(P3-Pad9)")
      (node (ref P3) (pin 9)))
    (net (code 63) (name "Net-(P3-Pad8)")
      (node (ref P3) (pin 8)))
    (net (code 64) (name "Net-(P3-Pad7)")
      (node (ref P3) (pin 7)))
    (net (code 65) (name "Net-(P3-Pad6)")
      (node (ref P3) (pin 6)))
    (net (code 66) (name "Net-(P3-Pad5)")
      (node (ref P3) (pin 5)))
    (net (code 67) (name "Net-(P3-Pad4)")
      (node (ref P3) (pin 4)))
    (net (code 68) (name "Net-(P3-Pad3)")
      (node (ref P3) (pin 3)))
    (net (code 69) (name "Net-(P6-Pad7)")
      (node (ref P6) (pin 7)))
    (net (code 70) (name "Net-(P6-Pad12)")
      (node (ref P6) (pin 12)))
    (net (code 71) (name "Net-(P6-Pad11)")
      (node (ref P6) (pin 11)))
    (net (code 72) (name "Net-(P6-Pad9)")
      (node (ref P6) (pin 9)))
    (net (code 73) (name "Net-(P6-Pad5)")
      (node (ref P6) (pin 5)))
    (net (code 74) (name "Net-(P6-Pad3)")
      (node (ref P6) (pin 3)))
    (net (code 75) (name ARD_TEMP_HB)
      (node (ref P6) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 76) (name "Net-(P6-Pad1)")
      (node (ref P6) (pin 1)))
    (net (code 77) (name DC_IN)
      (node (ref J2) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J7) (pin 2)))
    (net (code 78) (name DC_GND)
      (node (ref J2) (pin 2))
      (node (ref J3) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 79) (name ARD_GND)
      (node (ref J4) (pin 8))
      (node (ref J5) (pin 8))
      (node (ref J2) (pin 8))
      (node (ref J6) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref J3) (pin 8)))
    (net (code 80) (name "Net-(P4-Pad4)")
      (node (ref P4) (pin 4)))
    (net (code 81) (name "Net-(P4-Pad12)")
      (node (ref P4) (pin 12)))
    (net (code 82) (name "Net-(P4-Pad11)")
      (node (ref P4) (pin 11)))
    (net (code 83) (name "Net-(P4-Pad10)")
      (node (ref P4) (pin 10)))
    (net (code 84) (name "Net-(P4-Pad9)")
      (node (ref P4) (pin 9)))
    (net (code 85) (name "Net-(P4-Pad8)")
      (node (ref P4) (pin 8)))
    (net (code 86) (name "Net-(P4-Pad7)")
      (node (ref P4) (pin 7)))
    (net (code 87) (name "Net-(P4-Pad6)")
      (node (ref P4) (pin 6)))
    (net (code 88) (name "Net-(P4-Pad5)")
      (node (ref P4) (pin 5)))
    (net (code 89) (name "Net-(P4-Pad13)")
      (node (ref P4) (pin 13)))
    (net (code 90) (name "Net-(P4-Pad3)")
      (node (ref P4) (pin 3)))
    (net (code 91) (name "Net-(P4-Pad2)")
      (node (ref P4) (pin 2)))
    (net (code 92) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 97) (name "Net-(P1-Pad16)")
      (node (ref P1) (pin 16)))
    (net (code 98) (name "Net-(P4-Pad16)")
      (node (ref P4) (pin 16)))
    (net (code 99) (name "Net-(P4-Pad15)")
      (node (ref P4) (pin 15)))
    (net (code 100) (name "Net-(P4-Pad14)")
      (node (ref P4) (pin 14)))
    (net (code 101) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 102) (name ARD_TEMP_3)
      (node (ref J3) (pin 5))
      (node (ref P6) (pin 8)))
    (net (code 103) (name ARD_PWM_3)
      (node (ref J3) (pin 4))
      (node (ref P2) (pin 7)))
    (net (code 104) (name "Net-(J5-Pad7)")
      (node (ref J5) (pin 7)))
    (net (code 105) (name ARD_SRC_V)
      (node (ref J5) (pin 6))
      (node (ref J3) (pin 6))
      (node (ref J4) (pin 6))
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 6)))
    (net (code 106) (name ARD_TEMP_4)
      (node (ref J5) (pin 5))
      (node (ref P6) (pin 10)))
    (net (code 107) (name ARD_PWM_4)
      (node (ref J5) (pin 4))
      (node (ref P2) (pin 5)))
    (net (code 108) (name ARD_5V)
      (node (ref J3) (pin 3))
      (node (ref J1) (pin 3))
      (node (ref J4) (pin 3))
      (node (ref J5) (pin 3))
      (node (ref J2) (pin 3)))
    (net (code 109) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7)))
    (net (code 110) (name ARD_TEMP_1)
      (node (ref J2) (pin 5))
      (node (ref P6) (pin 4)))
    (net (code 111) (name ARD_PWM_1)
      (node (ref P2) (pin 11))
      (node (ref J2) (pin 4)))
    (net (code 112) (name ARD_TEMP_2)
      (node (ref J4) (pin 5))
      (node (ref P6) (pin 6)))
    (net (code 113) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7)))
    (net (code 114) (name ARD_PWM_2)
      (node (ref P2) (pin 9))
      (node (ref J4) (pin 4)))
    (net (code 115) (name "Net-(P1-Pad7)")
      (node (ref P1) (pin 7)))
    (net (code 116) (name "Net-(P1-Pad15)")
      (node (ref P1) (pin 15)))
    (net (code 117) (name "Net-(P1-Pad14)")
      (node (ref P1) (pin 14)))
    (net (code 118) (name "Net-(P1-Pad13)")
      (node (ref P1) (pin 13)))
    (net (code 119) (name "Net-(P1-Pad12)")
      (node (ref P1) (pin 12)))
    (net (code 120) (name "Net-(P1-Pad11)")
      (node (ref P1) (pin 11)))
    (net (code 121) (name "Net-(P1-Pad10)")
      (node (ref P1) (pin 10)))
    (net (code 122) (name "Net-(P1-Pad9)")
      (node (ref P1) (pin 9)))
    (net (code 123) (name "Net-(P1-Pad8)")
      (node (ref P1) (pin 8)))
    (net (code 124) (name "Net-(P1-Pad6)")
      (node (ref P1) (pin 6)))
    (net (code 125) (name "Net-(P1-Pad5)")
      (node (ref P1) (pin 5)))
    (net (code 126) (name "Net-(P1-Pad4)")
      (node (ref P1) (pin 4)))
    (net (code 127) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3)))
    (net (code 128) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2)))
    (net (code 129) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 130) (name "Net-(P2-Pad6)")
      (node (ref P2) (pin 6)))
    (net (code 131) (name "Net-(P2-Pad4)")
      (node (ref P2) (pin 4)))
    (net (code 132) (name "Net-(P2-Pad3)")
      (node (ref P2) (pin 3)))
    (net (code 133) (name "Net-(P2-Pad2)")
      (node (ref P2) (pin 2)))
    (net (code 134) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 135) (name ARD_PWM_B)
      (node (ref P2) (pin 13))
      (node (ref J1) (pin 6)))
    (net (code 136) (name ARD_PWM_A)
      (node (ref P2) (pin 15))
      (node (ref J1) (pin 4)))
    (net (code 137) (name "Net-(P2-Pad8)")
      (node (ref P2) (pin 8)))
    (net (code 138) (name "Net-(P2-Pad10)")
      (node (ref P2) (pin 10)))
    (net (code 139) (name "Net-(P2-Pad12)")
      (node (ref P2) (pin 12)))
    (net (code 140) (name "Net-(P2-Pad14)")
      (node (ref P2) (pin 14)))
    (net (code 141) (name "Net-(P2-Pad16)")
      (node (ref P2) (pin 16)))))