(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 7)
    (no_connects 4)
    (area 120.312199 84.8716 183.581 141.1528)
    (thickness 1.6)
    (drawings 0)
    (tracks 26)
    (zones 0)
    (modules 6)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 1)
    (uvia_drill 0.5)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND_ISO)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad3)")
  (net 5 DRV_GATE)

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 1)
    (uvia_drill 0.5)
    (add_net DRV_GATE)
    (add_net GND_ISO)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
  )

  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer B.Cu) (tedit 58CE52AE) (tstamp 59AEC147)
    (at 142.237292 102.107022)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (path /59AEBE37)
    (fp_text reference D1 (at 5.45 3.45) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value PWR_DIODE (at 5.45 -6.07) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 5.45 3.45) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.5 2.33) (end -2.5 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start -2.5 -2.7) (end 13.4 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start 13.4 -2.7) (end 13.4 2.33) (layer B.Fab) (width 0.1))
    (fp_line (start 13.4 2.33) (end -2.5 2.33) (layer B.Fab) (width 0.1))
    (fp_line (start 3.645 2.33) (end 3.645 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start 7.255 2.33) (end 7.255 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start -2.62 2.451) (end 13.52 2.451) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.62 -2.82) (end 13.52 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.62 2.451) (end -2.62 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 13.52 2.451) (end 13.52 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.646 2.451) (end 3.646 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 7.255 2.451) (end 7.255 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.75 2.59) (end -2.75 -2.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.75 -2.95) (end 13.65 -2.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 13.65 -2.95) (end 13.65 2.59) (layer B.CrtYd) (width 0.05))
    (fp_line (start 13.65 2.59) (end -2.75 2.59) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole oval (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 59AEC14D)
    (at 123.6872 113.03)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59AEBE3C)
    (fp_text reference J1 (at 1.25 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Control (at 1.25 4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 5 DRV_GATE))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer B.Cu) (tedit 58CE52AE) (tstamp 59AEC15E)
    (at 124.990692 102.056222)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (path /59AEBE38)
    (fp_text reference Q1 (at -0.9906 3.556) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value RFP12N10L (at 5.45 -6.07) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at -0.9906 3.556) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.5 2.33) (end -2.5 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start -2.5 -2.7) (end 13.4 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start 13.4 -2.7) (end 13.4 2.33) (layer B.Fab) (width 0.1))
    (fp_line (start 13.4 2.33) (end -2.5 2.33) (layer B.Fab) (width 0.1))
    (fp_line (start 3.645 2.33) (end 3.645 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start 7.255 2.33) (end 7.255 -2.7) (layer B.Fab) (width 0.1))
    (fp_line (start -2.62 2.451) (end 13.52 2.451) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.62 -2.82) (end 13.52 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.62 2.451) (end -2.62 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 13.52 2.451) (end 13.52 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.646 2.451) (end 3.646 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 7.255 2.451) (end 7.255 -2.82) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.75 2.59) (end -2.75 -2.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.75 -2.95) (end 13.65 -2.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start 13.65 -2.95) (end 13.65 2.59) (layer B.CrtYd) (width 0.05))
    (fp_line (start 13.65 2.59) (end -2.75 2.59) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 DRV_GATE))
    (pad 2 thru_hole oval (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 thru_hole oval (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59AEEBFE)
    (at 134.3914 108.585 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /59AEBE39)
    (fp_text reference C1 (at 1.25 -3.81 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59AECA0D) (tstamp 59AEF5D7)
    (at 130.429 90.2716)
    (path /59AEBE3B)
    (fp_text reference J2 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DRN (at 0 6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 10 10) (drill 4.3) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59AECA0D) (tstamp 59AEF5DC)
    (at 178.181 133.5278)
    (path /59AEBE3A)
    (fp_text reference J3 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SRC (at 0 6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 10 10) (drill 4.3) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )

  (segment (start 135.890692 102.056222) (end 142.186492 102.056222) (width 5) (layer F.Cu) (net 1))
  (segment (start 142.186492 102.056222) (end 142.237292 102.107022) (width 5) (layer F.Cu) (net 1))
  (segment (start 135.890692 102.056222) (end 135.89 102.108) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 135.89 102.108) (end 134.366 103.632) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 134.366 103.632) (end 134.366 108.585) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 134.366 108.585) (end 134.3914 108.585) (width 1) (layer F.Cu) (net 1) (tstamp 59AEFF11) (status 80000))
  (segment (start 142.237292 102.107022) (end 142.24 102.108) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 135.89 102.108) (end 135.890692 102.056222) (width 1) (layer B.Cu) (net 1) (tstamp 59AEFF10) (status 80000))
  (segment (start 130.429 90.2716) (end 130.429 102.04453) (width 5) (layer F.Cu) (net 2))
  (segment (start 130.429 102.04453) (end 130.440692 102.056222) (width 5) (layer F.Cu) (net 2))
  (segment (start 130.440692 102.056222) (end 130.429 102.108) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 130.440692 102.056222) (end 130.429 102.108) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 130.429 102.108) (end 131.953 103.632) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 131.953 103.632) (end 131.953 108.585) (width 1) (layer F.Cu) (net 2) (status 80000))
  (segment (start 131.953 108.585) (end 131.8914 108.585) (width 1) (layer F.Cu) (net 2) (tstamp 59AEFF12) (status 80000))
  (segment (start 147.687292 133.514092) (end 147.701 133.5278) (width 5) (layer F.Cu) (net 3))
  (segment (start 147.701 133.5278) (end 178.181 133.5278) (width 5) (layer F.Cu) (net 3))
  (segment (start 147.687292 102.107022) (end 147.687292 133.514092) (width 5) (layer F.Cu) (net 3))
  (segment (start 123.6872 113.03) (end 123.698 113.03) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 123.698 113.03) (end 124.46 112.268) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.46 112.268) (end 124.46 112.141) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.46 112.141) (end 124.714 111.887) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.714 111.887) (end 124.714 111.76) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.714 111.76) (end 124.968 111.506) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.968 111.506) (end 124.968 102.108) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 124.968 102.108) (end 124.990692 102.056222) (width 1) (layer F.Cu) (net 5) (tstamp 59AEFF13) (status 80000))

)
