(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 35)
    (no_connects 31)
    (area 23 25 282 191)
    (thickness 1.6)
    (drawings 8)
    (tracks 18)
    (zones 0)
    (modules 13)
    (nets 98)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 DC_IN)
  (net 2 DC_GND)
  (net 3 ARD_5V)
  (net 4 ARD_PWM_A)
  (net 5 ARD_TEMP_HB)
  (net 6 ARD_PWM_B)
  (net 7 ARD_SRC_V)
  (net 8 ARD_GND)
  (net 9 ARD_PWM_1)
  (net 10 ARD_TEMP_1)
  (net 11 "Net-(J2-Pad7)")
  (net 12 ARD_PWM_3)
  (net 13 ARD_TEMP_3)
  (net 14 "Net-(J3-Pad7)")
  (net 15 ARD_PWM_2)
  (net 16 ARD_TEMP_2)
  (net 17 "Net-(J4-Pad7)")
  (net 18 ARD_PWM_4)
  (net 19 ARD_TEMP_4)
  (net 20 "Net-(J5-Pad7)")
  (net 21 "Net-(P1-Pad1)")
  (net 22 "Net-(P1-Pad2)")
  (net 23 "Net-(P1-Pad3)")
  (net 24 "Net-(P1-Pad4)")
  (net 25 "Net-(P1-Pad5)")
  (net 26 "Net-(P1-Pad6)")
  (net 27 "Net-(P1-Pad7)")
  (net 28 "Net-(P1-Pad8)")
  (net 29 "Net-(P1-Pad9)")
  (net 30 "Net-(P1-Pad10)")
  (net 31 "Net-(P1-Pad11)")
  (net 32 "Net-(P1-Pad12)")
  (net 33 "Net-(P1-Pad13)")
  (net 34 "Net-(P1-Pad14)")
  (net 35 "Net-(P1-Pad15)")
  (net 36 "Net-(P1-Pad16)")
  (net 37 "Net-(P2-Pad1)")
  (net 38 "Net-(P2-Pad2)")
  (net 39 "Net-(P2-Pad3)")
  (net 40 "Net-(P2-Pad4)")
  (net 41 "Net-(P2-Pad6)")
  (net 42 "Net-(P2-Pad8)")
  (net 43 "Net-(P2-Pad10)")
  (net 44 "Net-(P2-Pad12)")
  (net 45 "Net-(P2-Pad14)")
  (net 46 "Net-(P2-Pad16)")
  (net 47 "Net-(P3-Pad1)")
  (net 48 "Net-(P3-Pad2)")
  (net 49 "Net-(P3-Pad3)")
  (net 50 "Net-(P3-Pad4)")
  (net 51 "Net-(P3-Pad5)")
  (net 52 "Net-(P3-Pad6)")
  (net 53 "Net-(P3-Pad7)")
  (net 54 "Net-(P3-Pad8)")
  (net 55 "Net-(P3-Pad9)")
  (net 56 "Net-(P3-Pad10)")
  (net 57 "Net-(P3-Pad11)")
  (net 58 "Net-(P3-Pad12)")
  (net 59 "Net-(P4-Pad1)")
  (net 60 "Net-(P4-Pad2)")
  (net 61 "Net-(P4-Pad3)")
  (net 62 "Net-(P4-Pad4)")
  (net 63 "Net-(P4-Pad5)")
  (net 64 "Net-(P4-Pad6)")
  (net 65 "Net-(P4-Pad7)")
  (net 66 "Net-(P4-Pad8)")
  (net 67 "Net-(P4-Pad9)")
  (net 68 "Net-(P4-Pad10)")
  (net 69 "Net-(P4-Pad11)")
  (net 70 "Net-(P4-Pad12)")
  (net 71 "Net-(P4-Pad13)")
  (net 72 "Net-(P4-Pad14)")
  (net 73 "Net-(P4-Pad15)")
  (net 74 "Net-(P4-Pad16)")
  (net 75 "Net-(P5-Pad1)")
  (net 76 "Net-(P5-Pad2)")
  (net 77 "Net-(P5-Pad3)")
  (net 78 "Net-(P5-Pad4)")
  (net 79 "Net-(P5-Pad5)")
  (net 80 "Net-(P5-Pad6)")
  (net 81 "Net-(P5-Pad7)")
  (net 82 "Net-(P5-Pad8)")
  (net 83 "Net-(P5-Pad9)")
  (net 84 "Net-(P5-Pad10)")
  (net 85 "Net-(P5-Pad11)")
  (net 86 "Net-(P5-Pad12)")
  (net 87 "Net-(P5-Pad13)")
  (net 88 "Net-(P5-Pad14)")
  (net 89 "Net-(P5-Pad15)")
  (net 90 "Net-(P5-Pad16)")
  (net 91 "Net-(P6-Pad1)")
  (net 92 "Net-(P6-Pad3)")
  (net 93 "Net-(P6-Pad5)")
  (net 94 "Net-(P6-Pad7)")
  (net 95 "Net-(P6-Pad9)")
  (net 96 "Net-(P6-Pad11)")
  (net 97 "Net-(P6-Pad12)")

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_5V)
    (add_net ARD_GND)
    (add_net ARD_PWM_1)
    (add_net ARD_PWM_2)
    (add_net ARD_PWM_3)
    (add_net ARD_PWM_4)
    (add_net ARD_PWM_A)
    (add_net ARD_PWM_B)
    (add_net ARD_SRC_V)
    (add_net ARD_TEMP_1)
    (add_net ARD_TEMP_2)
    (add_net ARD_TEMP_3)
    (add_net ARD_TEMP_4)
    (add_net ARD_TEMP_HB)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad12)")
    (add_net "Net-(P2-Pad14)")
    (add_net "Net-(P2-Pad16)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad10)")
    (add_net "Net-(P4-Pad11)")
    (add_net "Net-(P4-Pad12)")
    (add_net "Net-(P4-Pad13)")
    (add_net "Net-(P4-Pad14)")
    (add_net "Net-(P4-Pad15)")
    (add_net "Net-(P4-Pad16)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P4-Pad9)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad11)")
    (add_net "Net-(P5-Pad12)")
    (add_net "Net-(P5-Pad13)")
    (add_net "Net-(P5-Pad14)")
    (add_net "Net-(P5-Pad15)")
    (add_net "Net-(P5-Pad16)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P5-Pad7)")
    (add_net "Net-(P5-Pad8)")
    (add_net "Net-(P5-Pad9)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad11)")
    (add_net "Net-(P6-Pad12)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(P6-Pad7)")
    (add_net "Net-(P6-Pad9)")
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 599EFD13)
    (at 266.27 45.82 90)
    (tags RJ45)
    (path /599EE011)
    (fp_text reference J1 (at 4.7 11.18 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 ARD_PWM_A))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 ARD_TEMP_HB))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 ARD_PWM_B))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_SRC_V))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 599EFD2B)
    (at 266.27 65.4925 90)
    (tags RJ45)
    (path /599EEF12)
    (fp_text reference J2 (at 4.7 11.18 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 ARD_PWM_1))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 ARD_TEMP_1))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_SRC_V))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 599EFD43)
    (at 266.27 85.165 90)
    (tags RJ45)
    (path /599EF1B1)
    (fp_text reference J3 (at 4.7 11.18 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 ARD_PWM_3))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 ARD_TEMP_3))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_SRC_V))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 599EFD5B)
    (at 266.27 104.8375 90)
    (tags RJ45)
    (path /599EF0F4)
    (fp_text reference J4 (at 4.7 11.18 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 ARD_PWM_2))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 ARD_TEMP_2))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_SRC_V))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 599EFD73)
    (at 266.27 124.51 90)
    (tags RJ45)
    (path /599EF28B)
    (fp_text reference J5 (at 4.7 11.18 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 ARD_PWM_4))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 ARD_TEMP_4))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_SRC_V))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(J5-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446) (tstamp 599EFD88)
    (at 173.74 101.72)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (path /599F9F17)
    (fp_text reference J6 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ARD_GROUND (at 0 4.87) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 3.87) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 ARD_GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446) (tstamp 599EFD9D)
    (at 188.97 29.12)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (path /599FA2FA)
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONTROL_DC (at 0 4.87) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 3.87) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 DC_GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DC_IN))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFDC2)
    (at 26.67 95.25 90)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (path /599F28C2)
    (fp_text reference P1 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Digital (at -1.27 20.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 19.05) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 19.11) (end -3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 19.11) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 19.55) (end 1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad16)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFDE7)
    (at 49.53 95.25 90)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (path /599EFF88)
    (fp_text reference P2 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Digital (at -1.27 20.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 19.05) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 19.11) (end -3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 19.11) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 19.55) (end 1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 ARD_PWM_4))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 ARD_PWM_3))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 ARD_PWM_2))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 ARD_PWM_1))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ARD_PWM_B))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 ARD_PWM_A))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P2-Pad16)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFE08)
    (at 26.67 30.48 90)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (path /599F5771)
    (fp_text reference P3 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Analog (at -1.27 15.03 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 13.97) (end 1.27 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 13.97) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 14.03) (end -3.87 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 14.03) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 14.5) (end 1.8 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P3-Pad12)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFE2D)
    (at 26.67 186.69 90)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (path /599F7708)
    (fp_text reference P4 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Digital (at -1.27 20.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 19.05) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 19.11) (end -3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 19.11) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 19.55) (end 1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P4-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P4-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P4-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P4-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P4-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P4-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P4-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P4-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P4-Pad16)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFE52)
    (at 49.53 186.69 90)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (path /599F76EC)
    (fp_text reference P5 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Digital (at -1.27 20.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 19.05) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 19.11) (end -3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 19.11) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 19.55) (end 1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P5-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P5-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P5-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P5-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P5-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P5-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P5-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P5-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P5-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P5-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P5-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P5-Pad16)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5449) (tstamp 599EFE73)
    (at 26.67 119.38 90)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (path /599F771D)
    (fp_text reference P6 (at -1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Analog (at -1.27 15.03 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start -3.81 13.97) (end 1.27 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 13.97) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end -3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 14.03) (end -3.87 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 14.03) (end -3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 0) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 0.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -1.8) (end -4.35 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 14.5) (end 1.8 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 ARD_TEMP_HB))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 ARD_TEMP_1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P6-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 ARD_TEMP_2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P6-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 ARD_TEMP_3))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P6-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 ARD_TEMP_4))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P6-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P6-Pad12)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )

  (gr_line (start 114.3 180.34) (end 25.4 180.34) (layer Dwgs.User) (width 0.2) (tstamp 599F0005))
  (gr_line (start 114.3 127) (end 114.3 180.34) (layer Dwgs.User) (width 0.2) (tstamp 599F0004))
  (gr_line (start 25.4 127) (end 114.3 127) (layer Dwgs.User) (width 0.2) (tstamp 599F0003))
  (gr_line (start 25.4 180.34) (end 25.4 127) (layer Dwgs.User) (width 0.2) (tstamp 599F0002))
  (gr_line (start 114.3 91.44) (end 25.4 91.44) (layer Dwgs.User) (width 0.2))
  (gr_line (start 114.3 38.1) (end 114.3 91.44) (layer Dwgs.User) (width 0.2))
  (gr_line (start 25.4 38.1) (end 114.3 38.1) (layer Dwgs.User) (width 0.2))
  (gr_line (start 25.4 91.44) (end 25.4 38.1) (layer Dwgs.User) (width 0.2))

  (segment (start 266.27 45.82) (end 266 46) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 266 46) (end 265 47) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 265 47) (end 262 47) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 262 47) (end 247 32) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 247 32) (end 189 32) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 189 32) (end 188.97 31.66) (width 1) (layer B.Cu) (net 1) (tstamp 59C5045A) (status 80000))
  (segment (start 263.73 44.55) (end 264 45) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 264 45) (end 263 44) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 263 44) (end 262 44) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 262 44) (end 262 43) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 262 43) (end 248 29) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 248 29) (end 189 29) (width 1) (layer B.Cu) (net 2) (status 80000))
  (segment (start 189 29) (end 188.97 29.12) (width 1) (layer B.Cu) (net 2) (tstamp 59C5045B) (status 80000))
  (segment (start 173.74 104.26) (end 173.74 101.72) (width 1) (layer B.Cu) (net 8))
  (segment (start 173.74 101.72) (end 174 102) (width 1) (layer B.Cu) (net 8) (status 80000))
  (segment (start 174 102) (end 180 96) (width 1) (layer B.Cu) (net 8) (status 80000))
  (segment (start 180 96) (end 264 96) (width 1) (layer B.Cu) (net 8) (status 80000))
  (segment (start 264 96) (end 263.73 95.9475) (width 1) (layer B.Cu) (net 8) (tstamp 59C5050B) (status 80000))

)
