(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 21)
    (no_connects 0)
    (area 109.231665 89.312379 185.495001 119.455001)
    (thickness 1.6)
    (drawings 14)
    (tracks 63)
    (zones 0)
    (modules 13)
    (nets 26)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory SVG/))
  )

  (net 0 "")
  (net 1 DC_ISO)
  (net 2 GND_ISO)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad3)")
  (net 5 ARD_PWM)
  (net 6 ARD_GND)
  (net 7 ARD_PWR_LVL)
  (net 8 ARD_TEMP)
  (net 9 DC_IN)
  (net 10 DC_GND)
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(R3-Pad1)")
  (net 13 "Net-(U1-Pad2)")
  (net 14 "Net-(U1-Pad3)")
  (net 15 "Net-(U1-Pad6)")
  (net 16 "Net-(U1-Pad8)")
  (net 17 "Net-(J3-Pad1)")
  (net 18 "Net-(R1-Pad2)")
  (net 19 "Net-(R2-Pad2)")
  (net 20 "Net-(U2-Pad3)")
  (net 21 "Net-(U2-Pad6)")
  (net 22 "Net-(U3-Pad1)")
  (net 23 "Net-(U3-Pad4)")
  (net 24 "Net-(U3-Pad5)")
  (net 25 "Net-(U3-Pad8)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (net_class Control ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net DC_ISO)
    (add_net GND_ISO)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad8)")
  )

  (net_class Signal ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_PWR_LVL)
    (add_net ARD_TEMP)
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer B.Cu) (tedit 592DEB72) (tstamp 592DE59C)
    (at 139.7 114.3)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592AD9EF)
    (fp_text reference U3 (at 0 2.54) (layer B.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_text value "W30508TRC (ICL7667)" (at 0 0) (layer B.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_line (start -1.51 1.48) (end 9.13 1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 1.48) (end 9.13 -9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -9.1) (end -1.51 -9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 -9.1) (end -1.51 1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 1.23) (end 8.88 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 1.23) (end 8.88 -8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -8.85) (end -1.26 -8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -8.85) (end -1.26 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -0.04) (end 0.01 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -8.85) (end 8.88 -8.85) (layer B.SilkS) (width 0.2))
    (fp_line (start 8.88 1.23) (end -1.26 1.23) (layer B.SilkS) (width 0.2))
    (fp_line (start -1.26 1.23) (end -1.26 0) (layer B.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(U3-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(R2-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND_ISO))
    (pad 4 thru_hole circle (at 0 -7.62 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(U3-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(U3-Pad5)"))
    (pad 6 thru_hole circle (at 7.62 -5.08 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 1 DC_ISO))
    (pad 7 thru_hole circle (at 7.62 -2.54 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(R3-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(U3-Pad8)"))
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer B.Cu) (tedit 5920C257) (tstamp 592DE370)
    (at 134.62 95.25 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C1 (at 1 3.56 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 22uF (at 1 -3.56 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0.65 0 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 0.65) (end -1.6 -0.65) (layer B.Fab) (width 0.1))
    (fp_line (start 1 2.55) (end 1 -2.55) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.04 2.55) (end 1.04 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.04 -0.98) (end 1.04 -2.55) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.08 2.549) (end 1.08 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.08 -0.98) (end 1.08 -2.549) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.12 2.548) (end 1.12 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.12 -0.98) (end 1.12 -2.548) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.16 2.546) (end 1.16 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.16 -0.98) (end 1.16 -2.546) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.2 2.543) (end 1.2 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.2 -0.98) (end 1.2 -2.543) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.24 2.539) (end 1.24 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.24 -0.98) (end 1.24 -2.539) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.28 2.535) (end 1.28 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.28 -0.98) (end 1.28 -2.535) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.32 2.531) (end 1.32 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.32 -0.98) (end 1.32 -2.531) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.36 2.525) (end 1.36 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.36 -0.98) (end 1.36 -2.525) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 2.519) (end 1.4 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 -0.98) (end 1.4 -2.519) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 2.513) (end 1.44 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -0.98) (end 1.44 -2.513) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.48 2.506) (end 1.48 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.48 -0.98) (end 1.48 -2.506) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.52 2.498) (end 1.52 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.52 -0.98) (end 1.52 -2.498) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.56 2.489) (end 1.56 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.56 -0.98) (end 1.56 -2.489) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.6 2.48) (end 1.6 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.6 -0.98) (end 1.6 -2.48) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.64 2.47) (end 1.64 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.64 -0.98) (end 1.64 -2.47) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.68 2.46) (end 1.68 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.68 -0.98) (end 1.68 -2.46) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.721 2.448) (end 1.721 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.721 -0.98) (end 1.721 -2.448) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.761 2.436) (end 1.761 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.761 -0.98) (end 1.761 -2.436) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.801 2.424) (end 1.801 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.801 -0.98) (end 1.801 -2.424) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.841 2.41) (end 1.841 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.841 -0.98) (end 1.841 -2.41) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.881 2.396) (end 1.881 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.881 -0.98) (end 1.881 -2.396) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.921 2.382) (end 1.921 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.921 -0.98) (end 1.921 -2.382) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.961 2.366) (end 1.961 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.961 -0.98) (end 1.961 -2.366) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.001 2.35) (end 2.001 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.001 -0.98) (end 2.001 -2.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.041 2.333) (end 2.041 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.041 -0.98) (end 2.041 -2.333) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.081 2.315) (end 2.081 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.081 -0.98) (end 2.081 -2.315) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.121 2.296) (end 2.121 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.121 -0.98) (end 2.121 -2.296) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.161 2.276) (end 2.161 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.161 -0.98) (end 2.161 -2.276) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.201 2.256) (end 2.201 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.201 -0.98) (end 2.201 -2.256) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.241 2.234) (end 2.241 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.241 -0.98) (end 2.241 -2.234) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.281 2.212) (end 2.281 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.281 -0.98) (end 2.281 -2.212) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.321 2.189) (end 2.321 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.321 -0.98) (end 2.321 -2.189) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.361 2.165) (end 2.361 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.361 -0.98) (end 2.361 -2.165) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.401 2.14) (end 2.401 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.401 -0.98) (end 2.401 -2.14) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.441 2.113) (end 2.441 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.441 -0.98) (end 2.441 -2.113) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.481 2.086) (end 2.481 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.481 -0.98) (end 2.481 -2.086) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.521 2.058) (end 2.521 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.521 -0.98) (end 2.521 -2.058) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.561 2.028) (end 2.561 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.561 -0.98) (end 2.561 -2.028) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.601 1.997) (end 2.601 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.601 -0.98) (end 2.601 -1.997) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.641 1.965) (end 2.641 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.641 -0.98) (end 2.641 -1.965) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.681 1.932) (end 2.681 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.681 -0.98) (end 2.681 -1.932) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.721 1.897) (end 2.721 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.721 -0.98) (end 2.721 -1.897) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.761 1.861) (end 2.761 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.761 -0.98) (end 2.761 -1.861) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.801 1.823) (end 2.801 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.801 -0.98) (end 2.801 -1.823) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.841 1.783) (end 2.841 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.841 -0.98) (end 2.841 -1.783) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.881 1.742) (end 2.881 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.881 -0.98) (end 2.881 -1.742) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.921 1.699) (end 2.921 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.921 -0.98) (end 2.921 -1.699) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.961 1.654) (end 2.961 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.961 -0.98) (end 2.961 -1.654) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.001 1.606) (end 3.001 -1.606) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.041 1.556) (end 3.041 -1.556) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.081 1.504) (end 3.081 -1.504) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.121 1.448) (end 3.121 -1.448) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.161 1.39) (end 3.161 -1.39) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.201 1.327) (end 3.201 -1.327) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.241 1.261) (end 3.241 -1.261) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.281 1.189) (end 3.281 -1.189) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.321 1.112) (end 3.321 -1.112) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.361 1.028) (end 3.361 -1.028) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.401 0.934) (end 3.401 -0.934) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.441 0.829) (end 3.441 -0.829) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.481 0.707) (end 3.481 -0.707) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.521 0.559) (end 3.521 -0.559) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.561 0.354) (end 3.561 -0.354) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.6 0.65) (end -1.6 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.85 2.85) (end -1.85 -2.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.85 -2.85) (end 3.85 -2.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end 3.85 2.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end -1.85 2.85) (layer B.CrtYd) (width 0.05))
    (fp_circle (center 1 0) (end 3.5 0) (layer B.Fab) (width 0.1))
    (fp_arc (start 1 0) (end -1.397436 0.98) (angle -135.5) (layer B.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.397436 -0.98) (angle 135.5) (layer B.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.397436 0.98) (angle -44.5) (layer B.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4 (layer B.Cu) (tedit 592DF1BE) (tstamp 592DE376)
    (at 140.97 96.52)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor")
    (path /592ACBF5)
    (fp_text reference C2 (at 10.16 5.08) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 220nF (at 5 -5.06) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 5 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.5 4) (end -1.5 -4) (layer B.Fab) (width 0.1))
    (fp_line (start -1.5 -4) (end 11.5 -4) (layer B.Fab) (width 0.1))
    (fp_line (start 11.5 -4) (end 11.5 4) (layer B.Fab) (width 0.1))
    (fp_line (start 11.5 4) (end -1.5 4) (layer B.Fab) (width 0.1))
    (fp_line (start -1.56 4.06) (end 11.56 4.06) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.56 -4.06) (end 11.56 -4.06) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.56 4.06) (end -1.56 -4.06) (layer B.SilkS) (width 0.12))
    (fp_line (start 11.56 4.06) (end 11.56 -4.06) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.85 4.35) (end -1.85 -4.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.85 -4.35) (end 11.85 -4.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start 11.85 -4.35) (end 11.85 4.35) (layer B.CrtYd) (width 0.05))
    (fp_line (start 11.85 4.35) (end -1.85 4.35) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole circle (at 10 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-220_Horizontal_Reversed (layer F.Cu) (tedit 58CE52AD) (tstamp 592DE37E)
    (at 157.48 101.6 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (path /592DCE5E)
    (fp_text reference D1 (at 2.54 20.58 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky_x2_KCom_AKA (at 2.54 -1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 20.58 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.46 13.06) (end -2.46 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 19.46) (end 7.54 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 19.46) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 3.81) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 13.06) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end 7.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 3.81) (end -2.46 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 3.81) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 3.81) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 3.69) (end 7.66 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.18) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 3.69) (end -2.58 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 3.69) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 19.58) (end -1.38 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.181 19.58) (end 1.02 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.22 19.58) (end 3.42 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.62 19.58) (end 5.82 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 19.58) (end 7.66 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.42) (end -2.58 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 15.82) (end -2.58 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 18.22) (end -2.58 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 13.42) (end 7.66 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 15.82) (end 7.66 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 18.22) (end 7.66 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.05) (end 0 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.066) (end 2.54 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.08 1.066) (end 5.08 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.71 -1.15) (end -2.71 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 19.71) (end 7.79 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 19.71) (end 7.79 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 -1.15) (end -2.71 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 16.66) (end 4.39 16.66) (layer F.Fab) (width 0.1))
    (pad 0 np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal_Reversed.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 180))
    )
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0410_04x1.25mm_Straight (layer B.Cu) (tedit 58A3B615) (tstamp 592DE386)
    (at 116.84 110.49 90)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0410")
    (tags "connector molex picoblade")
    (path /592C94BD)
    (fp_text reference J1 (at 1.875 -2.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X04 (at 1.875 3.25 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2 2.55) (end -2 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2 -1.6) (end 5.75 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.75 -1.6) (end 5.75 2.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.75 2.55) (end -2 2.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.5 2.075) (end -1.5 -1.125) (layer B.Fab) (width 0.1))
    (fp_line (start -1.5 -1.125) (end 5.25 -1.125) (layer B.Fab) (width 0.1))
    (fp_line (start 5.25 -1.125) (end 5.25 2.075) (layer B.Fab) (width 0.1))
    (fp_line (start 5.25 2.075) (end -1.5 2.075) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 2.225) (end -1.65 -1.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.275) (end 5.4 -1.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.4 -1.275) (end 5.4 2.225) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.4 2.225) (end -1.65 2.225) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.875 -0.725) (end -1.1 -0.725) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.725) (end -1.1 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 0.8) (end -1.1 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 0.8) (end -1.1 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 1.675) (end 1.875 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.875 -0.725) (end 4.85 -0.725) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.85 -0.725) (end 4.85 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.85 0) (end 5.05 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.05 0) (end 5.05 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.05 0.8) (end 4.85 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.85 0.8) (end 4.85 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.85 1.675) (end 1.875 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.525) (end -1.9 -0.525) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.525) (end -0.9 -1.525) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 1.875 1.25 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 ARD_PWM))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 ARD_GND))
    (pad 3 thru_hole circle (at 2.5 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 ARD_PWR_LVL))
    (pad 4 thru_hole circle (at 3.75 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 ARD_TEMP))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410_04x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-220_Horizontal_Reversed (layer F.Cu) (tedit 58CE52AD) (tstamp 592DE39E)
    (at 157.48 113.03 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (path /592BF9D4)
    (fp_text reference Q1 (at 2.54 20.58 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RFP12N10L (at 2.54 -1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 20.58 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.46 13.06) (end -2.46 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 19.46) (end 7.54 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 19.46) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 3.81) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 13.06) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end 7.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 3.81) (end -2.46 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 3.81) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 3.81) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 3.69) (end 7.66 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.18) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 3.69) (end -2.58 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 3.69) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 19.58) (end -1.38 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.181 19.58) (end 1.02 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.22 19.58) (end 3.42 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.62 19.58) (end 5.82 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 19.58) (end 7.66 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.42) (end -2.58 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 15.82) (end -2.58 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 18.22) (end -2.58 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 13.42) (end 7.66 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 15.82) (end 7.66 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 18.22) (end 7.66 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.05) (end 0 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.066) (end 2.54 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.08 1.066) (end 5.08 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.71 -1.15) (end -2.71 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 19.71) (end 7.79 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 19.71) (end 7.79 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 -1.15) (end -2.71 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 16.66) (end 4.39 16.66) (layer F.Fab) (width 0.1))
    (pad 0 np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal_Reversed.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 592DF1C4) (tstamp 592DE3A4)
    (at 121.92 106.68 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R1 (at 7.62 2.54 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 200 (at 3.81 -2.31 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.66 1.25) (end 0.66 -1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.66 -1.25) (end 6.96 -1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 6.96 1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 0.66 1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer B.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.05 1.6) (end -1.05 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.6) (end 8.7 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end 8.7 1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end -1.05 1.6) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 ARD_GND))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 592DF1B7) (tstamp 592DE3AA)
    (at 133.35 102.87)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACAE5)
    (fp_text reference R2 (at 10.16 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 4K7 (at 3.81 -1.86) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.01 0.8) (end 2.01 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 2.01 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer B.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer B.Fab) (width 0.1))
    (fp_line (start 1.95 0.86) (end 1.95 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.95 -0.86) (end 5.67 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 5.67 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 1.95 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.95 1.15) (end -0.95 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.15) (end 8.6 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end 8.6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end -0.95 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 592DF1A9) (tstamp 592DE3B0)
    (at 151.13 114.3 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACDEB)
    (fp_text reference R3 (at -2.54 2.54 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 4K7 (at 3.81 -1.86 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.01 0.8) (end 2.01 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 2.01 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer B.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer B.Fab) (width 0.1))
    (fp_line (start 1.95 0.86) (end 1.95 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.95 -0.86) (end 5.67 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 5.67 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 1.95 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.95 1.15) (end -0.95 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.15) (end 8.6 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end 8.6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end -0.95 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 592DF1AE) (tstamp 592DE3B6)
    (at 153.67 106.68 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACE76)
    (fp_text reference R4 (at 10.16 2.54 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 470 (at 3.81 -1.86 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.01 0.8) (end 2.01 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 5.61 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 5.61 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 2.01 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer B.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer B.Fab) (width 0.1))
    (fp_line (start 1.95 0.86) (end 1.95 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.95 -0.86) (end 5.67 -0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 5.67 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 1.95 0.86) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.95 1.15) (end -0.95 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.15) (end 8.6 -1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end 8.6 1.15) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end -0.95 1.15) (layer B.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer B.Cu) (tedit 592DEB7A) (tstamp 592DE3C2)
    (at 121.92 102.87)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592C6117)
    (fp_text reference U1 (at -2.54 0) (layer B.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_text value "W30508TRC (NME1212DC)" (at 0 0) (layer B.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_line (start -1.51 1.48) (end 9.13 1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 1.48) (end 9.13 -9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -9.1) (end -1.51 -9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 -9.1) (end -1.51 1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 1.23) (end 8.88 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 1.23) (end 8.88 -8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -8.85) (end -1.26 -8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -8.85) (end -1.26 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -0.04) (end 0.01 1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -8.85) (end 8.88 -8.85) (layer B.SilkS) (width 0.2))
    (fp_line (start 8.88 1.23) (end -1.26 1.23) (layer B.SilkS) (width 0.2))
    (fp_line (start -1.26 1.23) (end -1.26 0) (layer B.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 10 DC_GND))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 0 -7.62 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 9 DC_IN))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 1 DC_ISO))
    (pad 6 thru_hole circle (at 7.62 -5.08 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 -2.54 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND_ISO))
    (pad 8 thru_hole circle (at 7.62 0 270) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(U1-Pad8)"))
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer B.Cu) (tedit 592DF1E1) (tstamp 592DE590)
    (at 116.84 97.79 270)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (path /592C95DB)
    (fp_text reference J2 (at -3.81 -1.27 360) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value CONN_01X02 (at 0.625 3.25 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2 2.55) (end -2 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2 -1.6) (end 3.25 -1.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.25 -1.6) (end 3.25 2.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.25 2.55) (end -2 2.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.5 2.075) (end -1.5 -1.125) (layer B.Fab) (width 0.1))
    (fp_line (start -1.5 -1.125) (end 2.75 -1.125) (layer B.Fab) (width 0.1))
    (fp_line (start 2.75 -1.125) (end 2.75 2.075) (layer B.Fab) (width 0.1))
    (fp_line (start 2.75 2.075) (end -1.5 2.075) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 2.225) (end -1.65 -1.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.275) (end 2.9 -1.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.9 -1.275) (end 2.9 2.225) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.9 2.225) (end -1.65 2.225) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.625 -0.725) (end -1.1 -0.725) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.725) (end -1.1 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 0.8) (end -1.1 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 0.8) (end -1.1 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.1 1.675) (end 0.625 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.625 -0.725) (end 2.35 -0.725) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.35 -0.725) (end 2.35 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.35 0) (end 2.55 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.55 0) (end 2.55 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.55 0.8) (end 2.35 0.8) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.35 0.8) (end 2.35 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.35 1.675) (end 0.625 1.675) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.525) (end -1.9 -0.525) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.525) (end -0.9 -1.525) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0.625 1.25 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 DC_IN))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 DC_GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:DIPS762W60P254L760H300Q6N (layer B.Cu) (tedit 592DA648) (tstamp 592DF394)
    (at 127 113.03)
    (descr "Dip Socket")
    (tags Connector)
    (path /592DA8DF)
    (fp_text reference U2 (at 0 0) (layer B.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_text value "W30506TRC (4N35)" (at 0 0) (layer B.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)) (justify mirror))
    )
    (fp_line (start -1.51 1.51) (end 9.13 1.51) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 1.51) (end 9.13 -6.59) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -6.59) (end -1.51 -6.59) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 -6.59) (end -1.51 1.51) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 1.26) (end 8.88 1.26) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 1.26) (end 8.88 -6.34) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -6.34) (end -1.26 -6.34) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -6.34) (end -1.26 1.26) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -0.01) (end 0.01 1.26) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 -6.34) (end 8.88 -6.34) (layer B.SilkS) (width 0.2))
    (fp_line (start 8.88 1.26) (end -1.26 1.26) (layer B.SilkS) (width 0.2))
    (fp_line (start -1.26 1.26) (end -1.26 0) (layer B.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 5 ARD_PWM))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 -5.08 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND_ISO))
    (pad 5 thru_hole circle (at 7.62 -2.54 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(R2-Pad2)"))
    (pad 6 thru_hole circle (at 7.62 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(U2-Pad6)"))
  )

  (gr_circle (center 181.61 97.79) (end 181.61 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 181.61 110.49) (end 181.61 107.95) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 182.88 92.71) (end 181.61 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 182.88 116.84) (end 181.61 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 115.57 116.84) (end 116.84 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 115.57 92.71) (end 116.84 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 182.88 116.84) (end 185.42 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.57 116.84) (end 115.57 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.57 92.71) (end 113.03 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 182.88 92.71) (end 182.88 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 116.84) (end 185.42 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.57 119.38) (end 182.88 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 92.71) (end 113.03 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.88 90.17) (end 115.57 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 140.97 96.52) (end 140.97 97.79) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 144.78 106.68) (end 147.32 109.22) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DEE9D))
  (segment (start 144.78 101.6) (end 144.78 106.68) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DEE9B))
  (segment (start 140.97 97.79) (end 144.78 101.6) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DEE99))
  (segment (start 133.35 102.87) (end 133.35 101.6) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 137.16 100.33) (end 140.97 96.52) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DECE5))
  (segment (start 134.62 100.33) (end 137.16 100.33) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DECE3))
  (segment (start 133.35 101.6) (end 134.62 100.33) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DECE1))
  (segment (start 134.62 95.25) (end 139.7 95.25) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 139.7 95.25) (end 140.97 96.52) (width 0.6) (layer F.Cu) (net 1) (tstamp 592DECD3))
  (segment (start 129.54 95.25) (end 134.62 95.25) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 150.97 96.52) (end 151.13 96.52) (width 0.6) (layer F.Cu) (net 2) (status C00000))
  (segment (start 151.13 96.52) (end 156.21 101.6) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DF52C) (status 400000))
  (segment (start 156.21 101.6) (end 157.48 101.6) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DF52D) (status 800000))
  (segment (start 151.13 106.68) (end 151.13 96.68) (width 0.6) (layer F.Cu) (net 2) (status C00000))
  (segment (start 151.13 96.68) (end 150.97 96.52) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DF52A) (status C00000))
  (segment (start 157.48 101.6) (end 157.48 107.95) (width 0.6) (layer F.Cu) (net 2) (status C00000))
  (segment (start 134.62 107.95) (end 138.43 107.95) (width 0.6) (layer F.Cu) (net 2))
  (segment (start 138.43 107.95) (end 139.7 109.22) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DF3BA))
  (segment (start 151.13 106.68) (end 151.13 107.95) (width 0.6) (layer F.Cu) (net 2))
  (segment (start 151.13 107.95) (end 148.59 110.49) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DEEAB))
  (segment (start 148.59 110.49) (end 140.97 110.49) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DEEAD))
  (segment (start 140.97 110.49) (end 139.7 109.22) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DEEAF))
  (segment (start 127 104.14) (end 128.27 106.68) (width 0.6) (layer F.Cu) (net 2))
  (segment (start 128.27 106.68) (end 132.08 110.49) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED13))
  (segment (start 132.08 110.49) (end 132.08 114.3) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED15))
  (segment (start 132.08 114.3) (end 134.62 116.84) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED17))
  (segment (start 134.62 116.84) (end 139.7 116.84) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED19))
  (segment (start 139.7 116.84) (end 142.24 114.3) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED1B))
  (segment (start 142.24 114.3) (end 142.24 111.76) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED1D))
  (segment (start 142.24 111.76) (end 139.7 109.22) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED1F))
  (segment (start 129.54 100.33) (end 128.27 100.33) (width 0.6) (layer F.Cu) (net 2))
  (segment (start 127 101.6) (end 127 104.14) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED10))
  (segment (start 128.27 100.33) (end 127 101.6) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DED0E))
  (segment (start 129.54 100.33) (end 131.54 100.33) (width 0.6) (layer F.Cu) (net 2))
  (segment (start 131.54 100.33) (end 134.62 97.25) (width 0.6) (layer F.Cu) (net 2) (tstamp 592DECE8))
  (segment (start 116.84 110.49) (end 116.84 114.3) (width 0.5) (layer F.Cu) (net 5))
  (segment (start 123.19 116.84) (end 127 113.03) (width 0.5) (layer F.Cu) (net 5) (tstamp 592DF3C7))
  (segment (start 119.38 116.84) (end 123.19 116.84) (width 0.5) (layer F.Cu) (net 5) (tstamp 592DF3C5))
  (segment (start 116.84 114.3) (end 119.38 116.84) (width 0.5) (layer F.Cu) (net 5) (tstamp 592DF3C1))
  (segment (start 116.84 109.24) (end 119.36 109.24) (width 0.5) (layer F.Cu) (net 6))
  (segment (start 119.36 109.24) (end 121.92 106.68) (width 0.5) (layer F.Cu) (net 6) (tstamp 592DECD6))
  (segment (start 116.84 97.79) (end 119.38 97.79) (width 0.6) (layer F.Cu) (net 9))
  (segment (start 119.38 97.79) (end 121.92 95.25) (width 0.6) (layer F.Cu) (net 9) (tstamp 592DECCC))
  (segment (start 116.84 99.04) (end 118.09 99.04) (width 0.6) (layer F.Cu) (net 10))
  (segment (start 118.09 99.04) (end 121.92 102.87) (width 0.6) (layer F.Cu) (net 10) (tstamp 592DECCF))
  (segment (start 153.67 106.68) (end 154.94 107.95) (width 0.6) (layer F.Cu) (net 11))
  (segment (start 156.21 113.03) (end 157.48 113.03) (width 0.6) (layer F.Cu) (net 11) (tstamp 592DEF07))
  (segment (start 154.94 111.76) (end 156.21 113.03) (width 0.6) (layer F.Cu) (net 11) (tstamp 592DEF05))
  (segment (start 154.94 107.95) (end 154.94 111.76) (width 0.6) (layer F.Cu) (net 11) (tstamp 592DEF04))
  (segment (start 151.13 114.3) (end 153.67 114.3) (width 0.6) (layer F.Cu) (net 12))
  (segment (start 147.32 111.76) (end 148.59 111.76) (width 0.6) (layer F.Cu) (net 12))
  (segment (start 148.59 111.76) (end 151.13 114.3) (width 0.6) (layer F.Cu) (net 12) (tstamp 592DEEA0))
  (segment (start 127 110.49) (end 125.73 110.49) (width 0.6) (layer F.Cu) (net 18))
  (segment (start 125.73 110.49) (end 121.92 114.3) (width 0.6) (layer F.Cu) (net 18) (tstamp 592DF3BC))
  (segment (start 134.62 110.49) (end 133.35 110.49) (width 0.6) (layer F.Cu) (net 19))
  (segment (start 138.43 105.41) (end 140.97 102.87) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3F1))
  (segment (start 133.35 105.41) (end 138.43 105.41) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3EF))
  (segment (start 132.08 106.68) (end 133.35 105.41) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3ED))
  (segment (start 132.08 109.22) (end 132.08 106.68) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3E9))
  (segment (start 133.35 110.49) (end 132.08 109.22) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3E4))
  (segment (start 134.62 110.49) (end 138.43 110.49) (width 0.6) (layer F.Cu) (net 19))
  (segment (start 138.43 110.49) (end 139.7 111.76) (width 0.6) (layer F.Cu) (net 19) (tstamp 592DF3B8))

)
