(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 23)
    (no_connects 13)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 15)
    (nets 23)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 VCC_ISO)
  (net 2 GND_ISO)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad3)")
  (net 6 ARD_GND)
  (net 7 "Net-(J1-Pad2)")
  (net 8 VCC)
  (net 9 GND)
  (net 10 ARD_5V)
  (net 11 "Net-(J3-Pad2)")
  (net 12 ARD_PWM)
  (net 13 ARD_SRC_V)
  (net 14 ARD_TEMP)
  (net 15 "Net-(J3-Pad6)")
  (net 16 "Net-(J3-Pad7)")
  (net 17 "Net-(J4-Pad1)")
  (net 18 "Net-(Q1-Pad4)")
  (net 19 "Net-(R2-Pad2)")
  (net 20 "Net-(U2-Pad1)")
  (net 21 "Net-(U2-Pad7)")
  (net 22 "Net-(U2-Pad4)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_5V)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_SRC_V)
    (add_net ARD_TEMP)
    (add_net GND)
    (add_net GND_ISO)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
    (add_net VCC)
    (add_net VCC_ISO)
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5920C257) (tstamp 593ECFE8)
    (at 153.6 75 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /592EA608)
    (fp_text reference C1 (at 2.5 -3.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 3.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC_ISO))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 593ECFEE)
    (at 153.6 90.1 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /592ED18A)
    (fp_text reference C2 (at 1.25 -4.21 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 4.21 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.1 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.2) (end 1.25 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.2) (end 1.29 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.2) (end 1.33 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.198) (end 1.37 3.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.197) (end 1.41 3.197) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.194) (end 1.45 3.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.192) (end 1.49 3.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.188) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 3.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.185) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 3.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.18) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 3.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.176) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 3.176) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.17) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 3.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.165) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 3.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.158) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 3.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.152) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.144) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 3.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.137) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 3.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.128) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 3.128) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.119) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 3.119) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.11) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.1) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.09) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.079) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 3.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.067) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 3.067) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.055) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.042) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 3.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.029) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 3.029) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.015) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 3.015) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.001) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 3.001) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.986) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.97) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.954) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.937) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.919) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.919) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.901) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.901) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.882) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.863) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.843) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.843) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.822) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.822) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.8) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.778) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 2.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.755) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 2.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.731) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 2.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.706) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 2.706) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.681) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.654) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 2.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.627) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 2.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.599) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 2.599) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.57) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 2.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.54) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.51) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 2.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.478) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 2.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.445) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 2.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.411) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 2.411) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.375) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 2.375) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.339) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 2.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.301) (end 3.491 2.301) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.262) (end 3.531 2.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.222) (end 3.571 2.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.18) (end 3.611 2.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.137) (end 3.651 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.092) (end 3.691 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.045) (end 3.731 2.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -1.997) (end 3.771 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.946) (end 3.811 1.946) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.894) (end 3.851 1.894) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.839) (end 3.891 1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.781) (end 3.931 1.781) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.721) (end 3.971 1.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.658) (end 4.011 1.658) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.591) (end 4.051 1.591) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.52) (end 4.091 1.52) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.445) (end 4.131 1.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.364) (end 4.171 1.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.278) (end 4.211 1.278) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.184) (end 4.251 1.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.081) (end 4.291 1.081) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -0.966) (end 4.331 0.966) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.834) (end 4.371 0.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.676) (end 4.411 0.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.468) (end 4.451 0.468) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -3.5) (end -2.25 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 3.5) (end 4.75 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 3.5) (end 4.75 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.5) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.838236 -0.98) (angle 144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.838236 0.98) (angle -144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 4.338236 -0.98) (angle 35.2) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 593ECFF4)
    (at 165.2 75.9 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C3 (at 1.25 -4.21 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 4.21 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.1 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.2) (end 1.25 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.2) (end 1.29 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.2) (end 1.33 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.198) (end 1.37 3.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.197) (end 1.41 3.197) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.194) (end 1.45 3.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.192) (end 1.49 3.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.188) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 3.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.185) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 3.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.18) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 3.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.176) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 3.176) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.17) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 3.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.165) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 3.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.158) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 3.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.152) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.144) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 3.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.137) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 3.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.128) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 3.128) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.119) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 3.119) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.11) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.1) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.09) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.079) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 3.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.067) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 3.067) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.055) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.042) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 3.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.029) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 3.029) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.015) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 3.015) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.001) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 3.001) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.986) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.97) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.954) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.937) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.919) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.919) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.901) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.901) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.882) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.863) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.843) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.843) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.822) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.822) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.8) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.778) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 2.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.755) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 2.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.731) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 2.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.706) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 2.706) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.681) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.654) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 2.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.627) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 2.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.599) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 2.599) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.57) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 2.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.54) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.51) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 2.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.478) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 2.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.445) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 2.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.411) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 2.411) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.375) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 2.375) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.339) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 2.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.301) (end 3.491 2.301) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.262) (end 3.531 2.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.222) (end 3.571 2.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.18) (end 3.611 2.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.137) (end 3.651 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.092) (end 3.691 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.045) (end 3.731 2.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -1.997) (end 3.771 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.946) (end 3.811 1.946) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.894) (end 3.851 1.894) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.839) (end 3.891 1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.781) (end 3.931 1.781) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.721) (end 3.971 1.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.658) (end 4.011 1.658) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.591) (end 4.051 1.591) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.52) (end 4.091 1.52) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.445) (end 4.131 1.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.364) (end 4.171 1.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.278) (end 4.211 1.278) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.184) (end 4.251 1.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.081) (end 4.291 1.081) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -0.966) (end 4.331 0.966) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.834) (end 4.371 0.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.676) (end 4.411 0.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.468) (end 4.451 0.468) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -3.5) (end -2.25 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 3.5) (end 4.75 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 3.5) (end 4.75 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.5) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.838236 -0.98) (angle 144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.838236 0.98) (angle -144.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 4.338236 -0.98) (angle 35.2) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC_ISO))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5920C257) (tstamp 593ECFFA)
    (at 142.9 74.8 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /592ACBF5)
    (fp_text reference C4 (at 2.5 -3.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 3.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC_ISO))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 58CE52AE) (tstamp 593ED001)
    (at 178.7 90.1 90)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (path /592DCE5E)
    (fp_text reference D1 (at 5.45 -3.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky_x2_KCom_AKA (at 5.45 6.07 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5.45 -3.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.5 -2.33) (end -2.5 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.7) (end 13.4 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start 13.4 2.7) (end 13.4 -2.33) (layer F.Fab) (width 0.1))
    (fp_line (start 13.4 -2.33) (end -2.5 -2.33) (layer F.Fab) (width 0.1))
    (fp_line (start 3.645 -2.33) (end 3.645 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start 7.255 -2.33) (end 7.255 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.62 -2.451) (end 13.52 -2.451) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.62 2.82) (end 13.52 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.62 -2.451) (end -2.62 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.52 -2.451) (end 13.52 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.646 -2.451) (end 3.646 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.255 -2.451) (end 7.255 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.75 -2.59) (end -2.75 2.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.75 2.95) (end 13.65 2.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.65 2.95) (end 13.65 -2.59) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.65 -2.59) (end -2.75 -2.59) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5.45 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (pad 3 thru_hole oval (at 10.9 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 593ED007)
    (at 109.2 93.6 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /59355101)
    (fp_text reference J1 (at 1.25 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TEMP_PROBE (at 1.25 4.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 ARD_GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58EAE7F0) (tstamp 593ED00D)
    (at 109.5 80.2 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /592C95DB)
    (fp_text reference J2 (at 1.25 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DC_CONN (at 1.25 4.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 9 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module OAE_Footprints:RJ45_8 (layer F.Cu) (tedit 593ECDA1) (tstamp 593ED025)
    (at 120.65 102.64 270)
    (tags RJ45)
    (path /593ECA34)
    (fp_text reference J3 (at 4.7 11.18 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45-U (at 4.59 6.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 ARD_5V))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 ARD_PWM))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 ARD_SRC_V))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 ARD_TEMP))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 ARD_GND))
    (model Connectors.3dshapes/RJ45_8.wrl
      (at (xyz 0.18 -0.25 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 593ED02A)
    (at 202.7 111.7)
    (path /592CA485)
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DrainLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad1)"))
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 593ED02F)
    (at 199.4 100.2)
    (path /592CA834)
    (fp_text reference J5 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SourceLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
  )

  (module TO_SOT_Packages_THT:TO-247-5_Vertical (layer F.Cu) (tedit 58CE52AE) (tstamp 593ED038)
    (at 179.2 110.28 90)
    (descr "TO-247-5, Vertical, RM 2.54mm")
    (tags "TO-247-5 Vertical RM 2.54mm")
    (path /592BF9D4)
    (fp_text reference Q1 (at 5.08 -3.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RFP12N10L (at 5.08 6.07 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5.08 -3.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.87 -2.33) (end -2.87 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.87 2.7) (end 13.03 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start 13.03 2.7) (end 13.03 -2.33) (layer F.Fab) (width 0.1))
    (fp_line (start 13.03 -2.33) (end -2.87 -2.33) (layer F.Fab) (width 0.1))
    (fp_line (start 3.275 -2.33) (end 3.275 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start 6.885 -2.33) (end 6.885 2.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.99 -2.451) (end 13.15 -2.451) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.99 2.82) (end 13.15 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.99 -2.451) (end -2.99 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.15 -2.451) (end 13.15 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.276 -2.451) (end 3.276 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.276 2.4) (end 3.276 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.885 -2.451) (end 6.885 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.885 2.4) (end 6.885 2.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.12 -2.59) (end -3.12 2.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.12 2.95) (end 13.28 2.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.28 2.95) (end 13.28 -2.59) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.28 -2.59) (end -3.12 -2.59) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "Net-(Q1-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247-5_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 593ED03E)
    (at 118 88.78 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /5935695A)
    (fp_text reference R1 (at 3.81 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 ARD_TEMP))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 593ED044)
    (at 129.6 111.4 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R2 (at 3.81 -2.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 3.81 2.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 ARD_GND))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 58CC8E33) (tstamp 593ED050)
    (at 125.48 75.16)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (path /592EC206)
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NME1212DC (at 3.81 10.01) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end 8.89 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 8.89) (end 8.89 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 9.01) (end 6.58 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 9.01) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.39 -1.39) (end -1.39 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.39 9.01) (end 9.01 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.01 9.01) (end 9.01 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.01 -1.39) (end -1.39 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.7) (end -1.7 9.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 9.3) (end 9.3 9.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.3 9.3) (end 9.3 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.3 -1.7) (end -1.7 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC_ISO))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 58CC8E33) (tstamp 593ED05C)
    (at 135.32 98.32 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (path /593ED3B7)
    (fp_text reference U2 (at 3.81 -2.39 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TLP250H (at 3.81 10.01 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end 8.89 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 8.89) (end 8.89 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 9.01) (end 6.58 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 9.01) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.39 -1.39) (end -1.39 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.39 9.01) (end 9.01 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.01 9.01) (end 9.01 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.01 -1.39) (end -1.39 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.7) (end -1.7 9.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 9.3) (end 9.3 9.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.3 9.3) (end 9.3 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.3 -1.7) (end -1.7 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_PWM))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R2-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC_ISO))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
