(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 0)
    (no_connects 0)
    (area 146.849673 46.4344 217.471601 105.4536)
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 39)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(SHIELD1-PadAD5)")
  (net 2 "Net-(SHIELD1-PadAD4)")
  (net 3 "Net-(SHIELD1-PadAD3)")
  (net 4 "Net-(SHIELD1-PadAD0)")
  (net 5 "Net-(SHIELD1-PadAD1)")
  (net 6 "Net-(SHIELD1-PadAD2)")
  (net 7 "Net-(SHIELD1-PadV_IN)")
  (net 8 "Net-(SHIELD1-PadGND2)")
  (net 9 "Net-(SHIELD1-PadGND1)")
  (net 10 "Net-(SHIELD1-Pad3V3)")
  (net 11 "Net-(SHIELD1-PadRST)")
  (net 12 "Net-(SHIELD1-Pad0)")
  (net 13 "Net-(SHIELD1-Pad1)")
  (net 14 "Net-(SHIELD1-Pad2)")
  (net 15 "Net-(SHIELD1-Pad3)")
  (net 16 "Net-(SHIELD1-Pad4)")
  (net 17 "Net-(SHIELD1-Pad5)")
  (net 18 "Net-(SHIELD1-Pad6)")
  (net 19 "Net-(SHIELD1-Pad7)")
  (net 20 "Net-(SHIELD1-Pad8)")
  (net 21 "Net-(SHIELD1-Pad9)")
  (net 22 "Net-(SHIELD1-Pad10)")
  (net 23 "Net-(SHIELD1-Pad11)")
  (net 24 "Net-(SHIELD1-Pad12)")
  (net 25 "Net-(SHIELD1-Pad13)")
  (net 26 "Net-(SHIELD1-PadGND3)")
  (net 27 "Net-(SHIELD1-PadAREF)")
  (net 28 "Net-(SHIELD1-Pad5V)")
  (net 29 "Net-(SHIELD1-PadSDA)")
  (net 30 "Net-(SHIELD1-PadSCL)")
  (net 31 "Net-(SHIELD1-PadIO_R)")
  (net 32 "Net-(SHIELD1-PadNC)")
  (net 33 "Net-(SHIELD1-PadSP1)")
  (net 34 "Net-(SHIELD1-PadSP2)")
  (net 35 "Net-(SHIELD1-PadSP3)")
  (net 36 "Net-(SHIELD1-PadSP4)")
  (net 37 "Net-(SHIELD1-PadSP5)")
  (net 38 "Net-(SHIELD1-PadSP6)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad12)")
    (add_net "Net-(SHIELD1-Pad13)")
    (add_net "Net-(SHIELD1-Pad2)")
    (add_net "Net-(SHIELD1-Pad3)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad4)")
    (add_net "Net-(SHIELD1-Pad5)")
    (add_net "Net-(SHIELD1-Pad5V)")
    (add_net "Net-(SHIELD1-Pad6)")
    (add_net "Net-(SHIELD1-Pad7)")
    (add_net "Net-(SHIELD1-Pad8)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD0)")
    (add_net "Net-(SHIELD1-PadAD1)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND1)")
    (add_net "Net-(SHIELD1-PadGND2)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadIO_R)")
    (add_net "Net-(SHIELD1-PadNC)")
    (add_net "Net-(SHIELD1-PadRST)")
    (add_net "Net-(SHIELD1-PadSCL)")
    (add_net "Net-(SHIELD1-PadSDA)")
    (add_net "Net-(SHIELD1-PadSP1)")
    (add_net "Net-(SHIELD1-PadSP2)")
    (add_net "Net-(SHIELD1-PadSP3)")
    (add_net "Net-(SHIELD1-PadSP4)")
    (add_net "Net-(SHIELD1-PadSP5)")
    (add_net "Net-(SHIELD1-PadSP6)")
    (add_net "Net-(SHIELD1-PadV_IN)")
  )

  (module FT:ARDUINO_SHIELD (layer F.Cu) (tedit 0) (tstamp 594A549B)
    (at 148.5011 105.0036)
    (descr http://www.thingiverse.com/thing:9630)
    (path /594A541D)
    (fp_text reference SHIELD1 (at 5.715 -57.15) (layer F.SilkS)
      (effects (font (thickness 0.3048)))
    )
    (fp_text value ARDUINO_FOOTPRINT (at 10.16 -54.61) (layer F.SilkS) hide
      (effects (font (thickness 0.3048)))
    )
    (fp_line (start 66.04 -40.64) (end 66.04 -52.07) (layer Cmts.User) (width 0.381))
    (fp_line (start 66.04 -52.07) (end 64.77 -53.34) (layer Cmts.User) (width 0.381))
    (fp_line (start 64.77 -53.34) (end 0 -53.34) (layer Cmts.User) (width 0.381))
    (fp_line (start 66.04 0) (end 0 0) (layer Cmts.User) (width 0.381))
    (fp_line (start 0 0) (end 0 -53.34) (layer Cmts.User) (width 0.381))
    (fp_line (start 66.04 -40.64) (end 68.58 -38.1) (layer Cmts.User) (width 0.381))
    (fp_line (start 68.58 -38.1) (end 68.58 -5.08) (layer Cmts.User) (width 0.381))
    (fp_line (start 68.58 -5.08) (end 66.04 -2.54) (layer Cmts.User) (width 0.381))
    (fp_line (start 66.04 -2.54) (end 66.04 0) (layer Cmts.User) (width 0.381))
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(SHIELD1-PadAD0)"))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(SHIELD1-PadAD1)"))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SHIELD1-PadGND2)"))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SHIELD1-PadGND1)"))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-Pad2)"))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-Pad3)"))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-Pad4)"))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SHIELD1-Pad5)"))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-Pad7)"))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SHIELD1-Pad8)"))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad12)"))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad13)"))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(SHIELD1-Pad5V)"))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-PadSDA)"))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-PadSCL)"))
    (pad IO_R thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-PadIO_R)"))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SHIELD1-PadNC)"))
    (pad SP1 thru_hole circle (at 63.5 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(SHIELD1-PadSP1)"))
    (pad SP2 thru_hole circle (at 66.04 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(SHIELD1-PadSP2)"))
    (pad SP3 thru_hole circle (at 63.5 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(SHIELD1-PadSP3)"))
    (pad SP4 thru_hole circle (at 66.04 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(SHIELD1-PadSP4)"))
    (pad SP5 thru_hole circle (at 63.5 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(SHIELD1-PadSP5)"))
    (pad SP6 thru_hole circle (at 66.04 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(SHIELD1-PadSP6)"))
  )

)
