(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 26)
    (no_connects 26)
    (area 106.604999 54.534999 181.685001 81.355001)
    (thickness 1.6)
    (drawings 8)
    (tracks 0)
    (zones 0)
    (modules 16)
    (nets 27)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 DC_ISO)
  (net 2 GND_ISO)
  (net 3 ARD_PWM)
  (net 4 ARD_GND)
  (net 5 ARD_PWR_LVL)
  (net 6 ARD_TEMP)
  (net 7 DC_IN)
  (net 8 DC_GND)
  (net 9 "Net-(Q1-Pad1)")
  (net 10 "Net-(U1-Pad2)")
  (net 11 "Net-(U1-Pad3)")
  (net 12 "Net-(U1-Pad6)")
  (net 13 "Net-(U1-Pad8)")
  (net 14 "Net-(U2-Pad1)")
  (net 15 "Net-(U2-Pad4)")
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(D1-Pad3)")
  (net 18 "Net-(J3-Pad1)")
  (net 19 "Net-(R1-Pad2)")
  (net 20 "Net-(R2-Pad2)")
  (net 21 "Net-(R3-Pad2)")
  (net 22 "Net-(R4-Pad1)")
  (net 23 "Net-(U3-Pad1)")
  (net 24 "Net-(U3-Pad4)")
  (net 25 "Net-(U3-Pad5)")
  (net 26 "Net-(U3-Pad8)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_PWR_LVL)
    (add_net ARD_TEMP)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net DC_ISO)
    (add_net GND_ISO)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad8)")
  )

  (net_class Power ""
    (clearance 0.2)
    (trace_width 3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5920C257) (tstamp 592DB25F)
    (at 129.54 59.69 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C1 (at 1 -3.56 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22uF (at 1 3.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.65 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.55) (end 1 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.55) (end 1.04 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0.98) (end 1.04 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.549) (end 1.08 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 0.98) (end 1.08 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.548) (end 1.12 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 0.98) (end 1.12 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.546) (end 1.16 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 0.98) (end 1.16 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.543) (end 1.2 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 0.98) (end 1.2 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.539) (end 1.24 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.98) (end 1.24 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.535) (end 1.28 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.98) (end 1.28 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.531) (end 1.32 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.98) (end 1.32 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.525) (end 1.36 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.98) (end 1.36 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.519) (end 1.4 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.98) (end 1.4 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.513) (end 1.44 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.98) (end 1.44 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -2.506) (end 1.48 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.98) (end 1.48 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -2.498) (end 1.52 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.98) (end 1.52 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -2.489) (end 1.56 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.98) (end 1.56 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -2.48) (end 1.6 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.98) (end 1.6 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -2.47) (end 1.64 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.98) (end 1.64 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -2.46) (end 1.68 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.98) (end 1.68 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -2.448) (end 1.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.98) (end 1.721 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -2.436) (end 1.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.98) (end 1.761 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -2.424) (end 1.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.98) (end 1.801 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -2.41) (end 1.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.98) (end 1.841 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -2.396) (end 1.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.98) (end 1.881 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -2.382) (end 1.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.98) (end 1.921 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -2.366) (end 1.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.98) (end 1.961 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -2.35) (end 2.001 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.98) (end 2.001 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -2.333) (end 2.041 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.98) (end 2.041 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -2.315) (end 2.081 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.98) (end 2.081 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -2.296) (end 2.121 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.98) (end 2.121 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -2.276) (end 2.161 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.98) (end 2.161 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -2.256) (end 2.201 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.98) (end 2.201 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -2.234) (end 2.241 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.98) (end 2.241 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -2.212) (end 2.281 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.98) (end 2.281 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -2.189) (end 2.321 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.98) (end 2.321 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -2.165) (end 2.361 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.98) (end 2.361 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -2.14) (end 2.401 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.98) (end 2.401 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -2.113) (end 2.441 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.98) (end 2.441 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -2.086) (end 2.481 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.98) (end 2.481 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -2.058) (end 2.521 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.98) (end 2.521 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -2.028) (end 2.561 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.98) (end 2.561 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.997) (end 2.601 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.98) (end 2.601 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.965) (end 2.641 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.98) (end 2.641 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.932) (end 2.681 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.98) (end 2.681 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.897) (end 2.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.98) (end 2.721 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.861) (end 2.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.98) (end 2.761 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.823) (end 2.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 0.98) (end 2.801 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -1.783) (end 2.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 0.98) (end 2.841 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -1.742) (end 2.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 0.98) (end 2.881 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -1.699) (end 2.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 0.98) (end 2.921 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -1.654) (end 2.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 0.98) (end 2.961 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -1.606) (end 3.001 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -1.556) (end 3.041 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -1.504) (end 3.081 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.121 -1.448) (end 3.121 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.161 -1.39) (end 3.161 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.201 -1.327) (end 3.201 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.241 -1.261) (end 3.241 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.281 -1.189) (end 3.281 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.321 -1.112) (end 3.321 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.361 -1.028) (end 3.361 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.401 -0.934) (end 3.401 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.441 -0.829) (end 3.441 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.481 -0.707) (end 3.481 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.521 -0.559) (end 3.521 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.561 -0.354) (end 3.561 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.85) (end -1.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 2.85) (end 3.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end 3.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end -1.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1 0) (end -1.397436 -0.98) (angle 135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.397436 0.98) (angle -135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.397436 -0.98) (angle 44.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0410_04x1.25mm_Straight (layer F.Cu) (tedit 592DC323) (tstamp 592DB297)
    (at 109.22 68.58 270)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0410")
    (tags "connector molex picoblade")
    (path /592C94BD)
    (fp_text reference J1 (at -3.175 0.635 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 1.875 -3.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2 -2.55) (end -2 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 1.6) (end 5.75 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 1.6) (end 5.75 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -2.55) (end -2 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -2.075) (end -1.5 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.125) (end 5.25 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start 5.25 1.125) (end 5.25 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start 5.25 -2.075) (end -1.5 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -2.225) (end -1.65 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 1.275) (end 5.4 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.4 1.275) (end 5.4 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.4 -2.225) (end -1.65 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.875 0.725) (end -1.1 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0.725) (end -1.1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.8) (end -1.1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.8) (end -1.1 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.675) (end 1.875 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.875 0.725) (end 4.85 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 0.725) (end 4.85 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 0) (end 5.05 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 0) (end 5.05 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.8) (end 4.85 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 -0.8) (end 4.85 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.85 -1.675) (end 1.875 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -1.9 0.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -0.9 1.525) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 1.875 -1.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 ARD_GND))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 ARD_PWM))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 ARD_PWR_LVL))
    (pad 4 thru_hole circle (at 3.75 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 ARD_TEMP))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0410_04x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 592DB303)
    (at 109.22 77.47)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R1 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200 (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 ARD_PWM))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 592DDAA4) (tstamp 592DB319)
    (at 135.89 64.77 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592AC85B)
    (fp_text reference R2 (at 10.16 -1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330 (at 3.81 1.86 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 592DB32F)
    (at 146.05 64.77 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACAE5)
    (fp_text reference R3 (at 3.81 -1.86 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4K7 (at 3.81 1.86 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(R3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 592DB345)
    (at 146.05 76.2 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACDEB)
    (fp_text reference R4 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4K7 (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592DDFA0) (tstamp 592DB35D)
    (at 114.3 57.15)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592C6117)
    (fp_text reference U1 (at -2.54 -1.27) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (NME1212DC)" (at 0 0) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 DC_GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 DC_IN))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 DC_ISO))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND_ISO))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad8)"))
  )

  (module Capacitors_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 592DDC50) (tstamp 592DB8E7)
    (at 134.62 59.69)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (path /592ACBF5)
    (fp_text reference C2 (at 15.24 5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220nF (at 7.5 4.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 7.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.5 -3.5) (end -1.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 3.5) (end 16.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 16.5 3.5) (end 16.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 16.5 -3.5) (end -1.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.56 -3.56) (end 16.56 -3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.56 3.56) (end 16.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.56 -3.56) (end -1.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.56 -3.56) (end 16.56 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -3.85) (end -1.85 3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 3.85) (end 16.85 3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.85 3.85) (end 16.85 -3.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.85 -3.85) (end -1.85 -3.85) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 DC_ISO))
    (pad 2 thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-220_Horizontal_Reversed (layer F.Cu) (tedit 58CE52AD) (tstamp 592DC345)
    (at 153.67 76.2 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (path /592BF9D4)
    (fp_text reference Q1 (at 2.54 20.58 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RFP12N10L (at 2.54 -1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 20.58 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.46 13.06) (end -2.46 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 19.46) (end 7.54 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 19.46) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 3.81) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 13.06) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end 7.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 3.81) (end -2.46 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 3.81) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 3.81) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 3.69) (end 7.66 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.18) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 3.69) (end -2.58 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 3.69) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 19.58) (end -1.38 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.181 19.58) (end 1.02 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.22 19.58) (end 3.42 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.62 19.58) (end 5.82 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 19.58) (end 7.66 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.42) (end -2.58 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 15.82) (end -2.58 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 18.22) (end -2.58 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 13.42) (end 7.66 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 15.82) (end 7.66 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 18.22) (end 7.66 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.05) (end 0 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.066) (end 2.54 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.08 1.066) (end 5.08 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.71 -1.15) (end -2.71 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 19.71) (end 7.79 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 19.71) (end 7.79 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 -1.15) (end -2.71 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 16.66) (end 4.39 16.66) (layer F.Fab) (width 0.1))
    (pad 0 np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal_Reversed.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 180))
    )
  )

  (module Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer F.Cu) (tedit 58A3B615) (tstamp 592DDE90)
    (at 110.49 60.96 90)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (path /592C95DB)
    (fp_text reference J2 (at 0.625 2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 0.625 -3.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2 -2.55) (end -2 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2 1.6) (end 3.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 1.6) (end 3.25 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 -2.55) (end -2 -2.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -2.075) (end -1.5 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.125) (end 2.75 1.125) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 1.125) (end 2.75 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -2.075) (end -1.5 -2.075) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -2.225) (end -1.65 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 1.275) (end 2.9 1.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 1.275) (end 2.9 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -2.225) (end -1.65 -2.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.625 0.725) (end -1.1 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0.725) (end -1.1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 0) (end -1.3 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0) (end -1.3 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.8) (end -1.1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -0.8) (end -1.1 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.675) (end 0.625 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.625 0.725) (end 2.35 0.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0.725) (end 2.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0) (end 2.55 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.55 0) (end 2.55 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.55 -0.8) (end 2.35 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 -0.8) (end 2.35 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 -1.675) (end 0.625 -1.675) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -1.9 0.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 1.525) (end -0.9 1.525) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0.625 -1.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 DC_IN))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 DC_GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 592DDEA6)
    (at 149.86 68.58 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ACE76)
    (fp_text reference R5 (at 3.81 -1.86 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470 (at 3.81 1.86 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(R4-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 592DE134)
    (at 177.8 73.66)
    (path /592CA485)
    (fp_text reference J3 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DrainLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad1)"))
  )

  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 0) (tstamp 592DE139)
    (at 177.8 62.23)
    (path /592CA834)
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SourceLarge (at 1.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592DDF98) (tstamp 592DE151)
    (at 120.65 68.58)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592ADB99)
    (fp_text reference U2 (at 0 10.16) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (6N317)" (at 0 0) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 ARD_GND))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND_ISO))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R3-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(R2-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(R2-Pad2)"))
  )

  (module SamacSys_Parts:DIPS762W50P254L1008H460Q8N (layer F.Cu) (tedit 592DDF9B) (tstamp 592DE169)
    (at 133.35 68.58)
    (descr W30508TRC)
    (tags "Undefined or Miscellaneous")
    (path /592AD9EF)
    (fp_text reference U3 (at 0 10.16) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_text value "W30508TRC (ICL7667)" (at 0 0) (layer F.SilkS) hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
    )
    (fp_line (start -1.51 -1.48) (end 9.13 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 -1.48) (end 9.13 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start 9.13 9.1) (end -1.51 9.1) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.51 9.1) (end -1.51 -1.48) (layer Dwgs.User) (width 0.05))
    (fp_line (start -1.26 -1.23) (end 8.88 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 -1.23) (end 8.88 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start 8.88 8.85) (end -1.26 8.85) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end -1.26 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 0.04) (end 0.01 -1.23) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.26 8.85) (end 8.88 8.85) (layer F.SilkS) (width 0.2))
    (fp_line (start 8.88 -1.23) (end -1.26 -1.23) (layer F.SilkS) (width 0.2))
    (fp_line (start -1.26 -1.23) (end -1.26 0) (layer F.SilkS) (width 0.2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U3-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R3-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND_ISO))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U3-Pad4)"))
    (pad 5 thru_hole circle (at 7.62 7.62 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U3-Pad5)"))
    (pad 6 thru_hole circle (at 7.62 5.08 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 DC_ISO))
    (pad 7 thru_hole circle (at 7.62 2.54 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R4-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U3-Pad8)"))
  )

  (module TO_SOT_Packages_THT:TO-220_Horizontal_Reversed (layer F.Cu) (tedit 58CE52AD) (tstamp 592DE3EF)
    (at 153.67 64.77 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (path /592DED01)
    (fp_text reference D1 (at 2.54 20.58 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky_x2_KCom_AKA (at 2.54 -1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 20.58 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.46 13.06) (end -2.46 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 19.46) (end 7.54 19.46) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 19.46) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 3.81) (end -2.46 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 13.06) (end 7.54 13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 13.06) (end 7.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 3.81) (end -2.46 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 3.81) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 3.81) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 3.69) (end 7.66 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.18) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 3.69) (end -2.58 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 3.69) (end 7.66 13.18) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 19.58) (end -1.38 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.181 19.58) (end 1.02 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.22 19.58) (end 3.42 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.62 19.58) (end 5.82 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 19.58) (end 7.66 19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 13.42) (end -2.58 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 15.82) (end -2.58 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 18.22) (end -2.58 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 13.42) (end 7.66 14.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 15.82) (end 7.66 17.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 18.22) (end 7.66 19.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.05) (end 0 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.066) (end 2.54 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.08 1.066) (end 5.08 3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.71 -1.15) (end -2.71 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 19.71) (end 7.79 19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 19.71) (end 7.79 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 -1.15) (end -2.71 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 16.66) (end 4.39 16.66) (layer F.Fab) (width 0.1))
    (pad 0 np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND_ISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal_Reversed.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 180))
    )
  )

  (gr_line (start 106.68 54.61) (end 106.68 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 54.61) (end 181.61 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.315 80.645) (end 180.975 80.645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.315 53.975) (end 180.975 53.975) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.315 54.61) (end 106.68 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.315 80.01) (end 107.315 80.645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.975 80.01) (end 181.61 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.975 54.61) (end 180.975 53.975) (angle 90) (layer Edge.Cuts) (width 0.15))

)
