(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 28)
    (no_connects 0)
    (area 97.560001 76.04 163.485 116.385)
    (thickness 1.6)
    (drawings 11)
    (tracks 91)
    (zones 0)
    (modules 15)
    (nets 17)
  )

  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.4)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.2 4.2)
    (pad_drill 4.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 109.22 116.84)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x01060_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GRB/))
  )

  (net 0 "")
  (net 1 GND_ISO)
  (net 2 ARD_GND)
  (net 3 DC_IN)
  (net 4 DC_ISO)
  (net 5 ARD_5V)
  (net 6 ARD_TEMP)
  (net 7 ARD_PWM)
  (net 8 ARD_SRC_V)
  (net 9 "Net-(R2-Pad2)")
  (net 10 DC_GND)
  (net 11 "Net-(U2-Pad3)")
  (net 12 "Net-(U2-Pad6)")
  (net 13 DRV_GATE)
  (net 14 DRV_SIG)
  (net 15 "Net-(U3-Pad3)")
  (net 16 "Net-(J2-Pad7)")

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ARD_5V)
    (add_net ARD_GND)
    (add_net ARD_PWM)
    (add_net ARD_SRC_V)
    (add_net ARD_TEMP)
    (add_net DC_GND)
    (add_net DC_IN)
    (add_net DC_ISO)
    (add_net DRV_GATE)
    (add_net DRV_SIG)
    (add_net GND_ISO)
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad3)")
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 59514246) (tstamp 594A6BE3)
    (at 157.71 110.11 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /594A5A11)
    (fp_text reference J3 (at -3.67 2.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 1.25 4.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 13 DRV_GATE))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5946D525) (tstamp 593FC421)
    (at 133.43 94)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /592EC206)
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NME1212DC (at 3.81 10.01) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 9.01) (end 6.58 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 9.01) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 9.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.2) (end 8.7 9.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.2) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 DC_GND))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 4 thru_hole circle (at 0 7.62) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 DC_IN))
    (pad 8 thru_hole circle (at 7.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5946D707) (tstamp 593FC415)
    (at 141.58 106.18 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /592ED01B)
    (fp_text reference R3 (at -1.73 0.31 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1K5 (at 2.54 1.86 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 -0.8) (end 0.74 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.74 0.8) (end 4.34 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 0.8) (end 4.34 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 -0.8) (end 0.74 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.74 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.34 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.68 -0.86) (end 4.4 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.68 0.86) (end 4.4 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 6.05 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.15) (end 6.05 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 DRV_SIG))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 595121BF)
    (at 125.3 89.64 270)
    (tags RJ45)
    (path /595274F5)
    (fp_text reference J2 (at 13.01 13.49 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 DC_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 DC_GND))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 ARD_5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 ARD_PWM))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 ARD_TEMP))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 ARD_SRC_V))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594A6A3B) (tstamp 593FC409)
    (at 121.84 104.67 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /593FD687)
    (fp_text reference R1 (at 4.87 1.45 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 ARD_TEMP))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5946E255) (tstamp 593FC3BE)
    (at 156.63 93.9)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /592ACBF5)
    (fp_text reference C2 (at -2.8 1.01) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.775 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.147436 -0.98) (angle 135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.147436 0.98) (angle -135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.647436 -0.98) (angle 44.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 594A6A0F) (tstamp 593FC3CA)
    (at 156.53 100.22)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /592ED18A)
    (fp_text reference C4 (at -2.97 -2.22) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.775 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -1.147436 -0.98) (angle 135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.147436 0.98) (angle -135.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.647436 -0.98) (angle 44.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 DRV_GATE))
    (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 594A6A36) (tstamp 593FC40F)
    (at 126.16 104.64 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /592BF392)
    (fp_text reference R2 (at 4.95 1.33 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 180 (at 3.81 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 ARD_GND))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5946D62A) (tstamp 593FC3E3)
    (at 115.26 110.77 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (path /593FD4A9)
    (fp_text reference J1 (at 6.08 2.73 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X02 (at 1.25 4.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.45 -2.35) (end -2.45 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.45 3.4) (end 4.95 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 3.4) (end 4.95 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -2.35) (end -2.45 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -2.85) (end -2.95 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.95 3.9) (end 5.45 3.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 3.9) (end 5.45 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.45 -2.85) (end -2.95 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.55 -2.45) (end -2.55 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 3.5) (end 5.05 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 3.5) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -2.45) (end 0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.75 -1.7) (end 1.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1.7) (end 1.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -2.45) (end 0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -2.45) (end -2.55 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1.7) (end -0.75 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.7) (end -0.75 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -2.45) (end -2.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.45) (end 3.25 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.7) (end 5.05 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -1.7) (end 5.05 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -2.45) (end 3.25 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -0.2) (end -1.8 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.2) (end -1.8 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.05 -0.2) (end 4.3 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -0.2) (end 4.3 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -2.75) (end -2.85 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.85 -2.75) (end -2.85 -0.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 ARD_5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 ARD_TEMP))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 5946D5E2) (tstamp 593FC42B)
    (at 130.27 106.8)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /592E7A66)
    (fp_text reference U2 (at 3.81 -2.39) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4N35 (at 3.81 7.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 6.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 6.47) (end 6.58 6.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 6.47) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 6.6) (end 8.7 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 6.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 ARD_PWM))
    (pad 4 thru_hole circle (at 7.62 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 5 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 DRV_SIG))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad3)"))
    (pad 6 thru_hole circle (at 7.62 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad6)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 58CC8E33) (tstamp 594A5986)
    (at 145.37 105.1)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /592E820A)
    (fp_text reference U3 (at 1.16 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TC4422AVPA (at 3.81 10.01) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 9.01) (end 6.58 9.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 9.01) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 9.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.2) (end 8.7 9.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.2) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 DRV_SIG))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 DRV_GATE))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U3-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 DRV_GATE))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5942BB67)
    (at 134.32 88.64)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB) (tstamp 5942B0A6)
    (at 154.32 88.64)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference "" (at 0 -5.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1pin (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 59512E37)
    (at 147.85 99.88)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /59400A26)
    (fp_text reference C3 (at -2.7 -1.88) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 1.25 3.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.65 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -0.8749 -0.98) (angle 130.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.8749 0.98) (angle -130.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.3749 -0.98) (angle 49.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 DRV_GATE))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 5920C257) (tstamp 5951312D)
    (at 147.89 94.39)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (path /592ACB50)
    (fp_text reference C1 (at 1.25 -3.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7uF (at 1.25 3.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.65 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.6) (end -1.35 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.6) (end 3.85 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.6) (end 3.85 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.6) (end -1.35 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.25 0) (end -0.8749 -0.98) (angle 130.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -0.8749 0.98) (angle -130.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.3749 -0.98) (angle 49.5) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DC_ISO))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND_ISO))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "Control\nRev1a" (at 144 89) (layer B.Cu)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (dimension 30.48 (width 0.3) (layer Dwgs.User)
    (gr_text "30.480 mm" (at 104.06 100.33 270) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 107.95 115.57) (xy 102.71 115.57)))
    (feature2 (pts (xy 107.95 85.09) (xy 102.71 85.09)))
    (crossbar (pts (xy 105.41 85.09) (xy 105.41 115.57)))
    (arrow1a (pts (xy 105.41 115.57) (xy 104.823579 114.443496)))
    (arrow1b (pts (xy 105.41 115.57) (xy 105.996421 114.443496)))
    (arrow2a (pts (xy 105.41 85.09) (xy 104.823579 86.216504)))
    (arrow2b (pts (xy 105.41 85.09) (xy 105.996421 86.216504)))
  )
  (dimension 52.07 (width 0.3) (layer Dwgs.User)
    (gr_text "52.070 mm" (at 136.525 77.39) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 162.56 81.28) (xy 162.56 76.04)))
    (feature2 (pts (xy 110.49 81.28) (xy 110.49 76.04)))
    (crossbar (pts (xy 110.49 78.74) (xy 162.56 78.74)))
    (arrow1a (pts (xy 162.56 78.74) (xy 161.433496 79.326421)))
    (arrow1b (pts (xy 162.56 78.74) (xy 161.433496 78.153579)))
    (arrow2a (pts (xy 110.49 78.74) (xy 111.616504 79.326421)))
    (arrow2b (pts (xy 110.49 78.74) (xy 111.616504 78.153579)))
  )
  (gr_line (start 110.49 87.63) (end 110.49 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 87.63) (end 162.56 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.02 87.63) (end 160.02 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.02 113.03) (end 162.56 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 113.03) (end 113.03 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 87.63) (end 110.49 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 85.09) (end 160.02 85.09) (angle 90) (layer Edge.Cuts) (width 0.15) (tstamp 592EF4C2))
  (gr_line (start 113.03 115.57) (end 160.02 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 137.89 111.88) (end 137.250001 111.240001) (width 1) (layer B.Cu) (net 1))
  (segment (start 137.250001 111.240001) (end 136.977999 111.240001) (width 1) (layer B.Cu) (net 1))
  (segment (start 136.977999 111.240001) (end 135.707155 109.969157) (width 1) (layer B.Cu) (net 1))
  (segment (start 135.707155 109.969157) (end 135.707155 101.610843) (width 1) (layer B.Cu) (net 1))
  (segment (start 135.707155 101.610843) (end 140.137999 97.179999) (width 1) (layer B.Cu) (net 1))
  (segment (start 140.137999 97.179999) (end 140.410001 97.179999) (width 1) (layer B.Cu) (net 1))
  (segment (start 140.410001 97.179999) (end 141.05 96.54) (width 1) (layer B.Cu) (net 1))
  (segment (start 157.71 110.11) (end 158.434999 109.385001) (width 1) (layer B.Cu) (net 1))
  (segment (start 158.434999 109.385001) (end 159.614388 109.385001) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.614388 109.385001) (end 159.614388 102.218601) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.614388 102.218601) (end 159.03 101.634213) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.03 101.634213) (end 159.03 100.22) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.03 100.22) (end 158.961957 100.22) (width 1) (layer B.Cu) (net 1))
  (segment (start 158.961957 100.22) (end 158.430001 99.688044) (width 1) (layer B.Cu) (net 1))
  (segment (start 158.430001 99.688044) (end 158.430001 98.499999) (width 1) (layer B.Cu) (net 1))
  (segment (start 151.52137 94.39) (end 150.39 94.39) (width 1) (layer B.Cu) (net 1))
  (segment (start 158.430001 98.499999) (end 157.829583 97.899581) (width 1) (layer B.Cu) (net 1))
  (segment (start 157.829583 97.899581) (end 156.641538 97.899581) (width 1) (layer B.Cu) (net 1))
  (segment (start 156.641538 97.899581) (end 153.131957 94.39) (width 1) (layer B.Cu) (net 1))
  (segment (start 153.131957 94.39) (end 151.52137 94.39) (width 1) (layer B.Cu) (net 1))
  (segment (start 150.39 94.39) (end 150.39 97.34) (width 1) (layer B.Cu) (net 1))
  (segment (start 150.39 97.34) (end 147.85 99.88) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.03 100.22) (end 159.03 94) (width 1) (layer B.Cu) (net 1))
  (segment (start 159.03 94) (end 159.13 93.9) (width 1) (layer B.Cu) (net 1))
  (segment (start 152.99 112.72) (end 155.1 112.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 155.1 112.72) (end 157.71 110.11) (width 1) (layer B.Cu) (net 1))
  (segment (start 145.37 112.72) (end 152.99 112.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 137.89 111.88) (end 139.529999 113.519999) (width 1) (layer B.Cu) (net 1))
  (segment (start 139.529999 113.519999) (end 144.570001 113.519999) (width 1) (layer B.Cu) (net 1))
  (segment (start 144.570001 113.519999) (end 145.37 112.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 127.84 98.53) (end 127.84 102.96) (width 1) (layer B.Cu) (net 2))
  (segment (start 127.84 102.96) (end 126.16 104.64) (width 1) (layer B.Cu) (net 2))
  (segment (start 121.84 112.29) (end 121.84 108.96) (width 1) (layer B.Cu) (net 2))
  (segment (start 121.84 108.96) (end 126.16 104.64) (width 1) (layer B.Cu) (net 2))
  (segment (start 125.3 89.64) (end 125.3 88.591136) (width 1) (layer B.Cu) (net 3))
  (segment (start 136.16669 93.116688) (end 136.16669 99.155312) (width 1) (layer B.Cu) (net 3))
  (segment (start 125.3 88.591136) (end 129.718206 88.591136) (width 1) (layer B.Cu) (net 3))
  (segment (start 129.718206 88.591136) (end 130.637061 89.509991) (width 1) (layer B.Cu) (net 3))
  (segment (start 133.040559 91.874563) (end 134.924565 91.874563) (width 1) (layer B.Cu) (net 3))
  (segment (start 134.924565 91.874563) (end 136.16669 93.116688) (width 1) (layer B.Cu) (net 3))
  (segment (start 130.637061 89.509991) (end 130.675988 89.509992) (width 1) (layer B.Cu) (net 3))
  (segment (start 130.675988 89.509992) (end 133.040559 91.874563) (width 1) (layer B.Cu) (net 3))
  (segment (start 134.069999 100.980001) (end 133.43 101.62) (width 1) (layer B.Cu) (net 3))
  (segment (start 136.16669 99.155312) (end 134.342001 100.980001) (width 1) (layer B.Cu) (net 3))
  (segment (start 134.342001 100.980001) (end 134.069999 100.980001) (width 1) (layer B.Cu) (net 3))
  (segment (start 147.89 94.39) (end 147.89 93.988371) (width 1) (layer B.Cu) (net 4))
  (segment (start 147.89 93.988371) (end 149.288975 92.589396) (width 1) (layer B.Cu) (net 4))
  (segment (start 149.288975 92.589396) (end 155.319396 92.589396) (width 1) (layer B.Cu) (net 4))
  (segment (start 155.319396 92.589396) (end 156.63 93.9) (width 1) (layer B.Cu) (net 4))
  (segment (start 141.58 106.18) (end 141.0684 105.6684) (width 1) (layer B.Cu) (net 4))
  (segment (start 141.0684 105.6684) (end 141.0684 101.6384) (width 1) (layer B.Cu) (net 4))
  (segment (start 141.0684 101.6384) (end 141.05 101.62) (width 1) (layer B.Cu) (net 4))
  (segment (start 141.05 101.62) (end 141.739095 101.62) (width 1) (layer B.Cu) (net 4))
  (segment (start 141.739095 101.62) (end 147.89 95.469095) (width 1) (layer B.Cu) (net 4))
  (segment (start 147.89 95.469095) (end 147.89 94.39) (width 1) (layer B.Cu) (net 4))
  (segment (start 145.37 105.1) (end 142.66 105.1) (width 1) (layer B.Cu) (net 4))
  (segment (start 142.66 105.1) (end 141.58 106.18) (width 1) (layer B.Cu) (net 4))
  (segment (start 145.37 105.1) (end 152.99 105.1) (width 1) (layer B.Cu) (net 4))
  (segment (start 113.26 110.77) (end 115.26 110.77) (width 1) (layer B.Cu) (net 5))
  (segment (start 112.832511 110.342511) (end 113.26 110.77) (width 1) (layer B.Cu) (net 5))
  (segment (start 112.832511 99.384777) (end 112.832511 110.342511) (width 1) (layer B.Cu) (net 5))
  (segment (start 125.3 92.18) (end 120.037288 92.18) (width 1) (layer B.Cu) (net 5))
  (segment (start 120.037288 92.18) (end 112.832511 99.384777) (width 1) (layer B.Cu) (net 5))
  (segment (start 125.3 94.72) (end 119.477202 94.72) (width 1) (layer B.Cu) (net 6))
  (segment (start 115.26 98.937202) (end 115.26 106.855787) (width 1) (layer B.Cu) (net 6))
  (segment (start 119.477202 94.72) (end 115.26 98.937202) (width 1) (layer B.Cu) (net 6))
  (segment (start 115.26 106.855787) (end 115.26 108.27) (width 1) (layer B.Cu) (net 6))
  (segment (start 115.26 108.27) (end 118.24 108.27) (width 1) (layer B.Cu) (net 6))
  (segment (start 118.24 108.27) (end 121.84 104.67) (width 1) (layer B.Cu) (net 6))
  (segment (start 127.84 93.45) (end 128.90066 93.45) (width 1) (layer B.Cu) (net 7))
  (segment (start 128.90066 93.45) (end 129.879999 94.429339) (width 1) (layer B.Cu) (net 7))
  (segment (start 129.879999 94.429339) (end 129.879999 104.409999) (width 1) (layer B.Cu) (net 7))
  (segment (start 130.27 104.8) (end 130.27 106.8) (width 1) (layer B.Cu) (net 7))
  (segment (start 129.879999 104.409999) (end 130.27 104.8) (width 1) (layer B.Cu) (net 7))
  (segment (start 126.16 112.26) (end 126.248445 112.26) (width 1) (layer B.Cu) (net 9))
  (segment (start 126.248445 112.26) (end 129.168445 109.34) (width 1) (layer B.Cu) (net 9))
  (segment (start 129.168445 109.34) (end 130.27 109.34) (width 1) (layer B.Cu) (net 9))
  (segment (start 133.186084 94) (end 133.43 94) (width 1) (layer B.Cu) (net 10))
  (segment (start 130.096085 90.910001) (end 133.186084 94) (width 1) (layer B.Cu) (net 10))
  (segment (start 127.84 90.91) (end 130.096085 90.910001) (width 1) (layer B.Cu) (net 10))
  (segment (start 157.71 107.61) (end 153.02 107.61) (width 1) (layer B.Cu) (net 13))
  (segment (start 153.02 107.61) (end 152.99 107.64) (width 1) (layer B.Cu) (net 13))
  (segment (start 156.53 100.22) (end 156.53 106.43) (width 1) (layer B.Cu) (net 13))
  (segment (start 156.53 106.43) (end 157.71 107.61) (width 1) (layer B.Cu) (net 13))
  (segment (start 150.35 99.88) (end 156.19 99.88) (width 1) (layer B.Cu) (net 13))
  (segment (start 156.19 99.88) (end 156.53 100.22) (width 1) (layer B.Cu) (net 13))
  (segment (start 152.99 107.64) (end 152.99 110.18) (width 1) (layer B.Cu) (net 13))
  (segment (start 141.58 111.26) (end 141.75 111.26) (width 1) (layer B.Cu) (net 14))
  (segment (start 141.75 111.26) (end 145.37 107.64) (width 1) (layer B.Cu) (net 14))
  (segment (start 137.89 109.34) (end 139.66 109.34) (width 1) (layer B.Cu) (net 14))
  (segment (start 139.66 109.34) (end 141.58 111.26) (width 1) (layer B.Cu) (net 14))

)
