(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 144)
    (no_connects 112)
    (area 44.374999 20.244999 268.045001 149.935001)
    (thickness 1.6)
    (drawings 4)
    (tracks 140)
    (zones 0)
    (modules 72)
    (nets 55)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 1)
    (uvia_drill 0.5)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(F2-Pad2)")
  (net 3 "Net-(F2-Pad1)")
  (net 4 "Net-(F3-Pad2)")
  (net 5 "Net-(F3-Pad1)")
  (net 6 "Net-(F4-Pad2)")
  (net 7 "Net-(F4-Pad1)")
  (net 8 "Net-(F5-Pad2)")
  (net 9 "Net-(F5-Pad1)")
  (net 10 CUR_1)
  (net 11 CUR_3)
  (net 12 ARD_5V)
  (net 13 CUR_2)
  (net 14 CUR_4)
  (net 15 "Net-(F1-Pad2)")
  (net 16 ARD_GND)
  (net 17 ARD_REF)
  (net 18 "Net-(J7-Pad8)")
  (net 19 "Net-(F6-Pad2)")
  (net 20 "Net-(F6-Pad1)")
  (net 21 "Net-(F7-Pad2)")
  (net 22 "Net-(F7-Pad1)")
  (net 23 "Net-(F8-Pad2)")
  (net 24 "Net-(F8-Pad1)")
  (net 25 "Net-(F9-Pad2)")
  (net 26 "Net-(F9-Pad1)")
  (net 27 "Net-(F10-Pad2)")
  (net 28 "Net-(F10-Pad1)")
  (net 29 "Net-(F11-Pad2)")
  (net 30 "Net-(F11-Pad1)")
  (net 31 "Net-(F12-Pad2)")
  (net 32 "Net-(F12-Pad1)")
  (net 33 "Net-(F13-Pad2)")
  (net 34 "Net-(F13-Pad1)")
  (net 35 "Net-(F14-Pad2)")
  (net 36 "Net-(F14-Pad1)")
  (net 37 "Net-(F15-Pad2)")
  (net 38 "Net-(F15-Pad1)")
  (net 39 "Net-(F16-Pad2)")
  (net 40 "Net-(F16-Pad1)")
  (net 41 "Net-(F17-Pad2)")
  (net 42 "Net-(F17-Pad1)")
  (net 43 CUR_9)
  (net 44 CUR_11)
  (net 45 CUR_10)
  (net 46 CUR_12)
  (net 47 CUR_5)
  (net 48 CUR_13)
  (net 49 CUR_6)
  (net 50 CUR_14)
  (net 51 CUR_7)
  (net 52 CUR_15)
  (net 53 CUR_8)
  (net 54 CUR_16)

  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 1)
    (uvia_drill 0.5)
    (add_net ARD_5V)
    (add_net ARD_GND)
    (add_net ARD_REF)
    (add_net CUR_1)
    (add_net CUR_10)
    (add_net CUR_11)
    (add_net CUR_12)
    (add_net CUR_13)
    (add_net CUR_14)
    (add_net CUR_15)
    (add_net CUR_16)
    (add_net CUR_2)
    (add_net CUR_3)
    (add_net CUR_4)
    (add_net CUR_5)
    (add_net CUR_6)
    (add_net CUR_7)
    (add_net CUR_8)
    (add_net CUR_9)
    (add_net GND)
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F10-Pad1)")
    (add_net "Net-(F10-Pad2)")
    (add_net "Net-(F11-Pad1)")
    (add_net "Net-(F11-Pad2)")
    (add_net "Net-(F12-Pad1)")
    (add_net "Net-(F12-Pad2)")
    (add_net "Net-(F13-Pad1)")
    (add_net "Net-(F13-Pad2)")
    (add_net "Net-(F14-Pad1)")
    (add_net "Net-(F14-Pad2)")
    (add_net "Net-(F15-Pad1)")
    (add_net "Net-(F15-Pad2)")
    (add_net "Net-(F16-Pad1)")
    (add_net "Net-(F16-Pad2)")
    (add_net "Net-(F17-Pad1)")
    (add_net "Net-(F17-Pad2)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(F3-Pad1)")
    (add_net "Net-(F3-Pad2)")
    (add_net "Net-(F4-Pad1)")
    (add_net "Net-(F4-Pad2)")
    (add_net "Net-(F5-Pad1)")
    (add_net "Net-(F5-Pad2)")
    (add_net "Net-(F6-Pad1)")
    (add_net "Net-(F6-Pad2)")
    (add_net "Net-(F7-Pad1)")
    (add_net "Net-(F7-Pad2)")
    (add_net "Net-(F8-Pad1)")
    (add_net "Net-(F8-Pad2)")
    (add_net "Net-(F9-Pad1)")
    (add_net "Net-(F9-Pad2)")
    (add_net "Net-(J7-Pad8)")
  )

  (net_class Power ""
    (clearance 0.5)
    (trace_width 5)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 1)
    (uvia_drill 0.5)
  )

  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 58CC8E2C) (tstamp 59A80BC8)
    (at 69.85 72.39 270)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /59A802DA)
    (fp_text reference U1 (at 3.81 -2.39 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP604 (at 3.81 17.63 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 7.62 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 16.63) (end 6.58 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 16.63) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 16.8) (end 8.7 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 16.8) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 CUR_1))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 CUR_3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 CUR_1))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 CUR_3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(F2-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_5V))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(F3-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(F5-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 CUR_2))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 CUR_4))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 CUR_2))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 CUR_4))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A7F67A)
    (at 86.04 127 180)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8067F)
    (fp_text reference F1 (at 10 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 20 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A80AFA)
    (at 84.77 44.45 180)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A7F37B)
    (fp_text reference F2 (at 10 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 "Net-(F2-Pad2)"))
    (pad 2 thru_hole circle (at 20 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 "Net-(F2-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(F2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(F2-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A80B26)
    (at 84.77 63.5 180)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A81937)
    (fp_text reference F3 (at 10 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 4 "Net-(F3-Pad2)"))
    (pad 2 thru_hole circle (at 20 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 4 "Net-(F3-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 5 "Net-(F3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 5 "Net-(F3-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A80B52)
    (at 84.77 88.9 180)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A81E2A)
    (fp_text reference F4 (at 10 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F4-Pad2)"))
    (pad 2 thru_hole circle (at 20 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F4-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A80B7E)
    (at 84.77 107.95 180)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A82012)
    (fp_text reference F5 (at 10 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
    (pad 2 thru_hole circle (at 20 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 9 "Net-(F5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 9 "Net-(F5-Pad1)"))
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A81B88)
    (at 78.74 76.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A80E6E)
    (fp_text reference R1 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(F2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A81B8E)
    (at 78.74 53.34)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A81956)
    (fp_text reference R2 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(F3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A81B94)
    (at 85.09 99.06 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A81E43)
    (fp_text reference R3 (at 3.81 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A81B9A)
    (at 78.74 118.11)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8202B)
    (fp_text reference R4 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(F5-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:RJ45 (layer F.Cu) (tedit 59511D7C) (tstamp 59A81DCA)
    (at 78.74 31.75 180)
    (tags RJ45)
    (path /59A7FB58)
    (fp_text reference J7 (at 4.7 11.18 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RJ45 (at 4.59 6.25 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.17 14.22) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end 12.06 5.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.07 -3.81) (end -3.17 -3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 -3.81) (end -3.17 5.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.06 7.52) (end 12.07 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.17 7.51) (end -3.17 14.22) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.56 -4.06) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.56 -4.06) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end 12.46 -4.06) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.46 14.47) (end -3.56 14.47) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 10.16 6.35 180) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 180) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 ARD_GND))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 ARD_5V))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 ARD_REF))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 CUR_1))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 CUR_2))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 CUR_3))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 CUR_4))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(J7-Pad8)"))
    (model ../../../../../../Development/multilevelinverter/Hardware/3D/RJ45.wrl
      (at (xyz 0.175 -0.667 0.3))
      (scale (xyz 10 10 10))
      (rotate (xyz 270 0 0))
    )
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A8305B)
    (at 212.41 137.159985)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8AF14)
    (fp_text reference F6 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 19 "Net-(F6-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 19 "Net-(F6-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 20 "Net-(F6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 20 "Net-(F6-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A83087)
    (at 209.55 70.678255)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8AF47)
    (fp_text reference F7 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 21 "Net-(F7-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 21 "Net-(F7-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 22 "Net-(F7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 22 "Net-(F7-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A830B3)
    (at 209.55 75.42695)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8AF7A)
    (fp_text reference F8 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 23 "Net-(F8-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 23 "Net-(F8-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 24 "Net-(F8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 24 "Net-(F8-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A830DF)
    (at 133.59 107.95)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8AFA7)
    (fp_text reference F9 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 25 "Net-(F9-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 25 "Net-(F9-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 26 "Net-(F9-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 26 "Net-(F9-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A8310B)
    (at 209.55 113.41651)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8A83E)
    (fp_text reference F10 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 27 "Net-(F10-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 27 "Net-(F10-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 28 "Net-(F10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 28 "Net-(F10-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A83137)
    (at 209.55 118.165205)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8A871)
    (fp_text reference F11 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 29 "Net-(F11-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 29 "Net-(F11-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 30 "Net-(F11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 30 "Net-(F11-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A83163)
    (at 209.55 122.9139)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8AFE0)
    (fp_text reference F12 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 31 "Net-(F12-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 31 "Net-(F12-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 32 "Net-(F12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 32 "Net-(F12-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A8318F)
    (at 209.55 127.662595)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8B013)
    (fp_text reference F13 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 33 "Net-(F13-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 33 "Net-(F13-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 34 "Net-(F13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 34 "Net-(F13-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A831BB)
    (at 209.55 89.673035)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8A8A4)
    (fp_text reference F14 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 35 "Net-(F14-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 35 "Net-(F14-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 36 "Net-(F14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 36 "Net-(F14-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A831E7)
    (at 209.55 65.92956)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8A8D1)
    (fp_text reference F15 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 37 "Net-(F15-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 37 "Net-(F15-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 38 "Net-(F15-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 38 "Net-(F15-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A83213)
    (at 209.55 84.92434)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8B046)
    (fp_text reference F16 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 39 "Net-(F16-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 39 "Net-(F16-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 40 "Net-(F16-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 40 "Net-(F16-Pad1)"))
  )

  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I (layer F.Cu) (tedit 5880C3AD) (tstamp 59A8323F)
    (at 209.55 132.41129)
    (descr "Fuseholder, 5x20, open, horizontal, Type-I, Inline,")
    (tags "Fuseholder 5x20 open horizontal Type-I Inline Sicherungshalter offen ")
    (path /59A8B073)
    (fp_text reference F17 (at 10 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 11.27 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 0) (end 15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2 -2.5) (end 22 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 22 2.5) (end -2 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2 2.5) (end -2 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 -3.4) (end 13.35 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.35 3.4) (end 22.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 3.4) (end 22.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 22.9 -3.4) (end 13.35 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.95 -3.4) (end 6.65 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 -3.4) (end 6.65 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.65 3.4) (end -2.9 3.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.9 3.4) (end -2.9 -3.4) (layer F.Fab) (width 0.1))
    (fp_line (start 13.25 0) (end 6.75 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.25 -3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 3.5) (end 13.25 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -3.5) (end 13.25 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2.5) (end -2 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.5 2.5) (end -0.75 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.25 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 2.5) (end 11.5 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 11.25 -2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 22 -2.5) (end 22 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 22 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 -3.5) (end 23 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 23 3.5) (end 22 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 -2.5) (end -2 2.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end -3 -3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3 -3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3.5) (end -3 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 -3.5) (end 6.75 3.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.2 -3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end 23.15 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 23.15 3.65) (end -3.2 3.65) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole circle (at 15 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 41 "Net-(F17-Pad2)"))
    (pad 2 thru_hole circle (at 20 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 41 "Net-(F17-Pad2)"))
    (pad 1 thru_hole circle (at 5 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 42 "Net-(F17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 42 "Net-(F17-Pad1)"))
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832BD)
    (at 252.73 32.688695)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8AF33)
    (fp_text reference R5 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(F6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832C3)
    (at 209.55 94.42173)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8AF60)
    (fp_text reference R6 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(F7-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832C9)
    (at 252.73 37.43739)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8AF93)
    (fp_text reference R7 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(F8-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832CF)
    (at 209.55 99.170425)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8AFC0)
    (fp_text reference R8 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(F9-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832D5)
    (at 209.55 103.91912)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8A85D)
    (fp_text reference R9 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(F10-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832DB)
    (at 209.55 108.667815)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8A88A)
    (fp_text reference R10 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(F11-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832E1)
    (at 252.73 46.93478)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8AFFF)
    (fp_text reference R11 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(F12-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832E7)
    (at 252.73 51.683475)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8B02C)
    (fp_text reference R12 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(F13-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832ED)
    (at 252.73 42.186085)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8A8BD)
    (fp_text reference R13 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(F14-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832F3)
    (at 252.73 56.43217)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8A8EA)
    (fp_text reference R14 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(F15-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832F9)
    (at 252.73 27.94)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8B05F)
    (fp_text reference R15 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(F16-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59A832FF)
    (at 252.73 61.180865)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59A8B08C)
    (fp_text reference R16 (at 3.81 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 -0.98) (end 0.6 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 -1.31) (end 7.02 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 -1.31) (end 7.02 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.98) (end 0.6 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 1.31) (end 7.02 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.02 1.31) (end 7.02 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 8.7 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 1.6) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(F17-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-14_W7.62mm placed (layer F.Cu) (tedit 58CC8E2C) (tstamp 59A83321)
    (at 127 80.01 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /59A8AF26)
    (fp_text reference U2 (at 3.81 -2.39 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP604 (at 3.81 17.63 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 16.63) (end 6.58 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 16.63) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 16.8) (end 8.7 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 16.8) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 CUR_9))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 CUR_11))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 CUR_9))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 CUR_11))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(F6-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(F8-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_5V))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(F7-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(F9-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CUR_10))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 CUR_12))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CUR_10))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 CUR_12))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-14_W7.62mm placed (layer F.Cu) (tedit 58CC8E2C) (tstamp 59A83343)
    (at 182.88 80.01 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /59A8A850)
    (fp_text reference U3 (at 3.81 -2.39 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP604 (at 3.81 17.63 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 16.63) (end 6.58 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 16.63) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 16.8) (end 8.7 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 16.8) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 CUR_5))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 CUR_13))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 CUR_5))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 CUR_13))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(F10-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(F12-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_5V))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(F11-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(F13-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 CUR_6))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 CUR_14))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 CUR_6))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 CUR_14))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_DIP:DIP-14_W7.62mm placed (layer F.Cu) (tedit 58CC8E2C) (tstamp 59A83365)
    (at 245.11 80.01 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (path /59A8A8FE)
    (fp_text reference U4 (at 3.81 -2.39 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP604 (at 3.81 17.63 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.39) (end 1.04 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -1.39) (end 1.04 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 16.63) (end 6.58 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 16.63) (end 6.58 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.58 -1.39) (end 4.81 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.6) (end -1.1 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 16.8) (end 8.7 16.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 16.8) (end 8.7 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.6) (end -1.1 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.39) (end 2.81 -1.39) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 CUR_7))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 CUR_15))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 CUR_7))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 CUR_15))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(F14-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(F16-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 ARD_5V))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(F15-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(F17-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 CUR_8))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 CUR_16))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 CUR_8))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 CUR_16))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84050)
    (at 50.8 127)
    (path /59A80685)
    (fp_text reference J1 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84055)
    (at 50.8 44.45)
    (path /59A7F5EE)
    (fp_text reference J2 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 2 "Net-(F2-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8405A)
    (at 50.8 63.5)
    (path /59A8193D)
    (fp_text reference J3 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 4 "Net-(F3-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8405F)
    (at 101.6 127)
    (path /59A8068B)
    (fp_text reference J4 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84064)
    (at 101.6 44.45)
    (path /59A7F611)
    (fp_text reference J5 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 3 "Net-(F2-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84069)
    (at 101.6 63.5)
    (path /59A81943)
    (fp_text reference J6 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 5 "Net-(F3-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8406E)
    (at 50.8 88.9)
    (path /59A81E30)
    (fp_text reference J8 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 6 "Net-(F4-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84073)
    (at 50.8 107.95)
    (path /59A82018)
    (fp_text reference J9 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84078)
    (at 101.6 88.9)
    (path /59A81E36)
    (fp_text reference J10 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8407D)
    (at 101.6 107.95)
    (path /59A8201E)
    (fp_text reference J11 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 9 "Net-(F5-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84082)
    (at 152.515444 168.825001)
    (path /59A8AF1A)
    (fp_text reference J12 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 19 "Net-(F6-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84087)
    (at 235.180888 168.825001)
    (path /59A8AF4D)
    (fp_text reference J13 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 21 "Net-(F7-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8408C)
    (at 221.403314 168.825001)
    (path /59A8AF20)
    (fp_text reference J14 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 20 "Net-(F6-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84091)
    (at 180.070592 168.825001)
    (path /59A8AF53)
    (fp_text reference J15 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 22 "Net-(F7-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A84096)
    (at 255.847249 168.825001)
    (path /59A8AF80)
    (fp_text reference J16 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 23 "Net-(F8-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A8409B)
    (at 179.07 97.79)
    (path /59A8AFAD)
    (fp_text reference J17 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 25 "Net-(F9-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840A0)
    (at 104.293935 168.825001)
    (path /59A8AF86)
    (fp_text reference J18 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 24 "Net-(F8-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840A5)
    (at 297.179971 168.825001)
    (path /59A8AFB3)
    (fp_text reference J19 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 26 "Net-(F9-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840AA)
    (at 138.73787 168.825001)
    (path /59A8A844)
    (fp_text reference J20 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 27 "Net-(F10-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840AF)
    (at 193.848166 168.825001)
    (path /59A8A877)
    (fp_text reference J21 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 29 "Net-(F11-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840B4)
    (at 173.181805 168.825001)
    (path /59A8AFE6)
    (fp_text reference J22 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 31 "Net-(F12-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840B9)
    (at 166.293018 168.825001)
    (path /59A8B019)
    (fp_text reference J23 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 33 "Net-(F13-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840BE)
    (at 269.624823 168.825001)
    (path /59A8A84A)
    (fp_text reference J24 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 28 "Net-(F10-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840C3)
    (at 111.182722 168.825001)
    (path /59A8A87D)
    (fp_text reference J25 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 30 "Net-(F11-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840C8)
    (at 248.958462 168.825001)
    (path /59A8AFEC)
    (fp_text reference J26 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 32 "Net-(F12-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840CD)
    (at 214.514527 168.825001)
    (path /59A8B01F)
    (fp_text reference J27 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 34 "Net-(F13-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840D2)
    (at 159.404231 168.825001)
    (path /59A8A8AA)
    (fp_text reference J28 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 35 "Net-(F14-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840D7)
    (at 283.402397 168.825001)
    (path /59A8A8D7)
    (fp_text reference J29 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 37 "Net-(F15-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840DC)
    (at 124.960296 168.825001)
    (path /59A8B04C)
    (fp_text reference J30 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 39 "Net-(F16-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840E1)
    (at 145.626657 168.825001)
    (path /59A8B079)
    (fp_text reference J31 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IN (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 41 "Net-(F17-Pad2)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840E6)
    (at 207.62574 168.825001)
    (path /59A8A8B0)
    (fp_text reference J32 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 36 "Net-(F14-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840EB)
    (at 242.069675 168.825001)
    (path /59A8A8DD)
    (fp_text reference J33 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 38 "Net-(F15-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840F0)
    (at 259.08 157.48)
    (path /59A8B052)
    (fp_text reference J34 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 40 "Net-(F16-Pad1)"))
  )

  (module PartsLibraries:PowerConnectorRound (layer F.Cu) (tedit 59A824E3) (tstamp 59A840F5)
    (at 276.51361 168.825001)
    (path /59A8B07F)
    (fp_text reference J35 (at 0.254 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OUT (at 0 4.064) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.3) (layers *.Cu *.Mask)
      (net 42 "Net-(F17-Pad1)"))
  )

  (gr_line (start 267.97 20.32) (end 44.45 20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 267.97 149.86) (end 267.97 20.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.45 149.86) (end 267.97 149.86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.45 20.32) (end 44.45 149.86) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 86.04 127) (end 101.6 127) (width 5) (layer B.Cu) (net 1))
  (segment (start 77.47 99.06) (end 82.55 93.98) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 82.55 93.98) (end 82.55 86.36) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 82.55 86.36) (end 86.36 82.55) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.36 82.55) (end 86.36 76.2) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.36 118.11) (end 82.55 114.3) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 82.55 114.3) (end 82.55 105.41) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 82.55 105.41) (end 77.47 100.33) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 77.47 100.33) (end 77.47 99.06) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.36 76.2) (end 83.82 78.74) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 83.82 78.74) (end 76.2 78.74) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 76.2 78.74) (end 74.93 77.47) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 74.93 77.47) (end 62.23 77.47) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 62.23 77.47) (end 62.23 80.01) (width 1) (layer B.Cu) (net 1) (status 80000))
  (segment (start 86.36 76.2) (end 87.63 74.93) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 87.63 74.93) (end 87.63 60.96) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 87.63 60.96) (end 86.36 59.69) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.36 59.69) (end 86.36 53.34) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.04 127) (end 86.36 127) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.36 127) (end 86.36 118.11) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 86.04 127) (end 86.36 127) (width 1) (layer F.Cu) (net 1) (status 80000))
  (segment (start 81.04 127) (end 86.04 127) (width 5) (layer B.Cu) (net 1))
  (segment (start 50.8 44.45) (end 64.77 44.45) (width 5) (layer B.Cu) (net 2))
  (segment (start 64.77 44.45) (end 69.77 44.45) (width 5) (layer B.Cu) (net 2))
  (segment (start 84.77 44.45) (end 101.6 44.45) (width 5) (layer B.Cu) (net 3))
  (segment (start 81.28 67.31) (end 76.2 67.31) (width 1) (layer B.Cu) (net 3))
  (segment (start 76.2 67.31) (end 71.12 67.31) (width 1) (layer B.Cu) (net 3))
  (segment (start 76.26999 67.24001) (end 76.2 67.31) (width 1) (layer B.Cu) (net 3))
  (segment (start 79.77 44.45) (end 80.944999 45.624999) (width 1) (layer B.Cu) (net 3))
  (segment (start 80.944999 45.624999) (end 80.944999 57.37524) (width 1) (layer B.Cu) (net 3))
  (segment (start 80.944999 57.37524) (end 76.26999 62.050249) (width 1) (layer B.Cu) (net 3))
  (segment (start 76.26999 62.050249) (end 76.26999 67.24001) (width 1) (layer B.Cu) (net 3))
  (segment (start 78.74 76.2) (end 78.74 74.93) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 78.74 74.93) (end 82.55 71.12) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 82.55 71.12) (end 82.55 68.58) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 82.55 68.58) (end 81.28 67.31) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 71.12 67.31) (end 68.58 69.85) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 68.58 69.85) (end 64.77 69.85) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 64.77 69.85) (end 64.77 72.39) (width 1) (layer B.Cu) (net 3) (status 80000))
  (segment (start 79.77 44.45) (end 80.01 44.45) (width 1) (layer F.Cu) (net 3) (status 80000))
  (segment (start 79.77 44.45) (end 84.77 44.45) (width 5) (layer B.Cu) (net 3))
  (segment (start 50.8 63.5) (end 64.77 63.5) (width 5) (layer B.Cu) (net 4))
  (segment (start 64.77 63.5) (end 69.77 63.5) (width 5) (layer B.Cu) (net 4))
  (segment (start 84.77 63.5) (end 101.6 63.5) (width 5) (layer B.Cu) (net 5))
  (segment (start 78.74 69.85) (end 78.74 64.53) (width 1) (layer F.Cu) (net 5))
  (segment (start 78.74 64.53) (end 79.77 63.5) (width 1) (layer F.Cu) (net 5))
  (segment (start 74.399999 74.190001) (end 78.74 69.85) (width 1) (layer B.Cu) (net 5))
  (via (at 78.74 69.85) (size 1.5) (drill 1) (layers F.Cu B.Cu) (net 5))
  (segment (start 59.69 72.39) (end 59.69 73.52137) (width 1) (layer B.Cu) (net 5))
  (segment (start 60.358631 74.190001) (end 74.399999 74.190001) (width 1) (layer B.Cu) (net 5))
  (segment (start 59.69 73.52137) (end 60.358631 74.190001) (width 1) (layer B.Cu) (net 5))
  (segment (start 79.77 63.5) (end 80.01 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 80.01 63.5) (end 78.74 62.23) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 78.74 62.23) (end 78.74 53.34) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 79.77 63.5) (end 80.01 63.5) (width 1) (layer B.Cu) (net 5) (status 80000))
  (segment (start 79.77 63.5) (end 80.01 63.5) (width 1) (layer F.Cu) (net 5) (status 80000))
  (segment (start 79.77 63.5) (end 84.77 63.5) (width 5) (layer B.Cu) (net 5))
  (segment (start 50.8 88.9) (end 64.77 88.9) (width 5) (layer B.Cu) (net 6))
  (segment (start 64.77 88.9) (end 69.77 88.9) (width 5) (layer B.Cu) (net 6))
  (segment (start 84.77 88.9) (end 101.6 88.9) (width 5) (layer B.Cu) (net 7))
  (segment (start 79.77 88.9) (end 80.01 88.9) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 80.01 88.9) (end 78.74 87.63) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 78.74 87.63) (end 76.2 87.63) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 76.2 87.63) (end 71.12 82.55) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 71.12 82.55) (end 59.69 82.55) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 59.69 82.55) (end 59.69 80.01) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 84.77 88.9) (end 85.09 88.9) (width 1) (layer F.Cu) (net 7) (status 80000))
  (segment (start 85.09 88.9) (end 85.09 99.06) (width 1) (layer F.Cu) (net 7) (status 80000))
  (segment (start 79.77 88.9) (end 80.01 88.9) (width 1) (layer B.Cu) (net 7) (status 80000))
  (segment (start 84.77 88.9) (end 85.09 88.9) (width 1) (layer F.Cu) (net 7) (status 80000))
  (segment (start 79.77 88.9) (end 84.77 88.9) (width 5) (layer B.Cu) (net 7))
  (segment (start 50.8 107.95) (end 64.77 107.95) (width 5) (layer B.Cu) (net 8))
  (segment (start 64.77 107.95) (end 69.77 107.95) (width 5) (layer B.Cu) (net 8))
  (segment (start 84.77 107.95) (end 101.6 107.95) (width 5) (layer B.Cu) (net 9))
  (segment (start 79.77 107.95) (end 80.01 107.95) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 80.01 107.95) (end 67.31 95.25) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 67.31 95.25) (end 67.31 86.36) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 67.31 86.36) (end 64.77 83.82) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 64.77 83.82) (end 64.77 80.01) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 79.77 107.95) (end 80.01 107.95) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 80.01 107.95) (end 78.74 109.22) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 78.74 109.22) (end 78.74 118.11) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 79.77 107.95) (end 80.01 107.95) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 79.77 107.95) (end 80.01 107.95) (width 1) (layer F.Cu) (net 9) (status 80000))
  (segment (start 79.77 107.95) (end 84.77 107.95) (width 5) (layer B.Cu) (net 9))
  (segment (start 72.455112 72.39) (end 74.847557 69.997555) (width 1) (layer B.Cu) (net 10))
  (segment (start 74.847557 69.997555) (end 75.597556 69.247556) (width 1) (layer B.Cu) (net 10))
  (via (at 75.597556 69.247556) (size 1.5) (drill 1) (layers F.Cu B.Cu) (net 10))
  (segment (start 69.85 72.39) (end 72.455112 72.39) (width 1) (layer B.Cu) (net 10))
  (segment (start 74.93 34.29) (end 74.93 68.58) (width 1) (layer F.Cu) (net 10))
  (segment (start 74.93 68.58) (end 75.597556 69.247556) (width 1) (layer F.Cu) (net 10))
  (segment (start 67.31 72.39) (end 69.85 72.39) (width 1) (layer F.Cu) (net 10))
  (segment (start 63.5 38.1) (end 63.5 40.64) (width 1) (layer F.Cu) (net 11))
  (segment (start 63.5 40.64) (end 62.23 41.91) (width 1) (layer F.Cu) (net 11))
  (segment (start 62.23 41.91) (end 62.23 60.699663) (width 1) (layer F.Cu) (net 11))
  (segment (start 62.23 60.699663) (end 60.636149 62.293514) (width 1) (layer F.Cu) (net 11))
  (segment (start 60.636149 62.293514) (end 60.636149 64.9224) (width 1) (layer F.Cu) (net 11))
  (segment (start 60.636149 64.9224) (end 54.96855 70.589999) (width 1) (layer F.Cu) (net 11))
  (segment (start 54.96855 70.589999) (end 53.745999 70.589999) (width 1) (layer F.Cu) (net 11))
  (segment (start 53.745999 70.589999) (end 52.809999 71.525999) (width 1) (layer F.Cu) (net 11))
  (segment (start 52.809999 71.525999) (end 52.809999 78.209999) (width 1) (layer F.Cu) (net 11))
  (segment (start 52.809999 78.209999) (end 53.810001 79.210001) (width 1) (layer F.Cu) (net 11))
  (segment (start 53.810001 79.210001) (end 54.61 80.01) (width 1) (layer F.Cu) (net 11))
  (segment (start 54.61 80.01) (end 57.15 80.01) (width 1) (layer F.Cu) (net 11))
  (via (at 63.5 38.1) (size 1.5) (layers F.Cu B.Cu) (net 11) (status 80000))
  (segment (start 63.5 38.1) (end 64.77 36.83) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 64.77 36.83) (end 71.12 36.83) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 71.12 36.83) (end 72.39 35.56) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 72.39 35.56) (end 72.39 34.29) (width 1) (layer B.Cu) (net 11) (status 80000))
  (segment (start 63.98001 58.21066) (end 63.98001 57.15) (width 1) (layer F.Cu) (net 12))
  (segment (start 77.47 34.29) (end 76.2 35.56) (width 1) (layer B.Cu) (net 12))
  (segment (start 62.23 62.820997) (end 63.98001 61.070987) (width 1) (layer F.Cu) (net 12))
  (segment (start 62.23 72.39) (end 62.23 62.820997) (width 1) (layer F.Cu) (net 12))
  (segment (start 76.2 35.56) (end 76.2 44.93001) (width 1) (layer B.Cu) (net 12))
  (via (at 63.98001 57.15) (size 1.5) (drill 1) (layers F.Cu B.Cu) (net 12))
  (segment (start 76.2 44.93001) (end 64.730009 56.400001) (width 1) (layer B.Cu) (net 12))
  (segment (start 63.98001 61.070987) (end 63.98001 58.21066) (width 1) (layer F.Cu) (net 12))
  (segment (start 64.730009 56.400001) (end 63.98001 57.15) (width 1) (layer B.Cu) (net 12))
  (segment (start 80.740013 70.660657) (end 80.740013 69.85) (width 1) (layer B.Cu) (net 13))
  (segment (start 59.318642 75.690012) (end 75.710658 75.690012) (width 1) (layer B.Cu) (net 13))
  (segment (start 57.15 73.52137) (end 59.318642 75.690012) (width 1) (layer B.Cu) (net 13))
  (segment (start 82.55 68.040013) (end 81.490012 69.100001) (width 1) (layer F.Cu) (net 13))
  (segment (start 76.2 29.21) (end 81.28 29.21) (width 1) (layer F.Cu) (net 13))
  (segment (start 73.66 31.75) (end 76.2 29.21) (width 1) (layer F.Cu) (net 13))
  (segment (start 75.710658 75.690012) (end 80.740013 70.660657) (width 1) (layer B.Cu) (net 13))
  (segment (start 81.28 29.21) (end 82.55 30.48) (width 1) (layer F.Cu) (net 13))
  (segment (start 57.15 72.39) (end 57.15 73.52137) (width 1) (layer B.Cu) (net 13))
  (segment (start 81.490012 69.100001) (end 80.740013 69.85) (width 1) (layer F.Cu) (net 13))
  (via (at 80.740013 69.85) (size 1.5) (drill 1) (layers F.Cu B.Cu) (net 13))
  (segment (start 82.55 30.48) (end 82.55 68.040013) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.61 72.39) (end 57.15 72.39) (width 1) (layer F.Cu) (net 13))
  (segment (start 69.85 80.01) (end 67.31 80.01) (width 1) (layer F.Cu) (net 14))
  (segment (start 69.85 80.01) (end 72.39 77.47) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 72.39 77.47) (end 72.39 60.96) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 72.39 60.96) (end 67.31 55.88) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 67.31 55.88) (end 67.31 33.02) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 67.31 33.02) (end 68.58 31.75) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 68.58 31.75) (end 71.12 31.75) (width 1) (layer F.Cu) (net 14) (status 80000))
  (segment (start 50.8 127) (end 66.04 127) (width 5) (layer B.Cu) (net 15))
  (segment (start 66.04 127) (end 71.04 127) (width 5) (layer B.Cu) (net 15))

)
