EESchema Schematic File Version 2
LIBS:OAE.Parts
LIBS:power
LIBS:device
LIBS:transistors
LIBS:conn
LIBS:linear
LIBS:regul
LIBS:74xx
LIBS:cmos4000
LIBS:adc-dac
LIBS:memory
LIBS:xilinx
LIBS:microcontrollers
LIBS:dsp
LIBS:microchip
LIBS:analog_switches
LIBS:motorola
LIBS:texas
LIBS:intel
LIBS:audio
LIBS:interface
LIBS:digital-audio
LIBS:philips
LIBS:display
LIBS:cypress
LIBS:siliconi
LIBS:opto
LIBS:atmel
LIBS:contrib
LIBS:valves
LIBS:PsuSwitchModule-cache
EELAYER 25 0
EELAYER END
$Descr A4 11693 8268
encoding utf-8
Sheet 1 5
Title "Power Module (Control Board)"
Date "2017-12-14"
Rev "Rev3.3"
Comp "Enertechnos Ltd"
Comment1 "FOR REVIEW"
Comment2 ""
Comment3 ""
Comment4 ""
$EndDescr
Text GLabel 2250 3150 0    60   Output ~ 0
ARD_PWM_C
Text GLabel 2250 3250 0    60   Output ~ 0
ARD_PWM_D
$Sheet
S 4550 1800 1250 1100
U 59498AA5
F0 "PsuSwitchModule.Switch.1" 60
F1 "PsuSwitchModule.Switch.sch" 60
F2 "ARD_PWM" I L 4550 2050 60 
F3 "DC_GND" U L 4550 2500 60 
F4 "DC_IN" I L 4550 2650 60 
F5 "ARD_GND" U L 4550 1900 60 
F6 "DRV_SIG" O R 5800 2300 60 
F7 "GND_ISO" U R 5800 2600 60 
$EndSheet
Text GLabel 4550 2050 0    60   Input ~ 0
ARD_PWM_A
Text GLabel 4550 1900 0    60   UnSpc ~ 0
ARD_GND
$Comp
L RJ45 J1
U 1 1 59526541
P 2700 2100
F 0 "J1" H 2900 2600 50  0000 C CNN
F 1 "Monitor" H 2550 2600 50  0000 C CNN
F 2 "PartsLibraries:RJ45" H 2700 2100 50  0001 C CNN
F 3 "" H 2700 2100 50  0001 C CNN
	1    2700 2100
	0    1    1    0   
$EndComp
$Comp
L Conn_01x02 J2
U 1 1 599EAAF2
P 2750 4100
F 0 "J2" H 2750 4250 50  0000 C CNN
F 1 "Temperature Probe" V 2850 4100 50  0000 C CNN
F 2 "Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight" H 2750 4100 50  0001 C CNN
F 3 "" H 2750 4100 50  0001 C CNN
	1    2750 4100
	1    0    0    -1  
$EndComp
$Comp
L R R1
U 1 1 599EAAF9
P 2400 4450
F 0 "R1" V 2300 4450 50  0000 C CNN
F 1 "100" V 2400 4450 50  0000 C CNN
F 2 "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" V 2330 4450 50  0001 C CNN
F 3 "" H 2400 4450 50  0001 C CNN
	1    2400 4450
	1    0    0    -1  
$EndComp
Text Notes 1650 5400 0    60   ~ 0
The resistance is matched to the\nR value of the attached thermistor
Wire Wire Line
	2550 4200 2250 4200
Connection ~ 2400 4200
Wire Wire Line
	2400 4200 2400 4300
Wire Wire Line
	2400 4600 2400 4700
Text GLabel 4550 2500 0    60   UnSpc ~ 0
DC_GND
Text GLabel 4550 2650 0    60   Input ~ 0
DC_IN
$Sheet
S 4550 3400 1250 1100
U 59A7109E
F0 "PsuSwitchModule.Switch.2" 60
F1 "PsuSwitchModule.Switch.sch" 60
F2 "ARD_PWM" I L 4550 3650 60 
F3 "DC_GND" U L 4550 4100 60 
F4 "DC_IN" I L 4550 4250 60 
F5 "ARD_GND" U L 4550 3500 60 
F6 "DRV_SIG" O R 5800 3800 60 
F7 "GND_ISO" U R 5800 4100 60 
$EndSheet
Text GLabel 4550 3650 0    60   Input ~ 0
ARD_PWM_B
Text GLabel 4550 3500 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 4550 4100 0    60   UnSpc ~ 0
DC_GND
Text GLabel 4550 4250 0    60   Input ~ 0
DC_IN
$Sheet
S 6850 1800 1250 1100
U 59A71299
F0 "PsuSwitchModule.Switch.3" 60
F1 "PsuSwitchModule.Switch.sch" 60
F2 "ARD_PWM" I L 6850 2050 60 
F3 "DC_GND" U L 6850 2500 60 
F4 "DC_IN" I L 6850 2650 60 
F5 "ARD_GND" U L 6850 1900 60 
F6 "DRV_SIG" O R 8100 2250 60 
F7 "GND_ISO" U R 8100 2550 60 
$EndSheet
Text GLabel 6850 2050 0    60   Input ~ 0
ARD_PWM_C
Text GLabel 6850 1900 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 6850 2500 0    60   UnSpc ~ 0
DC_GND
Text GLabel 6850 2650 0    60   Input ~ 0
DC_IN
$Sheet
S 6850 3400 1250 1100
U 59A712A3
F0 "PsuSwitchModule.Switch.4" 60
F1 "PsuSwitchModule.Switch.sch" 60
F2 "ARD_PWM" I L 6850 3650 60 
F3 "DC_GND" U L 6850 4100 60 
F4 "DC_IN" I L 6850 4250 60 
F5 "ARD_GND" U L 6850 3500 60 
F6 "GND_ISO" U R 8100 4100 60 
F7 "DRV_SIG" O R 8100 3800 60 
$EndSheet
Text GLabel 6850 3650 0    60   Input ~ 0
ARD_PWM_D
Text GLabel 6850 3500 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 6850 4100 0    60   UnSpc ~ 0
DC_GND
Text GLabel 6850 4250 0    60   Input ~ 0
DC_IN
Text GLabel 2550 4100 0    60   Input ~ 0
ARD_VCC
Text GLabel 2250 4200 0    60   Output ~ 0
ARD_TEMP
Text GLabel 2250 2450 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 2250 2950 0    60   Output ~ 0
ARD_PWM_A
Text GLabel 2250 2850 0    60   UnSpc ~ 0
DC_GND
Text GLabel 2250 2750 0    60   Output ~ 0
DC_IN
Text GLabel 2250 3050 0    60   Output ~ 0
ARD_PWM_B
Text GLabel 2250 2350 0    60   Output ~ 0
ARD_VCC
Text GLabel 2250 2250 0    60   Input ~ 0
ARD_TEMP
$Comp
L RJ45 J7
U 1 1 59A7EBD8
P 2700 3100
F 0 "J7" H 2900 3600 50  0000 C CNN
F 1 "Control" H 2550 3600 50  0000 C CNN
F 2 "PartsLibraries:RJ45" H 2700 3100 50  0001 C CNN
F 3 "" H 2700 3100 50  0001 C CNN
	1    2700 3100
	0    1    1    0   
$EndComp
$Comp
L RJ45 J3
U 1 1 5A16B56F
P 10150 3150
F 0 "J3" H 10350 3650 50  0000 C CNN
F 1 "SignalToPower" H 10000 3650 50  0000 C CNN
F 2 "PartsLibraries:RJ45" H 10150 3150 50  0001 C CNN
F 3 "" H 10150 3150 50  0001 C CNN
	1    10150 3150
	0    1    1    0   
$EndComp
Text GLabel 5800 2300 2    60   Output ~ 0
DRV_GATE_A
Text GLabel 5800 2600 2    60   UnSpc ~ 0
GND_ISO_1
Text GLabel 8100 2250 2    60   Output ~ 0
DRV_GATE_C
Text GLabel 8100 2550 2    60   UnSpc ~ 0
GND_ISO_3
Text GLabel 5800 3800 2    60   Output ~ 0
DRV_GATE_B
Text GLabel 5800 4100 2    60   UnSpc ~ 0
GND_ISO_2
Text GLabel 8100 3800 2    60   Output ~ 0
DRV_GATE_D
Text GLabel 8100 4100 2    60   UnSpc ~ 0
GND_ISO_4
Text GLabel 9700 3400 0    60   Input ~ 0
DRV_GATE_A
Text GLabel 9700 3200 0    60   UnSpc ~ 0
GND_ISO_1
Text GLabel 9700 3300 0    60   Input ~ 0
DRV_GATE_B
Text GLabel 9700 3500 0    60   UnSpc ~ 0
GND_ISO_2
Text GLabel 9700 3000 0    60   Input ~ 0
DRV_GATE_C
Text GLabel 9700 2800 0    60   UnSpc ~ 0
GND_ISO_3
Text GLabel 9700 2900 0    60   Input ~ 0
DRV_GATE_D
Text GLabel 9700 3100 0    60   UnSpc ~ 0
GND_ISO_4
Text Notes 1250 1550 0    60   ~ 0
In the event there are 2 arduinos on the control board \n(one for driving, the other for monitoring) the runs for \neach should be kept on separate RJ45s for clarity.
Text GLabel 2400 4700 3    60   UnSpc ~ 0
ARD_GND
$Comp
L Conn_01x03 J101
U 1 1 5A3469C9
P 10200 4050
F 0 "J101" H 10200 4250 50  0000 C CNN
F 1 "Conn_01x03" H 10200 3850 50  0000 C CNN
F 2 "Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight" H 10200 4050 50  0001 C CNN
F 3 "" H 10200 4050 50  0001 C CNN
	1    10200 4050
	1    0    0    -1  
$EndComp
Text GLabel 2250 1750 0    60   Input ~ 0
ARD_CUR
Text GLabel 10000 3950 0    60   Output ~ 0
ARD_CUR
Text GLabel 10000 4050 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 10000 4150 0    60   Input ~ 0
ARD_VCC
$EndSCHEMATC
