EESchema Schematic File Version 2
LIBS:OAE.Parts
LIBS:power
LIBS:device
LIBS:transistors
LIBS:conn
LIBS:linear
LIBS:regul
LIBS:74xx
LIBS:cmos4000
LIBS:adc-dac
LIBS:memory
LIBS:xilinx
LIBS:microcontrollers
LIBS:dsp
LIBS:microchip
LIBS:analog_switches
LIBS:motorola
LIBS:texas
LIBS:intel
LIBS:audio
LIBS:interface
LIBS:digital-audio
LIBS:philips
LIBS:display
LIBS:cypress
LIBS:siliconi
LIBS:opto
LIBS:atmel
LIBS:contrib
LIBS:valves
LIBS:BreakoutBoard-cache
EELAYER 25 0
EELAYER END
$Descr User 8268 5846
encoding utf-8
Sheet 10 10
Title "Breakout Board"
Date "2018-01-04"
Rev "Release 0.1"
Comp "Enertechnos Ltd."
Comment1 "APPROVED for Prototype"
Comment2 ""
Comment3 "As such ANALOG INPUTS must receive voltage not higher than 3.3V."
Comment4 "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."
$EndDescr
$Comp
L RJ45 J801
U 1 1 5A31FF65
P 2150 2000
AR Path="/5A31FD72/5A31FF65" Ref="J801"  Part="1" 
AR Path="/5A320551/5A31FF65" Ref="J802"  Part="1" 
AR Path="/5A332152/5A31FF65" Ref="J901"  Part="1" 
AR Path="/5A3324C4/5A31FF65" Ref="J1001"  Part="1" 
F 0 "J1001" H 2350 2500 50  0000 C CNN
F 1 "RJ45" H 2000 2500 50  0000 C CNN
F 2 "PartsLibraries:RJ45" H 2150 2000 50  0001 C CNN
F 3 "" H 2150 2000 50  0001 C CNN
	1    2150 2000
	0    1    1    0   
$EndComp
Text GLabel 1700 1650 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 1700 1850 0    60   Input ~ 0
ARD_VCC
Text HLabel 1700 1750 0    60   Input ~ 0
A
Text HLabel 1700 1950 0    60   Input ~ 0
B
Text HLabel 1700 2150 0    60   Input ~ 0
C
Text HLabel 1700 2350 0    60   Output ~ 0
COM
$EndSCHEMATC
