(module TerminalBlock_2_P5.00mm (layer F.Cu) (tedit 5B575216)
  (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
  (tags "Altech AK300 terminal block pitch 5.0mm")
  (fp_text reference J501 (at -5.24 0 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Conn_01x02_Male (at 3 7.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 -5) (end -3 6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 6) (end 8 6) (layer F.SilkS) (width 0.12))
  (fp_line (start 8 6) (end 8 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 8 5) (end 8.5 5.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.5 5.5) (end 8.5 3.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.5 3.5) (end 8 4) (layer F.SilkS) (width 0.12))
  (fp_line (start 8 4) (end 8 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 8 -1.5) (end 8.5 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.5 -1) (end 8.5 -5) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.5 -5) (end -3 -5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.5 -5.5) (end 9 -5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.5 -5.5) (end -3.5 6.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 6.5) (end 9 -5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 6.5) (end -3.5 6.5) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 2 thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask))
  (model C:/Development/mlihardware/3D/13986.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
