(module RJ45-shielded-Molex (layer F.Cu) (tedit 5AC4A305)
  (tags RJ45)
  (fp_text reference J7 (at -0.6 -6.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Control (at 9 -6.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.2 13) (end 12.2 13) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.2 -3.8) (end 12.2 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.2 -3.8) (end -3.2 -3.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.2 -3.8) (end -3.2 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.2 11) (end 12.2 13) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.2 11) (end -3.2 13) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.6 -4.1) (end 12.5 -4.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 -4.1) (end -3.6 13.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.5 13.3) (end 12.5 -4.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.5 13.3) (end -3.6 13.3) (layer F.CrtYd) (width 0.05))
  (pad "" np_thru_hole circle (at 10.16 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
  (pad "" np_thru_hole circle (at -1.27 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -3.355 9.4) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 9 thru_hole circle (at 12.245 9.4) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
    (zone_connect 2))
  (model "C:/Development/mlihardware/3D/RJ45 Shielded Molex.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
