EESchema Schematic File Version 2
LIBS:OAE.Parts
LIBS:power
LIBS:device
LIBS:transistors
LIBS:conn
LIBS:linear
LIBS:regul
LIBS:74xx
LIBS:cmos4000
LIBS:adc-dac
LIBS:memory
LIBS:xilinx
LIBS:microcontrollers
LIBS:dsp
LIBS:microchip
LIBS:analog_switches
LIBS:motorola
LIBS:texas
LIBS:intel
LIBS:audio
LIBS:interface
LIBS:digital-audio
LIBS:philips
LIBS:display
LIBS:cypress
LIBS:siliconi
LIBS:opto
LIBS:atmel
LIBS:contrib
LIBS:valves
LIBS:BreakoutBoard-cache
EELAYER 25 0
EELAYER END
$Descr User 8268 5846
encoding utf-8
Sheet 3 10
Title "Breakout Board"
Date "2018-04-05"
Rev "Release 0.2"
Comp "Enertechnos Ltd."
Comment1 "For Approval"
Comment2 ""
Comment3 "As such ANALOG INPUTS must receive voltage not higher than 3.3V."
Comment4 "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."
$EndDescr
$Comp
L RJ45 J201
U 1 1 5A2E9F01
P 2150 2050
AR Path="/5A2F1991/5A2E9F01" Ref="J201"  Part="1" 
AR Path="/5A2F08D5/5A2E9F01" Ref="J301"  Part="1" 
AR Path="/5A2F40AA/5A2E9F01" Ref="J401"  Part="1" 
AR Path="/5A2F0F54/5A2E9F01" Ref="J501"  Part="1" 
AR Path="/5A2F6574/5A2E9F01" Ref="J601"  Part="1" 
AR Path="/5A327B0A/5A2E9F01" Ref="J701"  Part="1" 
F 0 "J301" H 2350 2550 50  0000 C CNN
F 1 "RJ45" H 2000 2550 50  0000 C CNN
F 2 "OAE_Parts:RJ45-shielded-Molex" H 2150 2050 50  0001 C CNN
F 3 "" H 2150 2050 50  0001 C CNN
	1    2150 2050
	0    1    1    0   
$EndComp
$Comp
L RJ45 J202
U 1 1 5A2E9F0E
P 2150 3350
AR Path="/5A2F1991/5A2E9F0E" Ref="J202"  Part="1" 
AR Path="/5A2F08D5/5A2E9F0E" Ref="J302"  Part="1" 
AR Path="/5A2F40AA/5A2E9F0E" Ref="J402"  Part="1" 
AR Path="/5A2F0F54/5A2E9F0E" Ref="J502"  Part="1" 
AR Path="/5A2F6574/5A2E9F0E" Ref="J602"  Part="1" 
AR Path="/5A327B0A/5A2E9F0E" Ref="J702"  Part="1" 
F 0 "J302" H 2350 3850 50  0000 C CNN
F 1 "RJ45" H 2000 3850 50  0000 C CNN
F 2 "OAE_Parts:RJ45-shielded-Molex" H 2150 3350 50  0001 C CNN
F 3 "" H 2150 3350 50  0001 C CNN
	1    2150 3350
	0    1    1    0   
$EndComp
Wire Notes Line
	2800 1450 1000 1450
Text HLabel 1700 2200 0    60   Output ~ 0
ARD_TEMP
Text HLabel 1700 3700 0    60   Input ~ 0
ARD_PWM_A
Text HLabel 1700 3500 0    60   Input ~ 0
ARD_PWM_B
Text HLabel 1700 3100 0    60   Input ~ 0
ARD_PWM_C
Text HLabel 1700 3300 0    60   Input ~ 0
ARD_PWM_D
Text GLabel 1700 2000 0    60   Input ~ 0
DC_IN
Text GLabel 1700 2100 0    60   UnSpc ~ 0
DC_GND
Text GLabel 1700 2300 0    60   Input ~ 0
ARD_VCC
Text GLabel 1700 2400 0    60   UnSpc ~ 0
ARD_GND
Text HLabel 1700 1700 0    60   Output ~ 0
ARD_CUR
Text GLabel 1700 3000 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 1700 3200 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 1700 3400 0    60   UnSpc ~ 0
ARD_GND
Text GLabel 1700 3600 0    60   UnSpc ~ 0
ARD_GND
$Comp
L Earth #PWR?
U 1 1 5AC3BDA5
P 2500 3950
F 0 "#PWR?" H 2500 3700 50  0001 C CNN
F 1 "Earth" H 2500 3800 50  0001 C CNN
F 2 "" H 2500 3950 50  0001 C CNN
F 3 "" H 2500 3950 50  0001 C CNN
	1    2500 3950
	1    0    0    -1  
$EndComp
$Comp
L Earth #PWR?
U 1 1 5AC3BDC7
P 2500 2650
F 0 "#PWR?" H 2500 2400 50  0001 C CNN
F 1 "Earth" H 2500 2500 50  0001 C CNN
F 2 "" H 2500 2650 50  0001 C CNN
F 3 "" H 2500 2650 50  0001 C CNN
	1    2500 2650
	1    0    0    -1  
$EndComp
$EndSCHEMATC
