(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/BreakoutBoard/BreakoutBoard.sch)
    (date "10/04/2018 13:03:16")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source BreakoutBoard.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 2) (name /H-Bridge/) (tstamps /5A2F1991/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 3) (name "/Module A/") (tstamps /5A2F08D5/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 4) (name "/Module B/") (tstamps /5A2F40AA/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 5) (name "/Module C/") (tstamps /5A2F0F54/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 6) (name "/Module D/") (tstamps /5A2F6574/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 7) (name "/Module E/") (tstamps /5A327B0A/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Module.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 8) (name "/Fuse Board 1/") (tstamps /5A31FD72/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source FuseBoardConnection.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 9) (name "/Fuse Board 2/") (tstamps /5A332152/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source FuseBoardConnection.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe."))))
    (sheet (number 10) (name "/Fuse Board 3/") (tstamps /5A3324C4/)
      (title_block
        (title "Breakout Board")
        (company "Enertechnos Ltd.")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source FuseBoardConnection.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value "As such ANALOG INPUTS must receive voltage not higher than 3.3V."))
        (comment (number 4) (value "WARNING: ChipKit WiFire runs at 3.3V AND IS NOT 5V-safe.")))))
  (components
    (comp (ref P102)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EFF88))
    (comp (ref P101)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F28C2))
    (comp (ref P103)
      (value Analog)
      (footprint Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x06_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F5771))
    (comp (ref P105)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F76EC))
    (comp (ref P104)
      (value Digital)
      (footprint Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x08_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F7708))
    (comp (ref P106)
      (value Analog)
      (footprint Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm)
      (libsource (lib conn) (part Conn_02x06_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F771D))
    (comp (ref J102)
      (value "12V DC")
      (footprint Connectors:JACK_ALIM)
      (libsource (lib conn) (part Barrel_Jack))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3109C7))
    (comp (ref J103)
      (value ARD_CONTROL)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31287D))
    (comp (ref J104)
      (value ARD_MONITOR)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599F9F17))
    (comp (ref U101)
      (value NCV7805BTG)
      (footprint TO_SOT_Packages_THT:TO-220-3_Vertical)
      (fields
        (field (name "Output Voltage") 5V))
      (libsource (lib BreakoutBoard-cache) (part UA78M33))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A342FBC))
    (comp (ref U102)
      (value MC7809ACTG)
      (footprint TO_SOT_Packages_THT:TO-220-3_Vertical)
      (fields
        (field (name "Output Voltage") 9V))
      (libsource (lib BreakoutBoard-cache) (part UA78M33))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A395520))
    (comp (ref J101)
      (value Earth)
      (footprint Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC39F77))
    (comp (ref J201)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /H-Bridge/) (tstamps /5A2F1991/))
      (tstamp 5A2E9F01))
    (comp (ref J202)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /H-Bridge/) (tstamps /5A2F1991/))
      (tstamp 5A2E9F0E))
    (comp (ref J301)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module A/") (tstamps /5A2F08D5/))
      (tstamp 5A2E9F01))
    (comp (ref J302)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module A/") (tstamps /5A2F08D5/))
      (tstamp 5A2E9F0E))
    (comp (ref J401)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module B/") (tstamps /5A2F40AA/))
      (tstamp 5A2E9F01))
    (comp (ref J402)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module B/") (tstamps /5A2F40AA/))
      (tstamp 5A2E9F0E))
    (comp (ref J501)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module C/") (tstamps /5A2F0F54/))
      (tstamp 5A2E9F01))
    (comp (ref J502)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module C/") (tstamps /5A2F0F54/))
      (tstamp 5A2E9F0E))
    (comp (ref J601)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module D/") (tstamps /5A2F6574/))
      (tstamp 5A2E9F01))
    (comp (ref J602)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module D/") (tstamps /5A2F6574/))
      (tstamp 5A2E9F0E))
    (comp (ref J701)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module E/") (tstamps /5A327B0A/))
      (tstamp 5A2E9F01))
    (comp (ref J702)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Module E/") (tstamps /5A327B0A/))
      (tstamp 5A2E9F0E))
    (comp (ref J801)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Fuse Board 1/") (tstamps /5A31FD72/))
      (tstamp 5A31FF65))
    (comp (ref J901)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Fuse Board 2/") (tstamps /5A332152/))
      (tstamp 5A31FF65))
    (comp (ref J1001)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names "/Fuse Board 3/") (tstamps /5A3324C4/))
      (tstamp 5A31FF65)))
  (libparts
    (libpart (lib conn) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib conn) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib conn) (part Conn_02x08_Odd_Even)
      (description "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name Earth) (type passive))))
    (libpart (lib BreakoutBoard-cache) (part UA78M33)
      (aliases
        (alias uA7808)
        (alias uA7810)
        (alias uA7812)
        (alias uA7815)
        (alias uA7824))
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) UA78M33))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical BreakoutBoard-cache)
      (uri C:\Development\mlihardware\MLI\Modular\BreakoutBoard\BreakoutBoard-cache.lib)))
  (nets
    (net (code 1) (name ARD_PWM_1)
      (node (ref J302) (pin 8))
      (node (ref P101) (pin 12)))
    (net (code 2) (name ARD_TEMP_B)
      (node (ref P106) (pin 7))
      (node (ref J401) (pin 6)))
    (net (code 3) (name ARD_PWM_4)
      (node (ref P101) (pin 8))
      (node (ref J302) (pin 4)))
    (net (code 4) (name ARD_PWM_3)
      (node (ref P101) (pin 6))
      (node (ref J302) (pin 2)))
    (net (code 5) (name ARD_PWM_2)
      (node (ref J302) (pin 6))
      (node (ref P101) (pin 10)))
    (net (code 6) (name ARD_PWM_5)
      (node (ref J402) (pin 8))
      (node (ref P102) (pin 4)))
    (net (code 7) (name ARD_TEMP_A)
      (node (ref P106) (pin 9))
      (node (ref J301) (pin 6)))
    (net (code 8) (name ARD_PWM_16)
      (node (ref J602) (pin 4))
      (node (ref P102) (pin 16)))
    (net (code 9) (name ARD_PWM_15)
      (node (ref J602) (pin 2))
      (node (ref P102) (pin 14)))
    (net (code 10) (name ARD_PWM_14)
      (node (ref J602) (pin 6))
      (node (ref P102) (pin 15)))
    (net (code 11) (name ARD_TEMP_D)
      (node (ref J601) (pin 6))
      (node (ref P106) (pin 3)))
    (net (code 12) (name ARD_PWM_12)
      (node (ref J502) (pin 4))
      (node (ref P102) (pin 8)))
    (net (code 13) (name ARD_PWM_11)
      (node (ref J502) (pin 2))
      (node (ref P102) (pin 6)))
    (net (code 14) (name ARD_PWM_10)
      (node (ref J502) (pin 6))
      (node (ref P102) (pin 10)))
    (net (code 15) (name ARD_PWM_9)
      (node (ref P102) (pin 12))
      (node (ref J502) (pin 8)))
    (net (code 16) (name ARD_TEMP_C)
      (node (ref P106) (pin 5))
      (node (ref J501) (pin 6)))
    (net (code 17) (name ARD_PWM_8)
      (node (ref P101) (pin 16))
      (node (ref J402) (pin 4)))
    (net (code 18) (name ARD_PWM_7)
      (node (ref P101) (pin 14))
      (node (ref J402) (pin 2)))
    (net (code 19) (name ARD_PWM_6)
      (node (ref J402) (pin 6))
      (node (ref P102) (pin 2)))
    (net (code 32) (name ARD_TEMP_HB)
      (node (ref J201) (pin 6))
      (node (ref P106) (pin 11)))
    (net (code 33) (name ARD_VCC)
      (node (ref J901) (pin 3))
      (node (ref J201) (pin 7))
      (node (ref J1001) (pin 3))
      (node (ref J301) (pin 7))
      (node (ref J501) (pin 7))
      (node (ref J701) (pin 7))
      (node (ref J801) (pin 3))
      (node (ref U101) (pin 3))
      (node (ref J401) (pin 7))
      (node (ref J601) (pin 7)))
    (net (code 34) (name Earth)
      (node (ref J302) (pin 9))
      (node (ref J301) (pin 9))
      (node (ref J1001) (pin 9))
      (node (ref J502) (pin 9))
      (node (ref J401) (pin 9))
      (node (ref J501) (pin 9))
      (node (ref J202) (pin 9))
      (node (ref J201) (pin 9))
      (node (ref J602) (pin 9))
      (node (ref J101) (pin 1))
      (node (ref J901) (pin 9))
      (node (ref J701) (pin 9))
      (node (ref J601) (pin 9))
      (node (ref J702) (pin 9))
      (node (ref J801) (pin 9))
      (node (ref J402) (pin 9)))
    (net (code 35) (name DC_IN)
      (node (ref J601) (pin 4))
      (node (ref U102) (pin 1))
      (node (ref J201) (pin 4))
      (node (ref J102) (pin 1))
      (node (ref J501) (pin 4))
      (node (ref J701) (pin 4))
      (node (ref U101) (pin 1))
      (node (ref J301) (pin 4))
      (node (ref J401) (pin 4)))
    (net (code 36) (name FB1B)
      (node (ref J801) (pin 4))
      (node (ref P105) (pin 14)))
    (net (code 37) (name FB1A)
      (node (ref J801) (pin 2))
      (node (ref P105) (pin 12)))
    (net (code 38) (name FB1C)
      (node (ref P105) (pin 16))
      (node (ref J801) (pin 6)))
    (net (code 39) (name ARD_VIN)
      (node (ref J104) (pin 1))
      (node (ref U102) (pin 3))
      (node (ref J103) (pin 1)))
    (net (code 40) (name "Net-(J102-Pad3)")
      (node (ref J102) (pin 3)))
    (net (code 41) (name ARD_GND)
      (node (ref J402) (pin 5))
      (node (ref J702) (pin 1))
      (node (ref J402) (pin 1))
      (node (ref J701) (pin 8))
      (node (ref J701) (pin 5))
      (node (ref J402) (pin 3))
      (node (ref J401) (pin 8))
      (node (ref J402) (pin 7))
      (node (ref J1001) (pin 1))
      (node (ref J702) (pin 7))
      (node (ref J901) (pin 1))
      (node (ref J302) (pin 7))
      (node (ref J302) (pin 5))
      (node (ref J302) (pin 3))
      (node (ref J302) (pin 1))
      (node (ref J401) (pin 5))
      (node (ref J301) (pin 8))
      (node (ref J301) (pin 5))
      (node (ref J702) (pin 5))
      (node (ref J702) (pin 3))
      (node (ref J501) (pin 5))
      (node (ref J501) (pin 8))
      (node (ref J502) (pin 1))
      (node (ref J502) (pin 3))
      (node (ref J602) (pin 3))
      (node (ref J502) (pin 5))
      (node (ref J801) (pin 1))
      (node (ref J502) (pin 7))
      (node (ref J602) (pin 5))
      (node (ref J602) (pin 1))
      (node (ref J602) (pin 7))
      (node (ref J202) (pin 7))
      (node (ref J202) (pin 5))
      (node (ref J202) (pin 3))
      (node (ref J601) (pin 8))
      (node (ref J202) (pin 1))
      (node (ref J201) (pin 8))
      (node (ref J601) (pin 5))
      (node (ref J201) (pin 5))
      (node (ref J103) (pin 2))
      (node (ref U102) (pin 2))
      (node (ref J104) (pin 2))
      (node (ref J102) (pin 2))
      (node (ref U101) (pin 2)))
    (net (code 43) (name ARD_VOLTS_3)
      (node (ref J1001) (pin 8))
      (node (ref P106) (pin 12)))
    (net (code 44) (name FB3C)
      (node (ref J1001) (pin 6))
      (node (ref P105) (pin 11)))
    (net (code 45) (name FB3B)
      (node (ref P105) (pin 13))
      (node (ref J1001) (pin 4)))
    (net (code 46) (name FB3A)
      (node (ref P105) (pin 15))
      (node (ref J1001) (pin 2)))
    (net (code 47) (name ARD_VOLTS_2)
      (node (ref P106) (pin 8))
      (node (ref J901) (pin 8)))
    (net (code 48) (name FB2C)
      (node (ref J901) (pin 6))
      (node (ref P105) (pin 10)))
    (net (code 49) (name FB2B)
      (node (ref P105) (pin 8))
      (node (ref J901) (pin 4)))
    (net (code 50) (name FB2A)
      (node (ref P105) (pin 6))
      (node (ref J901) (pin 2)))
    (net (code 51) (name ARD_VOLTS_1)
      (node (ref J801) (pin 8))
      (node (ref P106) (pin 10)))
    (net (code 52) (name ARD_PWM_18)
      (node (ref P101) (pin 11))
      (node (ref J702) (pin 6)))
    (net (code 58) (name ARD_PWM_19)
      (node (ref P101) (pin 15))
      (node (ref J702) (pin 2)))
    (net (code 59) (name ARD_PWM_20)
      (node (ref P101) (pin 13))
      (node (ref J702) (pin 4)))
    (net (code 61) (name ARD_PWM_17)
      (node (ref P101) (pin 9))
      (node (ref J702) (pin 8)))
    (net (code 62) (name "Net-(P101-Pad7)")
      (node (ref P101) (pin 7)))
    (net (code 63) (name "Net-(P101-Pad5)")
      (node (ref P101) (pin 5)))
    (net (code 64) (name ARD_HBRIDGE_A)
      (node (ref P101) (pin 4))
      (node (ref J202) (pin 8))
      (node (ref J202) (pin 4)))
    (net (code 65) (name "Net-(P101-Pad3)")
      (node (ref P101) (pin 3)))
    (net (code 66) (name ARD_HBRIDGE_B)
      (node (ref P101) (pin 2))
      (node (ref J202) (pin 2))
      (node (ref J202) (pin 6)))
    (net (code 67) (name "Net-(P103-Pad1)")
      (node (ref P103) (pin 1)))
    (net (code 68) (name "Net-(P103-Pad11)")
      (node (ref P103) (pin 11)))
    (net (code 69) (name "Net-(P103-Pad10)")
      (node (ref P103) (pin 10)))
    (net (code 70) (name "Net-(P103-Pad9)")
      (node (ref P103) (pin 9)))
    (net (code 71) (name "Net-(P103-Pad8)")
      (node (ref P103) (pin 8)))
    (net (code 72) (name "Net-(P103-Pad7)")
      (node (ref P103) (pin 7)))
    (net (code 73) (name "Net-(P103-Pad6)")
      (node (ref P103) (pin 6)))
    (net (code 74) (name "Net-(P103-Pad5)")
      (node (ref P103) (pin 5)))
    (net (code 75) (name "Net-(P103-Pad4)")
      (node (ref P103) (pin 4)))
    (net (code 76) (name "Net-(P103-Pad3)")
      (node (ref P103) (pin 3)))
    (net (code 77) (name "Net-(P103-Pad2)")
      (node (ref P103) (pin 2)))
    (net (code 78) (name "Net-(P101-Pad1)")
      (node (ref P101) (pin 1)))
    (net (code 88) (name ARD_PWM_13)
      (node (ref P102) (pin 13))
      (node (ref J602) (pin 8)))
    (net (code 89) (name "Net-(P102-Pad11)")
      (node (ref P102) (pin 11)))
    (net (code 90) (name "Net-(P102-Pad9)")
      (node (ref P102) (pin 9)))
    (net (code 91) (name "Net-(P102-Pad7)")
      (node (ref P102) (pin 7)))
    (net (code 92) (name "Net-(P102-Pad5)")
      (node (ref P102) (pin 5)))
    (net (code 93) (name "Net-(P102-Pad3)")
      (node (ref P102) (pin 3)))
    (net (code 94) (name "Net-(P102-Pad1)")
      (node (ref P102) (pin 1)))
    (net (code 111) (name "Net-(P104-Pad6)")
      (node (ref P104) (pin 6)))
    (net (code 112) (name "Net-(P104-Pad16)")
      (node (ref P104) (pin 16)))
    (net (code 113) (name "Net-(P104-Pad15)")
      (node (ref P104) (pin 15)))
    (net (code 114) (name "Net-(P104-Pad14)")
      (node (ref P104) (pin 14)))
    (net (code 115) (name "Net-(P104-Pad13)")
      (node (ref P104) (pin 13)))
    (net (code 116) (name "Net-(P104-Pad12)")
      (node (ref P104) (pin 12)))
    (net (code 117) (name "Net-(P104-Pad11)")
      (node (ref P104) (pin 11)))
    (net (code 118) (name "Net-(P104-Pad10)")
      (node (ref P104) (pin 10)))
    (net (code 119) (name "Net-(P104-Pad9)")
      (node (ref P104) (pin 9)))
    (net (code 120) (name "Net-(P104-Pad8)")
      (node (ref P104) (pin 8)))
    (net (code 121) (name "Net-(P104-Pad7)")
      (node (ref P104) (pin 7)))
    (net (code 122) (name "Net-(P104-Pad5)")
      (node (ref P104) (pin 5)))
    (net (code 123) (name "Net-(P104-Pad4)")
      (node (ref P104) (pin 4)))
    (net (code 124) (name "Net-(P104-Pad3)")
      (node (ref P104) (pin 3)))
    (net (code 125) (name "Net-(P104-Pad2)")
      (node (ref P104) (pin 2)))
    (net (code 126) (name "Net-(P104-Pad1)")
      (node (ref P104) (pin 1)))
    (net (code 127) (name "Net-(P106-Pad6)")
      (node (ref P106) (pin 6)))
    (net (code 128) (name "Net-(P106-Pad4)")
      (node (ref P106) (pin 4)))
    (net (code 129) (name ARD_CUR_HB)
      (node (ref P106) (pin 2))
      (node (ref J201) (pin 1)))
    (net (code 130) (name ARD_TEMP_E)
      (node (ref P106) (pin 1))
      (node (ref J701) (pin 6)))
    (net (code 131) (name "Net-(P105-Pad7)")
      (node (ref P105) (pin 7)))
    (net (code 132) (name "Net-(P105-Pad5)")
      (node (ref P105) (pin 5)))
    (net (code 133) (name "Net-(P105-Pad4)")
      (node (ref P105) (pin 4)))
    (net (code 134) (name "Net-(P105-Pad3)")
      (node (ref P105) (pin 3)))
    (net (code 135) (name "Net-(P105-Pad2)")
      (node (ref P105) (pin 2)))
    (net (code 136) (name "Net-(P105-Pad1)")
      (node (ref P105) (pin 1)))
    (net (code 137) (name "Net-(P103-Pad12)")
      (node (ref P103) (pin 12)))
    (net (code 138) (name "Net-(P105-Pad9)")
      (node (ref P105) (pin 9)))
    (net (code 139) (name "Net-(J301-Pad3)")
      (node (ref J301) (pin 3)))
    (net (code 140) (name "Net-(J301-Pad2)")
      (node (ref J301) (pin 2)))
    (net (code 141) (name "/Module A/ARD_CUR")
      (node (ref J301) (pin 1)))
    (net (code 142) (name "/Module C/ARD_CUR")
      (node (ref J501) (pin 1)))
    (net (code 143) (name "Net-(J501-Pad2)")
      (node (ref J501) (pin 2)))
    (net (code 144) (name "Net-(J501-Pad3)")
      (node (ref J501) (pin 3)))
    (net (code 145) (name "Net-(J201-Pad2)")
      (node (ref J201) (pin 2)))
    (net (code 146) (name "Net-(J201-Pad3)")
      (node (ref J201) (pin 3)))
    (net (code 147) (name "Net-(J401-Pad3)")
      (node (ref J401) (pin 3)))
    (net (code 148) (name "Net-(J401-Pad2)")
      (node (ref J401) (pin 2)))
    (net (code 149) (name "/Module B/ARD_CUR")
      (node (ref J401) (pin 1)))
    (net (code 150) (name "/Module D/ARD_CUR")
      (node (ref J601) (pin 1)))
    (net (code 151) (name "Net-(J601-Pad2)")
      (node (ref J601) (pin 2)))
    (net (code 152) (name "Net-(J601-Pad3)")
      (node (ref J601) (pin 3)))
    (net (code 153) (name "Net-(J801-Pad7)")
      (node (ref J801) (pin 7)))
    (net (code 154) (name "Net-(J801-Pad5)")
      (node (ref J801) (pin 5)))
    (net (code 155) (name "/Module E/ARD_CUR")
      (node (ref J701) (pin 1)))
    (net (code 156) (name "Net-(J701-Pad2)")
      (node (ref J701) (pin 2)))
    (net (code 157) (name "Net-(J701-Pad3)")
      (node (ref J701) (pin 3)))
    (net (code 158) (name "Net-(J901-Pad7)")
      (node (ref J901) (pin 7)))
    (net (code 159) (name "Net-(J901-Pad5)")
      (node (ref J901) (pin 5)))
    (net (code 160) (name "Net-(J1001-Pad7)")
      (node (ref J1001) (pin 7)))
    (net (code 161) (name "Net-(J1001-Pad5)")
      (node (ref J1001) (pin 5)))))