(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MosfetSwitch/MosfetSwitch.sch)
    (date "30/05/2017 23:33:02")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source MosfetSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R2)
      (value 4K7)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACAE5))
    (comp (ref C1)
      (value 22uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACB50))
    (comp (ref C2)
      (value 220nF)
      (footprint Capacitors_THT:C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACBF5))
    (comp (ref R3)
      (value 4K7)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACDEB))
    (comp (ref R4)
      (value 470)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACE76))
    (comp (ref U3)
      (value "W30508TRC (ICL7667)")
      (footprint SamacSys_Parts:DIPS762W50P254L1008H460Q8N)
      (datasheet "http://www.winslowadaptics.com/gfx/productgroups/Production Screw Machine Sockets - DIL/W30508TRC/W30500 generic.pdf")
      (fields
        (field (name Description) "Winslow 2.54mm Pitch Vertical 8 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
        (field (name Manufacturer_Name) Winslow)
        (field (name Manufacturer_Part_Number) W30508TRC)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0813115)
        (field (name Height) 4.6))
      (libsource (lib SamacSys_Parts) (part W30508TRC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AD9EF))
    (comp (ref R1)
      (value 200)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF392))
    (comp (ref U1)
      (value "W30508TRC (NME1212DC)")
      (footprint SamacSys_Parts:DIPS762W50P254L1008H460Q8N)
      (datasheet "http://www.winslowadaptics.com/gfx/productgroups/Production Screw Machine Sockets - DIL/W30508TRC/W30500 generic.pdf")
      (fields
        (field (name Description) "Winslow 2.54mm Pitch Vertical 8 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
        (field (name Manufacturer_Name) Winslow)
        (field (name Manufacturer_Part_Number) W30508TRC)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0813115)
        (field (name Height) 4.6))
      (libsource (lib SamacSys_Parts) (part W30508TRC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C6117))
    (comp (ref J1)
      (value CONN_01X04)
      (footprint Connectors_Molex:Molex_PicoBlade_53047-0410_04x1.25mm_Straight)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C94BD))
    (comp (ref J2)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C95DB))
    (comp (ref J3)
      (value DrainLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA485))
    (comp (ref J4)
      (value SourceLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA834))
    (comp (ref U2)
      (value "W30506TRC (4N35)")
      (footprint SamacSys_Parts:DIPS762W60P254L760H300Q6N)
      (datasheet http://docs-europe.electrocomponents.com/webdocs/002b/0900766b8002bd2d.pdf)
      (fields
        (field (name Description) "Winslow 2.54mm Pitch Vertical 6 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
        (field (name Manufacturer_Name) Winslow)
        (field (name Manufacturer_Part_Number) W30506TRC)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0813109)
        (field (name Height) 3))
      (libsource (lib SamacSys_Parts) (part W30506TRC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DA8DF))
    (comp (ref D1)
      (value D_Schottky_x2_KCom_AKA)
      (footprint TO_SOT_Packages_THT:TO-220_Horizontal_Reversed)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DCE5E))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-220_Horizontal_Reversed)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib SamacSys_Parts) (part RFP12N10L))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF9D4)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib SamacSys_Parts) (part RFP12N10L)
      (description "N-channel logicFET,RFP12N10L 12A 100V")
      (docs https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib SamacSys_Parts) (part W30506TRC)
      (fields
        (field (name Reference) J)
        (field (name Value) W30506TRC)
        (field (name Footprint) DIPS762W60P254L760H300Q6N)
        (field (name Datasheet) http://docs-europe.electrocomponents.com/webdocs/002b/0900766b8002bd2d.pdf)
        (field (name Description) "Winslow 2.54mm Pitch Vertical 6 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
        (field (name Manufacturer_Name) Winslow)
        (field (name Manufacturer_Part_Number) W30506TRC)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0813109)
        (field (name Height) 3))
      (pins
        (pin (num 1) (name 1) (type unspc))
        (pin (num 2) (name 2) (type unspc))
        (pin (num 3) (name 3) (type unspc))
        (pin (num 4) (name 4) (type unspc))
        (pin (num 5) (name 5) (type unspc))
        (pin (num 6) (name 6) (type unspc))))
    (libpart (lib SamacSys_Parts) (part W30508TRC)
      (description "Winslow 2.54mm Pitch Vertical 8 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
      (docs "http://www.winslowadaptics.com/gfx/productgroups/Production Screw Machine Sockets - DIL/W30508TRC/W30500 generic.pdf")
      (fields
        (field (name Reference) U)
        (field (name Value) W30508TRC)
        (field (name Footprint) DIPS762W50P254L1008H460Q8N)
        (field (name Datasheet) "http://www.winslowadaptics.com/gfx/productgroups/Production Screw Machine Sockets - DIL/W30508TRC/W30500 generic.pdf")
        (field (name Description) "Winslow 2.54mm Pitch Vertical 8 Way, Through Hole Turned pin Open Frame IC Dip Socket, 5A")
        (field (name Manufacturer_Name) Winslow)
        (field (name Manufacturer_Part_Number) W30508TRC)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0813115)
        (field (name Height) 4.6))
      (pins
        (pin (num 1) (name 1) (type unspc))
        (pin (num 2) (name 2) (type unspc))
        (pin (num 3) (name 3) (type unspc))
        (pin (num 4) (name 4) (type unspc))
        (pin (num 5) (name 5) (type unspc))
        (pin (num 6) (name 6) (type unspc))
        (pin (num 7) (name 7) (type unspc))
        (pin (num 8) (name 8) (type unspc)))))
  (libraries
    (library (logical SamacSys_Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\SamacSys_Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name "Net-(R3-Pad1)")
      (node (ref R4) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref U3) (pin 7)))
    (net (code 2) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 5))
      (node (ref R2) (pin 2))
      (node (ref U3) (pin 2)))
    (net (code 3) (name "Net-(R1-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 4) (name ARD_GND)
      (node (ref J1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 5) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 6) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 7) (name "Net-(Q1-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 8) (name "Net-(D1-Pad2)")
      (node (ref J4) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 9) (name GND_ISO)
      (node (ref U3) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref Q1) (pin 3))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 10) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))
    (net (code 11) (name DC_IN)
      (node (ref U1) (pin 4))
      (node (ref J2) (pin 1)))
    (net (code 12) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 13) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 14) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 15) (name "Net-(U3-Pad8)")
      (node (ref U3) (pin 8)))
    (net (code 16) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 17) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 18) (name DC_ISO)
      (node (ref U1) (pin 5))
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 6))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 19) (name DC_GND)
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 20) (name ARD_TEMP)
      (node (ref J1) (pin 4)))
    (net (code 21) (name ARD_PWR_LVL)
      (node (ref J1) (pin 3)))
    (net (code 22) (name ARD_PWM)
      (node (ref U2) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 23) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 24) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 25) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 26) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))))