(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MosfetSwitch.r3/MosfetSwitch.r2.sch)
    (date "21/06/2017 10:15:32")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 2")
        (date 2017-06-13)
        (source MosfetSwitch.r2.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "For approval by Mansour")))))
  (components
    (comp (ref C2)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACB50))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACBF5))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF392))
    (comp (ref J2)
      (value CONN_01X05)
      (footprint Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C94BD))
    (comp (ref J3)
      (value CONN_01X02)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C95DB))
    (comp (ref J4)
      (value DrainLarge)
      (footprint PartsLibraries:PowerConnector)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA485))
    (comp (ref J5)
      (value SourceLarge)
      (footprint PartsLibraries:PowerConnector)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA834))
    (comp (ref D1)
      (value D_Schottky_x2_KCom_AKA)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DCE5E))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib MosfetSwitch.r2-cache) (part RFP12N10L))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF9D4))
    (comp (ref U2)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib opto) (part 4N26))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E7A66))
    (comp (ref IC1)
      (value TC4422AVPA)
      (footprint Housings_DIP:DIP-8_W7.62mm)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib MosfetSwitch.r2-cache) (part TC4422AVPA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E820A))
    (comp (ref U1)
      (value NME1212DC)
      (footprint Housings_DIP:DIP-8_W7.62mm)
      (libsource (lib MosfetSwitch.r2-cache) (part NME1212DC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EC206))
    (comp (ref R3)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED01B))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED18A))
    (comp (ref J1)
      (value CONN_01X02)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 593FD4A9))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593FD687))
    (comp (ref C5)
      (value C)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59400A26))
    (comp (ref C6)
      (value C)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59400AF8)))
  (libparts
    (libpart (lib opto) (part 4N25)
      (aliases
        (alias 4N26)
        (alias TIL111))
      (description "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 2500V, DIP6")
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 4N25)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (description "Connector, single row, 01x05, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib MosfetSwitch.r2-cache) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MosfetSwitch.r2-cache) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib MosfetSwitch.r2-cache) (part TC4422AVPA)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type unspc))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical opto)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\opto.lib"))
    (library (logical MosfetSwitch.r2-cache)
      (uri C:\Development\multilevelinverter\Hardware\MosfetSwitch.r3\MosfetSwitch.r2-cache.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name "Net-(IC1-Pad3)")
      (node (ref R3) (pin 2))
      (node (ref IC1) (pin 3))
      (node (ref U2) (pin 5)))
    (net (code 2) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 3) (name GND_ISO)
      (node (ref IC1) (pin 5))
      (node (ref C6) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref IC1) (pin 4))
      (node (ref C4) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U1) (pin 5))
      (node (ref Q1) (pin 3)))
    (net (code 4) (name "Net-(C4-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref IC1) (pin 6))
      (node (ref C5) (pin 2))
      (node (ref IC1) (pin 7)))
    (net (code 5) (name "Net-(C6-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref C6) (pin 2)))
    (net (code 6) (name ARD_GND)
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 7) (name ARD_TEMP)
      (node (ref J1) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref J2) (pin 4)))
    (net (code 8) (name DC_IN)
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 9) (name ARD_5V)
      (node (ref J2) (pin 5))
      (node (ref J1) (pin 1)))
    (net (code 10) (name ARD_SRC_V)
      (node (ref J2) (pin 3)))
    (net (code 11) (name ARD_PWM)
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 12) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 13) (name DC_GND)
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 14) (name DC_ISO)
      (node (ref R3) (pin 1))
      (node (ref IC1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref IC1) (pin 8))
      (node (ref U1) (pin 7))
      (node (ref C3) (pin 1)))
    (net (code 15) (name "Net-(IC1-Pad2)")
      (node (ref IC1) (pin 2)))
    (net (code 16) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 17) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 18) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 19) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))))