(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/Modular/PsuPowerModule/PsuPowerModule.sch)
    (date "06/09/2017 08:39:34")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 2")
        (date 2017-06-13)
        (source PsuPowerModule.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "For approval by Mansour"))))
    (sheet (number 2) (name "/SinglePowerSwitch 1/") (tstamps /59AEDD49/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AED755))
    (comp (ref J6)
      (value PWR_OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AEFF90))
    (comp (ref J7)
      (value PWR_OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AFA697))
    (comp (ref D1)
      (value PWR_DIODE)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE007))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE014))
    (comp (ref C1)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE01D))
    (comp (ref J2)
      (value PWR_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE02F))
    (comp (ref D2)
      (value PWR_DIODE)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE007))
    (comp (ref Q2)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE014))
    (comp (ref C2)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE01D))
    (comp (ref J3)
      (value PWR_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE02F))
    (comp (ref D3)
      (value PWR_DIODE)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE007))
    (comp (ref Q3)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE014))
    (comp (ref C3)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE01D))
    (comp (ref J4)
      (value PWR_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE02F))
    (comp (ref D4)
      (value PWR_DIODE)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE007))
    (comp (ref Q4)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE014))
    (comp (ref C4)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE01D))
    (comp (ref J5)
      (value PWR_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE02F)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib OAE.Parts) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name DRV_GATE_3)
      (node (ref J1) (pin 2))
      (node (ref Q3) (pin 1)))
    (net (code 2) (name GND_ISO_3)
      (node (ref J1) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref Q3) (pin 3)))
    (net (code 3) (name DRV_GATE_4)
      (node (ref J1) (pin 6))
      (node (ref Q4) (pin 1)))
    (net (code 4) (name GND_ISO_4)
      (node (ref Q4) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref J1) (pin 8)))
    (net (code 5) (name "/SinglePowerSwitch 1/PWR_OUT")
      (node (ref D1) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref J7) (pin 1)))
    (net (code 6) (name GND_ISO_1)
      (node (ref J1) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 7) (name DRV_GATE_1)
      (node (ref J1) (pin 3))
      (node (ref Q1) (pin 1)))
    (net (code 8) (name DRV_GATE_2)
      (node (ref Q2) (pin 1))
      (node (ref J1) (pin 7)))
    (net (code 9) (name GND_ISO_2)
      (node (ref J1) (pin 5))
      (node (ref D2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 10) (name "Net-(C1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 11) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))
    (net (code 12) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 13) (name "Net-(C2-Pad2)")
      (node (ref J3) (pin 1))
      (node (ref Q2) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 14) (name "Net-(Q2-Pad4)")
      (node (ref Q2) (pin 4)))
    (net (code 15) (name "Net-(D2-Pad3)")
      (node (ref D2) (pin 3)))
    (net (code 16) (name "Net-(C3-Pad2)")
      (node (ref J4) (pin 1))
      (node (ref Q3) (pin 2))
      (node (ref C3) (pin 2)))
    (net (code 17) (name "Net-(D3-Pad3)")
      (node (ref D3) (pin 3)))
    (net (code 18) (name "Net-(Q3-Pad4)")
      (node (ref Q3) (pin 4)))
    (net (code 19) (name "Net-(C4-Pad2)")
      (node (ref J5) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref Q4) (pin 2)))
    (net (code 20) (name "Net-(Q4-Pad4)")
      (node (ref Q4) (pin 4)))
    (net (code 21) (name "Net-(D4-Pad3)")
      (node (ref D4) (pin 3)))))