(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/PsuSwitchModule/PsuSwitchModule.sch)
    (date "25/10/2017 10:07:27")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "HBridge (Single Board)")
        (company Enertechnos)
        (rev Rev2)
        (date 2017-08-30)
        (source PsuSwitchModule.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /PsuSwitchModule.Switch.3/) (tstamps /59A71299/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59526541))
    (comp (ref J2)
      (value "Temperature Probe")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF2))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF9))
    (comp (ref J7)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7EBD8))
    (comp (ref IC1)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498139))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498146))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5949814D))
    (comp (ref J3)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 595237FD))
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3D9))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3E0))
    (comp (ref U1)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3EA))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DA9F))
    (comp (ref U2)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAA6))
    (comp (ref R3)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAAD))
    (comp (ref D1)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0E59))
    (comp (ref C17)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0ED7))
    (comp (ref R10)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0FC7))
    (comp (ref R11)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1A58))
    (comp (ref C18)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1DD4))
    (comp (ref IC2)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498139))
    (comp (ref C8)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498146))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5949814D))
    (comp (ref J4)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 595237FD))
    (comp (ref C5)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3D9))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3E0))
    (comp (ref U3)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3EA))
    (comp (ref R4)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DA9F))
    (comp (ref U4)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAA6))
    (comp (ref R5)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAAD))
    (comp (ref D2)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0E59))
    (comp (ref C19)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0ED7))
    (comp (ref R12)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0FC7))
    (comp (ref R13)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1A58))
    (comp (ref C20)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1DD4))
    (comp (ref IC3)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498139))
    (comp (ref C12)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498146))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5949814D))
    (comp (ref J5)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 595237FD))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3D9))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3E0))
    (comp (ref U5)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3EA))
    (comp (ref R6)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DA9F))
    (comp (ref U6)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAA6))
    (comp (ref R7)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAAD))
    (comp (ref D3)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0E59))
    (comp (ref C21)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0ED7))
    (comp (ref R14)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0FC7))
    (comp (ref R15)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1A58))
    (comp (ref C22)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1DD4))
    (comp (ref IC4)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498139))
    (comp (ref C16)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498146))
    (comp (ref C15)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5949814D))
    (comp (ref J6)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 595237FD))
    (comp (ref C13)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3D9))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3E0))
    (comp (ref U7)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3EA))
    (comp (ref R8)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DA9F))
    (comp (ref U8)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAA6))
    (comp (ref R9)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAAD))
    (comp (ref D4)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0E59))
    (comp (ref C23)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0ED7))
    (comp (ref R16)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0FC7))
    (comp (ref R17)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1A58))
    (comp (ref C24)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1DD4)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib device) (part D_Zener)
      (description "Zener Diode")
      (docs https://en.wikipedia.org/wiki/Zener_diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib OAE.Parts) (part H11N1M)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) H11N1M)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part TC4422AVPA)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name DC_GND)
      (node (ref U7) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 2) (name ARD_5V)
      (node (ref J7) (pin 7)))
    (net (code 3) (name ARD_GND)
      (node (ref U6) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref J7) (pin 8))
      (node (ref U4) (pin 2)))
    (net (code 4) (name DC_IN)
      (node (ref U3) (pin 4))
      (node (ref U5) (pin 4))
      (node (ref U7) (pin 4))
      (node (ref U1) (pin 4))
      (node (ref J7) (pin 1)))
    (net (code 5) (name ARD_PWM_D)
      (node (ref J7) (pin 6))
      (node (ref R8) (pin 1)))
    (net (code 6) (name ARD_PWM_B)
      (node (ref R4) (pin 1))
      (node (ref J7) (pin 4)))
    (net (code 7) (name ARD_PWM_A)
      (node (ref R2) (pin 1))
      (node (ref J7) (pin 3)))
    (net (code 8) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 9) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1)))
    (net (code 10) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 11) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 12) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 13) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 14) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 15) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 16) (name ARD_PWM_C)
      (node (ref R6) (pin 1))
      (node (ref J7) (pin 5)))
    (net (code 17) (name ARD_TEMP)
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 8)))
    (net (code 18) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2)))
    (net (code 19) (name "Net-(R3-Pad1)")
      (node (ref U1) (pin 7))
      (node (ref R3) (pin 1)))
    (net (code 20) (name Earth)
      (node (ref IC2) (pin 5))
      (node (ref IC2) (pin 4))
      (node (ref C16) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref IC4) (pin 4))
      (node (ref C11) (pin 1))
      (node (ref IC4) (pin 5))
      (node (ref C8) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref IC3) (pin 4))
      (node (ref C9) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref U6) (pin 5))
      (node (ref C22) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref C12) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref IC3) (pin 5))
      (node (ref C10) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref IC1) (pin 4))
      (node (ref IC1) (pin 5))
      (node (ref C20) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U8) (pin 5))
      (node (ref R11) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C19) (pin 2)))
    (net (code 21) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref IC1) (pin 7))
      (node (ref IC1) (pin 6)))
    (net (code 22) (name "Net-(IC1-Pad2)")
      (node (ref U2) (pin 4))
      (node (ref R10) (pin 2))
      (node (ref IC1) (pin 2)))
    (net (code 23) (name "Net-(C17-Pad1)")
      (node (ref C17) (pin 1))
      (node (ref IC1) (pin 8))
      (node (ref D1) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref IC1) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref R3) (pin 2)))
    (net (code 24) (name "Net-(IC1-Pad3)")
      (node (ref IC1) (pin 3)))
    (net (code 25) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref C18) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 26) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 27) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 28) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U3) (pin 7)))
    (net (code 29) (name "Net-(C7-Pad2)")
      (node (ref R13) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref IC2) (pin 7))
      (node (ref IC2) (pin 6)))
    (net (code 30) (name "Net-(IC2-Pad2)")
      (node (ref IC2) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref U4) (pin 4)))
    (net (code 31) (name "Net-(C19-Pad1)")
      (node (ref IC2) (pin 8))
      (node (ref R12) (pin 1))
      (node (ref IC2) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref U4) (pin 6))
      (node (ref C19) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 32) (name "Net-(IC2-Pad3)")
      (node (ref IC2) (pin 3)))
    (net (code 33) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 34) (name "Net-(R4-Pad2)")
      (node (ref U4) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 35) (name "Net-(C20-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref C20) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U3) (pin 5)))
    (net (code 36) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U5) (pin 7)))
    (net (code 37) (name "Net-(C11-Pad2)")
      (node (ref C11) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref IC3) (pin 7))
      (node (ref R15) (pin 1))
      (node (ref IC3) (pin 6)))
    (net (code 38) (name "Net-(IC3-Pad2)")
      (node (ref IC3) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref U6) (pin 4)))
    (net (code 39) (name "Net-(C21-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref IC3) (pin 8))
      (node (ref IC3) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 40) (name "Net-(IC3-Pad3)")
      (node (ref IC3) (pin 3)))
    (net (code 41) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 42) (name "Net-(R6-Pad2)")
      (node (ref U6) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 43) (name "Net-(C10-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref U5) (pin 5)))
    (net (code 44) (name "Net-(R9-Pad1)")
      (node (ref U7) (pin 7))
      (node (ref R9) (pin 1)))
    (net (code 45) (name "Net-(C15-Pad2)")
      (node (ref IC4) (pin 7))
      (node (ref C15) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref IC4) (pin 6))
      (node (ref J6) (pin 1))
      (node (ref R17) (pin 1)))
    (net (code 46) (name "Net-(IC4-Pad2)")
      (node (ref IC4) (pin 2))
      (node (ref U8) (pin 4))
      (node (ref R16) (pin 2)))
    (net (code 47) (name "Net-(C23-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref U8) (pin 6))
      (node (ref D4) (pin 1))
      (node (ref IC4) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref IC4) (pin 8)))
    (net (code 48) (name "Net-(IC4-Pad3)")
      (node (ref IC4) (pin 3)))
    (net (code 49) (name "Net-(R8-Pad2)")
      (node (ref R8) (pin 2))
      (node (ref U8) (pin 1)))
    (net (code 50) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 51) (name "Net-(C13-Pad1)")
      (node (ref U7) (pin 5))
      (node (ref C14) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C24) (pin 1)))))