(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MosfetSwitch.r1/MosfetSwitch.r1.sch)
    (date "05/06/2017 13:14:18")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 1")
        (date 2017-05-31)
        (source MosfetSwitch.r1.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C2)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACB50))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACBF5))
    (comp (ref R2)
      (value 200)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF392))
    (comp (ref J2)
      (value ARD_CONN)
      (footprint Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C94BD))
    (comp (ref J3)
      (value DC_CONN)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C95DB))
    (comp (ref J4)
      (value DrainLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA485))
    (comp (ref J5)
      (value SourceLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA834))
    (comp (ref D1)
      (value D_Schottky_x2_KCom_AKA)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Horizontal_Reversed)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DCE5E))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Horizontal_Reversed)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib SamacSys_Parts) (part RFP12N10L))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF9D4))
    (comp (ref U2)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib opto) (part 4N26))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E7A66))
    (comp (ref U3)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib SamacSys_Parts) (part TC4422AVPA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E820A))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EA608))
    (comp (ref U1)
      (value NME1212DC)
      (footprint RS:DIPS762W50P254L1008H460Q8N)
      (libsource (lib nme1212dc) (part NME1212DC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EC206))
    (comp (ref R3)
      (value 4K7)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED01B))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED18A))
    (comp (ref J1)
      (value TEMP_PROBE)
      (footprint Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 59355101))
    (comp (ref R1)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5935695A)))
  (libparts
    (libpart (lib opto) (part 4N25)
      (aliases
        (alias 4N26)
        (alias TIL111))
      (description "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 2500V, DIP6")
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 4N25)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib nme1212dc) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib SamacSys_Parts) (part RFP12N10L)
      (description "N-channel logicFET,RFP12N10L 12A 100V")
      (docs https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib SamacSys_Parts) (part TC4422AVPA)
      (description "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type unspc))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical SamacSys_Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\SamacSys_Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical opto)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\opto.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical nme1212dc)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\nme1212dc.lib)))
  (nets
    (net (code 1) (name "Net-(J4-Pad1)")
      (node (ref Q1) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 2) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 3) (name "Net-(R2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 4) (name "Net-(C4-Pad1)")
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 7))
      (node (ref C4) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 5) (name "Net-(J1-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 6) (name ARD_TEMP)
      (node (ref R1) (pin 2))
      (node (ref J2) (pin 4)))
    (net (code 7) (name ARD_GND)
      (node (ref R2) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 8) (name GND_ISO)
      (node (ref J5) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref U3) (pin 4))
      (node (ref U2) (pin 4))
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref C4) (pin 2)))
    (net (code 9) (name "Net-(R3-Pad2)")
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 3))
      (node (ref R3) (pin 2)))
    (net (code 10) (name GND)
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 11) (name VCC)
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 12) (name ARD_SRC_V)
      (node (ref J2) (pin 3)))
    (net (code 13) (name ARD_PWM)
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 14) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 15) (name VCC_ISO)
      (node (ref U3) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref R3) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 16) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 17) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 18) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 19) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))))