(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/PsuSwitch.RJ45/PsuSwitch.sch)
    (date "27/06/2017 16:27:51")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 2")
        (date 2017-06-13)
        (source PsuSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "For approval by Mansour")))))
  (components
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACB50))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACBF5))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF392))
    (comp (ref U2)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part 4N35))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E7A66))
    (comp (ref U3)
      (value TC4422AVPA)
      (footprint Housings_DIP:DIP-8_W7.62mm)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E820A))
    (comp (ref U1)
      (value NME1212DC)
      (footprint Housings_DIP:DIP-8_W7.62mm)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EC206))
    (comp (ref R3)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED01B))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED18A))
    (comp (ref J1)
      (value CONN_01X02)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 593FD4A9))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 593FD687))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59400A26))
    (comp (ref J3)
      (value CONN_01X02)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5A11))
    (comp (ref J2)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 595274F5)))
  (libparts
    (libpart (lib OAE.Parts) (part 4N35)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 4N35)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part TC4422AVPA)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name DRV_GATE)
      (node (ref C4) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 7)))
    (net (code 2) (name ARD_GND)
      (node (ref J2) (pin 8))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 3) (name ARD_TEMP)
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 5)))
    (net (code 4) (name ARD_5V)
      (node (ref J2) (pin 3))
      (node (ref J1) (pin 1)))
    (net (code 5) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7)))
    (net (code 6) (name ARD_SRC_V)
      (node (ref J2) (pin 6)))
    (net (code 7) (name ARD_PWM)
      (node (ref U2) (pin 1))
      (node (ref J2) (pin 4)))
    (net (code 8) (name DC_GND)
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 9) (name DC_IN)
      (node (ref J2) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 10) (name GND_ISO)
      (node (ref U3) (pin 4))
      (node (ref U3) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 11) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 12) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 13) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 14) (name DRV_SIG)
      (node (ref U3) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 15) (name DC_ISO)
      (node (ref C2) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref U3) (pin 8))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref R3) (pin 1)))
    (net (code 16) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))))