(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/Spikes/Arduino.sch)
    (date "21/06/2017 12:10:30")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Arduino.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref SHIELD1)
      (value ARDUINO_FOOTPRINT)
      (footprint FT:ARDUINO_SHIELD)
      (libsource (lib freetronics_schematic) (part ARDUINO_FOOTPRINT))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A541D)))
  (libparts
    (libpart (lib freetronics_schematic) (part ARDUINO_FOOTPRINT)
      (description "Arduino board device footprint (power inputs). Original by nicholasclewis")
      (docs http://www.thingiverse.com/thing:9630)
      (footprints
        (fp ARDUINO_SHIELD))
      (fields
        (field (name Reference) SHIELD)
        (field (name Value) ARDUINO_FOOTPRINT)
        (field (name Footprint) FT:ARDUINO_SHIELD))
      (pins
        (pin (num 0) (name 0) (type BiDi))
        (pin (num 1) (name 1) (type BiDi))
        (pin (num 2) (name 2) (type BiDi))
        (pin (num 3) (name 3) (type BiDi))
        (pin (num 4) (name 4) (type BiDi))
        (pin (num 5) (name 5) (type BiDi))
        (pin (num 5V) (name 5V) (type power_in))
        (pin (num 6) (name 6) (type BiDi))
        (pin (num 7) (name 7) (type BiDi))
        (pin (num 8) (name 8) (type BiDi))
        (pin (num 9) (name 9) (type BiDi))
        (pin (num 10) (name 10) (type BiDi))
        (pin (num 11) (name 11) (type BiDi))
        (pin (num 12) (name 12) (type BiDi))
        (pin (num 13) (name 13) (type BiDi))
        (pin (num 3V3) (name 3V3) (type power_in))
        (pin (num AD0) (name AD0) (type BiDi))
        (pin (num AD1) (name AD1) (type BiDi))
        (pin (num AD2) (name AD2) (type BiDi))
        (pin (num AD3) (name AD3) (type BiDi))
        (pin (num AD4) (name AD4) (type BiDi))
        (pin (num AD5) (name AD5) (type BiDi))
        (pin (num AREF) (name AREF) (type output))
        (pin (num GND1) (name GND1) (type power_in))
        (pin (num GND2) (name GND2) (type power_in))
        (pin (num GND3) (name GND3) (type power_in))
        (pin (num IO_R) (name IOREF) (type power_in))
        (pin (num NC) (name NC) (type passive))
        (pin (num RST) (name RST) (type BiDi))
        (pin (num SCL) (name SCL) (type BiDi))
        (pin (num SDA) (name SDA) (type BiDi))
        (pin (num SP1) (name MISO) (type BiDi))
        (pin (num SP2) (name Vcc) (type power_in))
        (pin (num SP3) (name SCK) (type BiDi))
        (pin (num SP4) (name MOSI) (type BiDi))
        (pin (num SP5) (name Reset) (type BiDi))
        (pin (num SP6) (name Gnd) (type power_in))
        (pin (num V_IN) (name V_IN) (type power_in)))))
  (libraries
    (library (logical freetronics_schematic)
      (uri C:\Development\freetronics_kicad_library\freetronics_schematic.lib)))
  (nets
    (net (code 1) (name "Net-(SHIELD1-PadSDA)")
      (node (ref SHIELD1) (pin SDA)))
    (net (code 2) (name "Net-(SHIELD1-PadSP2)")
      (node (ref SHIELD1) (pin SP2)))
    (net (code 3) (name "Net-(SHIELD1-PadAD3)")
      (node (ref SHIELD1) (pin AD3)))
    (net (code 4) (name "Net-(SHIELD1-PadSP3)")
      (node (ref SHIELD1) (pin SP3)))
    (net (code 5) (name "Net-(SHIELD1-Pad3V3)")
      (node (ref SHIELD1) (pin 3V3)))
    (net (code 6) (name "Net-(SHIELD1-PadAD4)")
      (node (ref SHIELD1) (pin AD4)))
    (net (code 7) (name "Net-(SHIELD1-PadSP4)")
      (node (ref SHIELD1) (pin SP4)))
    (net (code 8) (name "Net-(SHIELD1-PadAD5)")
      (node (ref SHIELD1) (pin AD5)))
    (net (code 9) (name "Net-(SHIELD1-PadSP5)")
      (node (ref SHIELD1) (pin SP5)))
    (net (code 10) (name "Net-(SHIELD1-PadSP6)")
      (node (ref SHIELD1) (pin SP6)))
    (net (code 11) (name "Net-(SHIELD1-PadAD2)")
      (node (ref SHIELD1) (pin AD2)))
    (net (code 12) (name "Net-(SHIELD1-PadSCL)")
      (node (ref SHIELD1) (pin SCL)))
    (net (code 13) (name "Net-(SHIELD1-PadRST)")
      (node (ref SHIELD1) (pin RST)))
    (net (code 14) (name "Net-(SHIELD1-PadGND1)")
      (node (ref SHIELD1) (pin GND1)))
    (net (code 15) (name "Net-(SHIELD1-PadGND2)")
      (node (ref SHIELD1) (pin GND2)))
    (net (code 16) (name "Net-(SHIELD1-PadGND3)")
      (node (ref SHIELD1) (pin GND3)))
    (net (code 17) (name "Net-(SHIELD1-PadAREF)")
      (node (ref SHIELD1) (pin AREF)))
    (net (code 18) (name "Net-(SHIELD1-PadV_IN)")
      (node (ref SHIELD1) (pin V_IN)))
    (net (code 19) (name "Net-(SHIELD1-PadIO_R)")
      (node (ref SHIELD1) (pin IO_R)))
    (net (code 20) (name "Net-(SHIELD1-Pad10)")
      (node (ref SHIELD1) (pin 10)))
    (net (code 21) (name "Net-(SHIELD1-Pad1)")
      (node (ref SHIELD1) (pin 1)))
    (net (code 22) (name "Net-(SHIELD1-Pad2)")
      (node (ref SHIELD1) (pin 2)))
    (net (code 23) (name "Net-(SHIELD1-Pad3)")
      (node (ref SHIELD1) (pin 3)))
    (net (code 24) (name "Net-(SHIELD1-Pad4)")
      (node (ref SHIELD1) (pin 4)))
    (net (code 25) (name "Net-(SHIELD1-Pad5)")
      (node (ref SHIELD1) (pin 5)))
    (net (code 26) (name "Net-(SHIELD1-Pad6)")
      (node (ref SHIELD1) (pin 6)))
    (net (code 27) (name "Net-(SHIELD1-Pad7)")
      (node (ref SHIELD1) (pin 7)))
    (net (code 28) (name "Net-(SHIELD1-Pad8)")
      (node (ref SHIELD1) (pin 8)))
    (net (code 29) (name "Net-(SHIELD1-Pad9)")
      (node (ref SHIELD1) (pin 9)))
    (net (code 30) (name "Net-(SHIELD1-Pad0)")
      (node (ref SHIELD1) (pin 0)))
    (net (code 31) (name "Net-(SHIELD1-Pad11)")
      (node (ref SHIELD1) (pin 11)))
    (net (code 32) (name "Net-(SHIELD1-Pad12)")
      (node (ref SHIELD1) (pin 12)))
    (net (code 33) (name "Net-(SHIELD1-Pad13)")
      (node (ref SHIELD1) (pin 13)))
    (net (code 34) (name "Net-(SHIELD1-PadNC)")
      (node (ref SHIELD1) (pin NC)))
    (net (code 35) (name "Net-(SHIELD1-Pad5V)")
      (node (ref SHIELD1) (pin 5V)))
    (net (code 36) (name "Net-(SHIELD1-PadAD0)")
      (node (ref SHIELD1) (pin AD0)))
    (net (code 37) (name "Net-(SHIELD1-PadAD1)")
      (node (ref SHIELD1) (pin AD1)))
    (net (code 38) (name "Net-(SHIELD1-PadSP1)")
      (node (ref SHIELD1) (pin SP1)))))