(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/FuseBoard/Fuseboard.sch)
    (date "21/09/2017 14:36:39")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Fuseboard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref F2)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7F37B))
    (comp (ref J2)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7F5EE))
    (comp (ref J7)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7F611))
    (comp (ref J21)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7FB58))
    (comp (ref U1)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A802DA))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8067F))
    (comp (ref J1)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A80685))
    (comp (ref J6)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8068B))
    (comp (ref R1)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A80E6E))
    (comp (ref F3)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81937))
    (comp (ref J3)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8193D))
    (comp (ref J8)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81943))
    (comp (ref R2)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81956))
    (comp (ref F6)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81E2A))
    (comp (ref J12)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81E30))
    (comp (ref J16)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81E36))
    (comp (ref R5)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A81E43))
    (comp (ref F7)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A82012))
    (comp (ref J13)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A82018))
    (comp (ref J17)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8201E))
    (comp (ref R6)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8202B))
    (comp (ref U2)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8265A))
    (comp (ref F10)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A83E))
    (comp (ref J22)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A844))
    (comp (ref J26)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A84A))
    (comp (ref U3)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A850))
    (comp (ref R9)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A85D))
    (comp (ref F11)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A871))
    (comp (ref J23)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A877))
    (comp (ref J27)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A87D))
    (comp (ref R10)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A88A))
    (comp (ref F14)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8A4))
    (comp (ref J30)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8AA))
    (comp (ref J34)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8B0))
    (comp (ref R13)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8BD))
    (comp (ref F15)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8D1))
    (comp (ref J31)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8D7))
    (comp (ref J35)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8DD))
    (comp (ref R14)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8EA))
    (comp (ref U4)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8A8FE))
    (comp (ref F4)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF14))
    (comp (ref J4)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF1A))
    (comp (ref J9)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF20))
    (comp (ref R3)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF33))
    (comp (ref F5)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF47))
    (comp (ref J5)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF4D))
    (comp (ref J10)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF53))
    (comp (ref R4)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF60))
    (comp (ref F8)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF7A))
    (comp (ref J14)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF80))
    (comp (ref J18)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF86))
    (comp (ref R7)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AF93))
    (comp (ref F9)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFA7))
    (comp (ref J15)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFAD))
    (comp (ref J19)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFB3))
    (comp (ref R8)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFC0))
    (comp (ref F12)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFE0))
    (comp (ref J24)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFE6))
    (comp (ref J28)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFEC))
    (comp (ref R11)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8AFFF))
    (comp (ref F13)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B013))
    (comp (ref J25)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B019))
    (comp (ref J29)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B01F))
    (comp (ref R12)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B02C))
    (comp (ref F16)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B046))
    (comp (ref J32)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B04C))
    (comp (ref J36)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B052))
    (comp (ref R15)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B05F))
    (comp (ref F17)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_inline_Type-I)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B073))
    (comp (ref J33)
      (value IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B079))
    (comp (ref J37)
      (value OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B07F))
    (comp (ref R16)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A8B08C))
    (comp (ref J20)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3C803))
    (comp (ref J11)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3DA36)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib linear) (part LM2902N)
      (aliases
        (alias LM324)
        (alias TLC274)
        (alias TL074)
        (alias LM324N)
        (alias LM324AN)
        (alias MCP6004)
        (alias TL084)
        (alias TL064)
        (alias LMV324)
        (alias LMC6484)
        (alias MCP604))
      (description "Quad Op amp.")
      (docs op_amps/lm324.pdf)
      (footprints
        (fp SOIC*Pitch1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*Pitch0.65mm*)
        (fp SSOP*)
        (fp MSOP*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2902N))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical linear)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\linear.lib")))
  (nets
    (net (code 1) (name "Net-(F9-Pad1)")
      (node (ref U2) (pin 12))
      (node (ref F9) (pin 1))
      (node (ref J19) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 2) (name GND)
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 11))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref F1) (pin 1))
      (node (ref U1) (pin 11))
      (node (ref R4) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U3) (pin 11))
      (node (ref R11) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref U4) (pin 11)))
    (net (code 3) (name CUR_12)
      (node (ref J11) (pin 4))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 14)))
    (net (code 4) (name "Net-(F9-Pad2)")
      (node (ref J15) (pin 1))
      (node (ref F9) (pin 2)))
    (net (code 5) (name CUR_11)
      (node (ref J11) (pin 3))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 9)))
    (net (code 6) (name "Net-(F8-Pad1)")
      (node (ref U2) (pin 10))
      (node (ref F8) (pin 1))
      (node (ref J18) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 7) (name "Net-(F12-Pad2)")
      (node (ref J24) (pin 1))
      (node (ref F12) (pin 2)))
    (net (code 8) (name CUR_13)
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 8))
      (node (ref J11) (pin 5)))
    (net (code 9) (name "Net-(F12-Pad1)")
      (node (ref U3) (pin 10))
      (node (ref J28) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref F12) (pin 1)))
    (net (code 10) (name ARD_5V)
      (node (ref U2) (pin 4))
      (node (ref J21) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref U3) (pin 4))
      (node (ref U4) (pin 4)))
    (net (code 11) (name "Net-(F5-Pad2)")
      (node (ref F5) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 12) (name CUR_9)
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 8))
      (node (ref J11) (pin 1)))
    (net (code 13) (name "Net-(F4-Pad1)")
      (node (ref J9) (pin 1))
      (node (ref U1) (pin 10))
      (node (ref R3) (pin 1))
      (node (ref F4) (pin 1)))
    (net (code 14) (name "Net-(F8-Pad2)")
      (node (ref F8) (pin 2))
      (node (ref J14) (pin 1)))
    (net (code 15) (name CUR_10)
      (node (ref U1) (pin 13))
      (node (ref U1) (pin 14))
      (node (ref J11) (pin 2)))
    (net (code 16) (name "Net-(F5-Pad1)")
      (node (ref F5) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref U1) (pin 12)))
    (net (code 17) (name CUR_1)
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref J20) (pin 1)))
    (net (code 18) (name CUR_16)
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 13))
      (node (ref J11) (pin 8)))
    (net (code 19) (name "Net-(F17-Pad1)")
      (node (ref R16) (pin 1))
      (node (ref J37) (pin 1))
      (node (ref U4) (pin 12))
      (node (ref F17) (pin 1)))
    (net (code 20) (name CUR_15)
      (node (ref J11) (pin 7))
      (node (ref U4) (pin 9))
      (node (ref U4) (pin 8)))
    (net (code 21) (name CUR_14)
      (node (ref U3) (pin 13))
      (node (ref J11) (pin 6))
      (node (ref U3) (pin 14)))
    (net (code 22) (name CUR_8)
      (node (ref J20) (pin 8))
      (node (ref U4) (pin 6))
      (node (ref U4) (pin 7)))
    (net (code 23) (name CUR_7)
      (node (ref U4) (pin 1))
      (node (ref J20) (pin 7))
      (node (ref U4) (pin 2)))
    (net (code 24) (name CUR_6)
      (node (ref U3) (pin 7))
      (node (ref U3) (pin 6))
      (node (ref J20) (pin 6)))
    (net (code 25) (name CUR_5)
      (node (ref U3) (pin 1))
      (node (ref J20) (pin 5))
      (node (ref U3) (pin 2)))
    (net (code 26) (name "Net-(F13-Pad1)")
      (node (ref F13) (pin 1))
      (node (ref J29) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref U3) (pin 12)))
    (net (code 27) (name "Net-(F13-Pad2)")
      (node (ref F13) (pin 2))
      (node (ref J25) (pin 1)))
    (net (code 28) (name "Net-(F17-Pad2)")
      (node (ref J33) (pin 1))
      (node (ref F17) (pin 2)))
    (net (code 29) (name "Net-(F16-Pad1)")
      (node (ref R15) (pin 1))
      (node (ref J36) (pin 1))
      (node (ref U4) (pin 10))
      (node (ref F16) (pin 1)))
    (net (code 30) (name "Net-(F16-Pad2)")
      (node (ref J32) (pin 1))
      (node (ref F16) (pin 2)))
    (net (code 31) (name "Net-(F6-Pad2)")
      (node (ref F6) (pin 2))
      (node (ref J12) (pin 1)))
    (net (code 32) (name "Net-(F6-Pad1)")
      (node (ref F6) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref R5) (pin 1)))
    (net (code 33) (name CUR_2)
      (node (ref U1) (pin 7))
      (node (ref J20) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 34) (name "Net-(F3-Pad1)")
      (node (ref J8) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref F3) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 35) (name CUR_3)
      (node (ref J20) (pin 3))
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 1)))
    (net (code 36) (name CUR_4)
      (node (ref J20) (pin 4))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 6)))
    (net (code 37) (name "Net-(F7-Pad1)")
      (node (ref F7) (pin 1))
      (node (ref J17) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 38) (name "Net-(F7-Pad2)")
      (node (ref J13) (pin 1))
      (node (ref F7) (pin 2)))
    (net (code 39) (name "Net-(F1-Pad2)")
      (node (ref F1) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 40) (name "Net-(J21-Pad8)")
      (node (ref J21) (pin 8)))
    (net (code 41) (name "Net-(J21-Pad7)")
      (node (ref J21) (pin 7)))
    (net (code 42) (name "Net-(J21-Pad6)")
      (node (ref J21) (pin 6)))
    (net (code 43) (name "Net-(J21-Pad5)")
      (node (ref J21) (pin 5)))
    (net (code 44) (name "Net-(J21-Pad4)")
      (node (ref J21) (pin 4)))
    (net (code 45) (name ARD_REF)
      (node (ref J21) (pin 3)))
    (net (code 46) (name ARD_GND)
      (node (ref J21) (pin 1)))
    (net (code 47) (name "Net-(F2-Pad2)")
      (node (ref J2) (pin 1))
      (node (ref F2) (pin 2)))
    (net (code 48) (name "Net-(F3-Pad2)")
      (node (ref J3) (pin 1))
      (node (ref F3) (pin 2)))
    (net (code 49) (name "Net-(F2-Pad1)")
      (node (ref F2) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 3)))
    (net (code 50) (name "Net-(F15-Pad2)")
      (node (ref J31) (pin 1))
      (node (ref F15) (pin 2)))
    (net (code 51) (name "Net-(F14-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref J34) (pin 1))
      (node (ref F14) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 52) (name "Net-(F14-Pad2)")
      (node (ref F14) (pin 2))
      (node (ref J30) (pin 1)))
    (net (code 53) (name "Net-(F4-Pad2)")
      (node (ref F4) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 54) (name "Net-(F15-Pad1)")
      (node (ref F15) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref J35) (pin 1))
      (node (ref R14) (pin 1)))
    (net (code 55) (name "Net-(F10-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref J26) (pin 1))
      (node (ref F10) (pin 1)))
    (net (code 56) (name "Net-(F10-Pad2)")
      (node (ref F10) (pin 2))
      (node (ref J22) (pin 1)))
    (net (code 57) (name "Net-(F11-Pad1)")
      (node (ref J27) (pin 1))
      (node (ref F11) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref R10) (pin 1)))
    (net (code 58) (name "Net-(F11-Pad2)")
      (node (ref J23) (pin 1))
      (node (ref F11) (pin 2)))))