(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/HBridge/HBridge.sch)
    (date "31/08/2017 11:26:32")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "HBridge (Single Board)")
        (company Enertechnos)
        (rev Rev2)
        (date 2017-08-30)
        (source HBridge.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /HBridge.Switch.1/) (tstamps /59498AA5/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source HBridge.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /HBridge.Switch.2/) (tstamps /59A7109E/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source HBridge.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /HBridge.Switch.3/) (tstamps /59A71299/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source HBridge.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /HBridge.Switch.4/) (tstamps /59A712A3/)
      (title_block
        (title "HBridge (Single Board)")
        (company)
        (rev Rev2)
        (date 2017-08-30)
        (source HBridge.Switch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59526541))
    (comp (ref J2)
      (value "Temperature Probe")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF2))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF9))
    (comp (ref IC1)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib HBridge-cache) (part TC4422AVPA-RESCUE-HBridge))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498139))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498146))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5949814D))
    (comp (ref J3)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 595237FD))
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3D9))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3E0))
    (comp (ref U1)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3EA))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DA9F))
    (comp (ref U2)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part 4N35))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAA6))
    (comp (ref R3)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAAD))
    (comp (ref IC2)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib HBridge-cache) (part TC4422AVPA-RESCUE-HBridge))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498139))
    (comp (ref C8)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498146))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5949814D))
    (comp (ref J4)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 595237FD))
    (comp (ref C5)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3D9))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3E0))
    (comp (ref U3)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3EA))
    (comp (ref R4)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DA9F))
    (comp (ref U4)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part 4N35))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAA6))
    (comp (ref R5)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAAD))
    (comp (ref IC3)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib HBridge-cache) (part TC4422AVPA-RESCUE-HBridge))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498139))
    (comp (ref C12)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498146))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 5949814D))
    (comp (ref J5)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 595237FD))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3D9))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3E0))
    (comp (ref U5)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3EA))
    (comp (ref R6)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DA9F))
    (comp (ref U6)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part 4N35))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAA6))
    (comp (ref R7)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAAD))
    (comp (ref IC4)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib HBridge-cache) (part TC4422AVPA-RESCUE-HBridge))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498139))
    (comp (ref C16)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498146))
    (comp (ref C15)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5949814D))
    (comp (ref J6)
      (value "Drive Signal")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 595237FD))
    (comp (ref C13)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3D9))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3E0))
    (comp (ref U7)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3EA))
    (comp (ref R8)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DA9F))
    (comp (ref U8)
      (value 4N35)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part 4N35))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAA6))
    (comp (ref R9)
      (value 1K5)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /HBridge.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAAD)))
  (libparts
    (libpart (lib OAE.Parts) (part 4N35)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 4N35)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib HBridge-cache) (part TC4422AVPA-RESCUE-HBridge)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA-RESCUE-HBridge)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type unspc))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical HBridge-cache)
      (uri C:\Development\multilevelinverter\Hardware\MLI\HBridge\HBridge-cache.lib)))
  (nets
    (net (code 1) (name DRV_SIG_B)
      (node (ref U6) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 2) (name DC_GND)
      (node (ref U5) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 3) (name ARD_GND)
      (node (ref R8) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref R6) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 4) (name DRV_SIG_A)
      (node (ref U2) (pin 1))
      (node (ref U8) (pin 1)))
    (net (code 5) (name DC_IN)
      (node (ref U1) (pin 4))
      (node (ref U7) (pin 4))
      (node (ref U5) (pin 4))
      (node (ref U3) (pin 4))
      (node (ref J1) (pin 1)))
    (net (code 6) (name ARD_PWM_B)
      (node (ref J1) (pin 4)))
    (net (code 7) (name ARD_PWM_A)
      (node (ref J1) (pin 3)))
    (net (code 8) (name ARD_TEMP)
      (node (ref R1) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 6)))
    (net (code 9) (name ARD_5V)
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 1)))
    (net (code 10) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 11) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 12) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 13) (name Earth)
      (node (ref J4) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref IC2) (pin 4))
      (node (ref IC2) (pin 5))
      (node (ref C5) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U8) (pin 4))
      (node (ref C15) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref IC4) (pin 5))
      (node (ref IC4) (pin 4))
      (node (ref IC3) (pin 4))
      (node (ref C11) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref IC3) (pin 5))
      (node (ref U6) (pin 4))
      (node (ref J5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref C6) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref IC1) (pin 5))
      (node (ref IC1) (pin 4))
      (node (ref J3) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref C2) (pin 2)))
    (net (code 14) (name "Net-(C3-Pad2)")
      (node (ref IC1) (pin 6))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref IC1) (pin 7))
      (node (ref J3) (pin 1)))
    (net (code 15) (name "Net-(IC1-Pad2)")
      (node (ref IC1) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 16) (name "Net-(R3-Pad2)")
      (node (ref U2) (pin 6))
      (node (ref R3) (pin 2)))
    (net (code 17) (name "Net-(IC1-Pad1)")
      (node (ref IC1) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref IC1) (pin 8))
      (node (ref R3) (pin 1)))
    (net (code 18) (name "Net-(IC1-Pad3)")
      (node (ref IC1) (pin 3)))
    (net (code 19) (name "Net-(C1-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 20) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 21) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 2)))
    (net (code 22) (name "Net-(IC2-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref IC2) (pin 8))
      (node (ref U3) (pin 7))
      (node (ref IC2) (pin 1)))
    (net (code 23) (name "Net-(IC2-Pad2)")
      (node (ref U4) (pin 5))
      (node (ref IC2) (pin 2)))
    (net (code 24) (name "Net-(R5-Pad2)")
      (node (ref U4) (pin 6))
      (node (ref R5) (pin 2)))
    (net (code 25) (name "Net-(C7-Pad2)")
      (node (ref C8) (pin 1))
      (node (ref IC2) (pin 7))
      (node (ref IC2) (pin 6))
      (node (ref C7) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 26) (name "Net-(IC2-Pad3)")
      (node (ref IC2) (pin 3)))
    (net (code 27) (name "Net-(C5-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref C5) (pin 1)))
    (net (code 28) (name "Net-(R6-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 29) (name "Net-(IC3-Pad1)")
      (node (ref IC3) (pin 8))
      (node (ref R7) (pin 1))
      (node (ref U5) (pin 7))
      (node (ref IC3) (pin 1)))
    (net (code 30) (name "Net-(IC3-Pad2)")
      (node (ref IC3) (pin 2))
      (node (ref U6) (pin 5)))
    (net (code 31) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 32) (name "Net-(R7-Pad2)")
      (node (ref U6) (pin 6))
      (node (ref R7) (pin 2)))
    (net (code 33) (name "Net-(C11-Pad2)")
      (node (ref IC3) (pin 6))
      (node (ref IC3) (pin 7))
      (node (ref C11) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref C12) (pin 1)))
    (net (code 34) (name "Net-(IC3-Pad3)")
      (node (ref IC3) (pin 3)))
    (net (code 35) (name "Net-(C10-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref C10) (pin 1)))
    (net (code 36) (name "Net-(R8-Pad2)")
      (node (ref U8) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 37) (name "Net-(IC4-Pad2)")
      (node (ref IC4) (pin 2))
      (node (ref U8) (pin 5)))
    (net (code 38) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 39) (name "Net-(R9-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref U8) (pin 6)))
    (net (code 40) (name "Net-(C15-Pad2)")
      (node (ref C15) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref IC4) (pin 7))
      (node (ref IC4) (pin 6)))
    (net (code 41) (name "Net-(IC4-Pad3)")
      (node (ref IC4) (pin 3)))
    (net (code 42) (name "Net-(IC4-Pad1)")
      (node (ref IC4) (pin 8))
      (node (ref IC4) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref U7) (pin 7)))
    (net (code 43) (name "Net-(C13-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref U7) (pin 5))
      (node (ref C13) (pin 1)))))