(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MosfetSwitch.OAE/MosfetSwitch.sch)
    (date "12/06/2017 18:38:54")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 1")
        (date 2017-05-31)
        (source MosfetSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C3)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACB50))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACBF5))
    (comp (ref R2)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF392))
    (comp (ref J2)
      (value DC_CONN)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 592C95DB))
    (comp (ref J4)
      (value DrainLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA485))
    (comp (ref J5)
      (value SourceLarge)
      (footprint Wire_Pads:SolderWirePad_single_2-5mmDrill)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 592CA834))
    (comp (ref D1)
      (value D_Schottky_x2_KCom_AKA)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DCE5E))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib MosfetSwitch-cache) (part RFP12N10L))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF9D4))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EA608))
    (comp (ref U1)
      (value NME1212DC)
      (footprint Housings_DIP:DIP-8_W7.62mm_Socket)
      (libsource (lib MosfetSwitch-cache) (part NME1212DC))
      (sheetpath (names /) (tstamps /))
      (tstamp 592EC206))
    (comp (ref C2)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ED18A))
    (comp (ref J1)
      (value TEMP_PROBE)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 59355101))
    (comp (ref R1)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5935695A))
    (comp (ref U2)
      (value TLP250H)
      (footprint Housings_DIP:DIP-8_W7.62mm_Socket)
      (libsource (lib OAE_parts) (part TLP250H))
      (sheetpath (names /) (tstamps /))
      (tstamp 593ED3B7))
    (comp (ref J3)
      (value RJ45-U)
      (footprint OAE_Footprints:RJ45_8)
      (libsource (lib OAE_parts) (part RJ45-U))
      (sheetpath (names /) (tstamps /))
      (tstamp 593ECA34)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib MosfetSwitch-cache) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MosfetSwitch-cache) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib OAE_parts) (part RJ45-U)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45-U))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE_parts) (part TLP250H)
      (description "Gate Drive Optocoupler, Output Current 1.5/1.5A")
      (docs http://toshiba.semicon-storage.com/info/docget.jsp?did=16821&prodName=TLP250)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TLP250H)
        (field (name Footprint) Housings_DIP:DIP-8_W7.62mm))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name A) (type passive))
        (pin (num 3) (name C) (type passive))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name VEE) (type power_out))
        (pin (num 6) (name VO) (type passive))
        (pin (num 7) (name NC) (type NotConnected))
        (pin (num 8) (name VCC) (type power_in)))))
  (libraries
    (library (logical MosfetSwitch-cache)
      (uri C:\Development\multilevelinverter\Hardware\MosfetSwitch.OAE\MosfetSwitch-cache.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical OAE_parts)
      (uri C:\Users\gobrien\ownCloud.Yupon\OAE\Electronics\PartsLibraries\OAE_parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name ARD_GND)
      (node (ref J1) (pin 1))
      (node (ref J3) (pin 8))
      (node (ref R2) (pin 1)))
    (net (code 2) (name GND_ISO)
      (node (ref D1) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 3) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref Q1) (pin 1)))
    (net (code 4) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 5) (name "Net-(J4-Pad1)")
      (node (ref Q1) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 6) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 7) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 8) (name ARD_SRC_V)
      (node (ref J3) (pin 4)))
    (net (code 9) (name ARD_PWM)
      (node (ref J3) (pin 3))
      (node (ref U2) (pin 2)))
    (net (code 10) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2)))
    (net (code 11) (name ARD_5V)
      (node (ref J3) (pin 1)))
    (net (code 12) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 13) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 14) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 15) (name ARD_TEMP)
      (node (ref J3) (pin 5))
      (node (ref R1) (pin 2)))
    (net (code 16) (name GND)
      (node (ref J2) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 17) (name VCC)
      (node (ref U1) (pin 4))
      (node (ref J2) (pin 1)))
    (net (code 18) (name "Net-(D1-Pad1)")
      (node (ref Q1) (pin 3))
      (node (ref D1) (pin 1)))
    (net (code 19) (name "Net-(R2-Pad2)")
      (node (ref U2) (pin 3))
      (node (ref R2) (pin 2)))
    (net (code 20) (name VCC_ISO)
      (node (ref C1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U1) (pin 7)))
    (net (code 21) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 22) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))))