(export (version D)
  (design
    (source C:/Development/multilevelinverter/Hardware/MLI/PsuSwitchPower/PsuSwitchPower.sch)
    (date "21/06/2017 12:14:57")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI MOSFET Driver Board")
        (company "Enertechnos Ltd")
        (rev "rev 2")
        (date 2017-06-13)
        (source PsuSwitchPower.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "For approval by Mansour")))))
  (components
    (comp (ref D1)
      (value PWR_DIODE)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (libsource (lib device) (part D_Schottky_x2_KCom_AKA))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DCE5E))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF9D4))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59400AF8))
    (comp (ref J3)
      (value SRC)
      (footprint PartsLibraries:PowerConnector)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A5470))
    (comp (ref J2)
      (value DRN)
      (footprint PartsLibraries:PowerConnector)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A55EB))
    (comp (ref J1)
      (value Control)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 594A533B)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02, pin header")
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib device) (part D_Schottky_x2_KCom_AKA)
      (description "Dual schottky diode, common cathode")
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_x2_KCom_AKA))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name A) (type passive))))
    (libpart (lib OAE.Parts) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc)))))
  (libraries
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib)))
  (nets
    (net (code 1) (name "Net-(C1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 2) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref J3) (pin 1)))
    (net (code 3) (name GND_ISO)
      (node (ref D1) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 4) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 5) (name DRV_GATE)
      (node (ref J1) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 6) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3)))))