(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/PsuSwitchModule/PsuSwitchModule.sch)
    (date "14/12/2017 17:44:59")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev Rev3.3)
        (date 2017-12-14)
        (source PsuSwitchModule.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev Rev3.3)
        (date 2017-12-14)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev Rev3.3)
        (date 2017-12-14)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /PsuSwitchModule.Switch.3/) (tstamps /59A71299/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev Rev3.3)
        (date 2017-12-14)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev Rev3.3)
        (date 2017-12-14)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Monitor)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59526541))
    (comp (ref J2)
      (value "Temperature Probe")
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF2))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF9))
    (comp (ref J7)
      (value Control)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7EBD8))
    (comp (ref J3)
      (value SignalToPower)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A16B56F))
    (comp (ref J101)
      (value Conn_01x03)
      (footprint Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3469C9))
    (comp (ref IC1)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498139))
    (comp (ref C4)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498146))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5949814D))
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3D9))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3E0))
    (comp (ref U1)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3EA))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DA9F))
    (comp (ref U2)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAA6))
    (comp (ref R3)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAAD))
    (comp (ref D1)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0E59))
    (comp (ref C17)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0ED7))
    (comp (ref R10)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0FC7))
    (comp (ref R11)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1A58))
    (comp (ref C18)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1DD4))
    (comp (ref C25)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5A16CD08))
    (comp (ref IC2)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498139))
    (comp (ref C8)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498146))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5949814D))
    (comp (ref C5)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3D9))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3E0))
    (comp (ref U3)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3EA))
    (comp (ref R4)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DA9F))
    (comp (ref U4)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAA6))
    (comp (ref R5)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAAD))
    (comp (ref D2)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0E59))
    (comp (ref C19)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0ED7))
    (comp (ref R12)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0FC7))
    (comp (ref R13)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1A58))
    (comp (ref C20)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1DD4))
    (comp (ref C26)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5A16CD08))
    (comp (ref IC3)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498139))
    (comp (ref C12)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498146))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5949814D))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3D9))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3E0))
    (comp (ref U5)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3EA))
    (comp (ref R6)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DA9F))
    (comp (ref U6)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAA6))
    (comp (ref R7)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAAD))
    (comp (ref D3)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0E59))
    (comp (ref C21)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0ED7))
    (comp (ref R14)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0FC7))
    (comp (ref R15)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1A58))
    (comp (ref C22)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1DD4))
    (comp (ref C27)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5A16CD08))
    (comp (ref IC4)
      (value TC4422AVPA)
      (footprint PartsLibraries:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (libsource (lib OAE.Parts) (part TC4422AVPA))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498139))
    (comp (ref C16)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498146))
    (comp (ref C15)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5949814D))
    (comp (ref C13)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3D9))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3E0))
    (comp (ref U7)
      (value NME1212DC)
      (footprint PartsLibraries:TC4422AVPA)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3EA))
    (comp (ref R8)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DA9F))
    (comp (ref U8)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAA6))
    (comp (ref R9)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAAD))
    (comp (ref D4)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib device) (part D_Zener))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0E59))
    (comp (ref C23)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0ED7))
    (comp (ref R16)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0FC7))
    (comp (ref R17)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1A58))
    (comp (ref C24)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1DD4))
    (comp (ref C28)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5A16CD08)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib conn) (part Conn_01x03)
      (description "Generic connector, single row, 01x03")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib device) (part D_Zener)
      (description "Zener Diode")
      (docs https://en.wikipedia.org/wiki/Zener_diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib OAE.Parts) (part H11N1M)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) H11N1M)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part TC4422AVPA)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name DC_IN)
      (node (ref U7) (pin 4))
      (node (ref U1) (pin 4))
      (node (ref U5) (pin 4))
      (node (ref J7) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 2) (name DRV_GATE_B)
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref IC2) (pin 7))
      (node (ref IC2) (pin 6))
      (node (ref R13) (pin 1))
      (node (ref J3) (pin 6)))
    (net (code 3) (name GND_ISO_1)
      (node (ref R11) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref IC1) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref C4) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref IC1) (pin 4))
      (node (ref J3) (pin 5)))
    (net (code 4) (name GND_ISO_4)
      (node (ref R17) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref J3) (pin 4))
      (node (ref C24) (pin 2))
      (node (ref U7) (pin 7))
      (node (ref IC4) (pin 4))
      (node (ref IC4) (pin 5))
      (node (ref U8) (pin 5))
      (node (ref C16) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C14) (pin 2)))
    (net (code 5) (name DRV_GATE_C)
      (node (ref IC3) (pin 6))
      (node (ref IC3) (pin 7))
      (node (ref C12) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref J3) (pin 3)))
    (net (code 6) (name DRV_GATE_D)
      (node (ref C15) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref IC4) (pin 7))
      (node (ref IC4) (pin 6))
      (node (ref R17) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 7) (name GND_ISO_3)
      (node (ref R15) (pin 2))
      (node (ref IC3) (pin 5))
      (node (ref C22) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref IC3) (pin 4))
      (node (ref U5) (pin 7))
      (node (ref C12) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref U6) (pin 5))
      (node (ref C11) (pin 1))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2)))
    (net (code 8) (name "Net-(J7-Pad8)")
      (node (ref J7) (pin 8)))
    (net (code 9) (name "Net-(J7-Pad7)")
      (node (ref J7) (pin 7)))
    (net (code 10) (name ARD_PWM_D)
      (node (ref C28) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref J7) (pin 6)))
    (net (code 11) (name ARD_PWM_C)
      (node (ref R6) (pin 1))
      (node (ref C27) (pin 2))
      (node (ref J7) (pin 5)))
    (net (code 12) (name ARD_PWM_B)
      (node (ref J7) (pin 4))
      (node (ref R4) (pin 1))
      (node (ref C26) (pin 2)))
    (net (code 13) (name ARD_PWM_A)
      (node (ref C25) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref J7) (pin 3)))
    (net (code 14) (name DC_GND)
      (node (ref J7) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 15) (name DRV_GATE_A)
      (node (ref J3) (pin 7))
      (node (ref IC1) (pin 6))
      (node (ref IC1) (pin 7))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 16) (name ARD_CUR)
      (node (ref J101) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 17) (name GND_ISO_2)
      (node (ref C5) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref U3) (pin 7))
      (node (ref C6) (pin 2))
      (node (ref IC2) (pin 4))
      (node (ref D2) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref J3) (pin 8))
      (node (ref IC2) (pin 5))
      (node (ref C7) (pin 1))
      (node (ref C19) (pin 2)))
    (net (code 18) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 19) (name ARD_GND)
      (node (ref J101) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref U6) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 8)))
    (net (code 20) (name ARD_VCC)
      (node (ref J1) (pin 7))
      (node (ref J101) (pin 3))
      (node (ref J2) (pin 1)))
    (net (code 21) (name ARD_TEMP)
      (node (ref J2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 22) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 23) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 24) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 25) (name "Net-(IC1-Pad2)")
      (node (ref U2) (pin 4))
      (node (ref R10) (pin 2))
      (node (ref IC1) (pin 2)))
    (net (code 26) (name "Net-(C17-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 6))
      (node (ref D1) (pin 1)))
    (net (code 27) (name "Net-(C25-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref C25) (pin 1)))
    (net (code 28) (name "Net-(C1-Pad1)")
      (node (ref C18) (pin 1))
      (node (ref IC1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref IC1) (pin 8))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 29) (name "Net-(IC1-Pad3)")
      (node (ref IC1) (pin 3)))
    (net (code 30) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 31) (name "Net-(IC2-Pad2)")
      (node (ref U4) (pin 4))
      (node (ref R12) (pin 2))
      (node (ref IC2) (pin 2)))
    (net (code 32) (name "Net-(C19-Pad1)")
      (node (ref U4) (pin 6))
      (node (ref D2) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 33) (name "Net-(C26-Pad1)")
      (node (ref C26) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 34) (name "Net-(C20-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref IC2) (pin 8))
      (node (ref C5) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref IC2) (pin 1))
      (node (ref C20) (pin 1)))
    (net (code 35) (name "Net-(IC2-Pad3)")
      (node (ref IC2) (pin 3)))
    (net (code 36) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 37) (name "Net-(C21-Pad1)")
      (node (ref C21) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U6) (pin 6))
      (node (ref R7) (pin 2)))
    (net (code 38) (name "Net-(IC3-Pad2)")
      (node (ref IC3) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref R14) (pin 2)))
    (net (code 39) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 40) (name "Net-(C10-Pad1)")
      (node (ref C22) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref IC3) (pin 1))
      (node (ref IC3) (pin 8))
      (node (ref C10) (pin 1))
      (node (ref U5) (pin 5)))
    (net (code 41) (name "Net-(IC3-Pad3)")
      (node (ref IC3) (pin 3)))
    (net (code 42) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 43) (name "Net-(IC4-Pad2)")
      (node (ref U8) (pin 4))
      (node (ref IC4) (pin 2))
      (node (ref R16) (pin 2)))
    (net (code 44) (name "Net-(C23-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref U8) (pin 6))
      (node (ref C23) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 45) (name "Net-(C28-Pad1)")
      (node (ref U8) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref C28) (pin 1)))
    (net (code 46) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 47) (name "Net-(C13-Pad1)")
      (node (ref U7) (pin 5))
      (node (ref R9) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref IC4) (pin 8))
      (node (ref IC4) (pin 1)))
    (net (code 48) (name "Net-(IC4-Pad3)")
      (node (ref IC4) (pin 3)))))