(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/FuseBoard/Fuseboard.sch)
    (date "14/12/2017 10:16:31")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source Fuseboard.sch)
        (comment (number 1) (value "FOR REVIEW"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /VoltMeter4/) (tstamps /59C4F642/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /VoltMeter3/) (tstamps /59C51A28/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /VoltMeter2/) (tstamps /59C51FF6/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /VoltMeter1/) (tstamps /59C5216A/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /VoltMeter8/) (tstamps /59C53BAD/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /VoltMeter7/) (tstamps /59C53BBB/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /VoltMeter6/) (tstamps /59C53BC9/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /VoltMeter5/) (tstamps /59C53BD7/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Rev 3.2")
        (date 2017-12-12)
        (source VoltMeter.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J110)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3DA36))
    (comp (ref J106)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A305622))
    (comp (ref F101)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A311AB6))
    (comp (ref J102)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A311D56))
    (comp (ref F102)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314BDF))
    (comp (ref F103)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31508D))
    (comp (ref F104)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A316DCF))
    (comp (ref F105)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A319EA5))
    (comp (ref F106)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B529))
    (comp (ref F107)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B608))
    (comp (ref F108)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B6ED))
    (comp (ref J103)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A313F9B))
    (comp (ref J104)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3140C8))
    (comp (ref J105)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314202))
    (comp (ref J107)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31433B))
    (comp (ref J108)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314473))
    (comp (ref J109)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314620))
    (comp (ref J111)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31493D))
    (comp (ref J112)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314C5C))
    (comp (ref J113)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314D91))
    (comp (ref J114)
      (value INPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314EE1))
    (comp (ref J115)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31577A))
    (comp (ref J116)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3158B0))
    (comp (ref J117)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3159DB))
    (comp (ref J118)
      (value OUTPUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A315B01))
    (comp (ref J123)
      (value -VE)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3187AF))
    (comp (ref U101)
      (value TC4051BP)
      (footprint Housings_DIP:DIP-16_W7.62mm_Socket)
      (libsource (lib OAE.Parts) (part TC4051BP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B088))
    (comp (ref U201)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F962))
    (comp (ref R202)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F970))
    (comp (ref R201)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A2FE363))
    (comp (ref R302)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 59C4F970))
    (comp (ref R301)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A2FE363))
    (comp (ref R402)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 59C4F970))
    (comp (ref R401)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A2FE363))
    (comp (ref R502)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 59C4F970))
    (comp (ref R501)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A2FE363))
    (comp (ref U601)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 59C4F962))
    (comp (ref R602)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 59C4F970))
    (comp (ref R601)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 5A2FE363))
    (comp (ref R702)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 59C4F970))
    (comp (ref R701)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 5A2FE363))
    (comp (ref R802)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 59C4F970))
    (comp (ref R801)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 5A2FE363))
    (comp (ref R902)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 59C4F970))
    (comp (ref R901)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 5A2FE363)))
  (libparts
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib linear) (part LM2902)
      (aliases
        (alias LM324)
        (alias TLC274)
        (alias TLC279)
        (alias TL074)
        (alias LM324A)
        (alias MCP6004)
        (alias TL084)
        (alias TL064)
        (alias LMV324)
        (alias LMC6484)
        (alias MCP604)
        (alias MC33079)
        (alias MC33179)
        (alias OPA4134)
        (alias OPA4340UA)
        (alias OPA4376)
        (alias MCP6L94)
        (alias TSV914)
        (alias ADA4807-4))
      (description "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14")
      (docs http://www.ti.com/lit/ds/symlink/lm2902-n.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*Pitch1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*Pitch0.65mm*)
        (fp SSOP*5.3x6.2mm*Pitch0.65mm*)
        (fp MSOP*3x3mm*Pitch0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2902))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part TC4051BP)
      (description "Analog Multiplexer 8 to 1 lins")
      (fields
        (field (name Reference) U)
        (field (name Value) TC4051BP))
      (pins
        (pin (num 1) (name X4) (type passive))
        (pin (num 2) (name X6) (type passive))
        (pin (num 3) (name X) (type passive))
        (pin (num 4) (name X7) (type passive))
        (pin (num 5) (name X5) (type passive))
        (pin (num 6) (name Inh) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name C) (type input))
        (pin (num 10) (name B) (type input))
        (pin (num 11) (name A) (type input))
        (pin (num 12) (name X3) (type passive))
        (pin (num 13) (name X0) (type passive))
        (pin (num 14) (name X1) (type passive))
        (pin (num 15) (name X2) (type passive))
        (pin (num 16) (name VDD) (type power_in)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical linear)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\linear.lib")))
  (nets
    (net (code 1) (name "Net-(F102-Pad2)")
      (node (ref F102) (pin 2))
      (node (ref J103) (pin 1)))
    (net (code 2) (name "Net-(F106-Pad2)")
      (node (ref F106) (pin 2))
      (node (ref J112) (pin 1)))
    (net (code 3) (name "Net-(F107-Pad2)")
      (node (ref F107) (pin 2))
      (node (ref J113) (pin 1)))
    (net (code 4) (name "Net-(F108-Pad2)")
      (node (ref F108) (pin 2))
      (node (ref J114) (pin 1)))
    (net (code 5) (name "Net-(F103-Pad2)")
      (node (ref J104) (pin 1))
      (node (ref F103) (pin 2)))
    (net (code 6) (name "Net-(F104-Pad2)")
      (node (ref J105) (pin 1))
      (node (ref F104) (pin 2)))
    (net (code 7) (name "Net-(F105-Pad2)")
      (node (ref F105) (pin 2))
      (node (ref J111) (pin 1)))
    (net (code 8) (name /VoltMeter7/+VE)
      (node (ref U601) (pin 13))
      (node (ref J117) (pin 1))
      (node (ref R802) (pin 2))
      (node (ref R701) (pin 1))
      (node (ref F107) (pin 1)))
    (net (code 9) (name /VoltMeter6/+VE)
      (node (ref J116) (pin 1))
      (node (ref R801) (pin 1))
      (node (ref U601) (pin 9))
      (node (ref R902) (pin 2))
      (node (ref F106) (pin 1)))
    (net (code 10) (name /VoltMeter4/+VE)
      (node (ref R302) (pin 2))
      (node (ref J109) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref U201) (pin 2))
      (node (ref F104) (pin 1)))
    (net (code 11) (name /VoltMeter3/+VE)
      (node (ref R301) (pin 1))
      (node (ref R402) (pin 2))
      (node (ref U201) (pin 13))
      (node (ref J108) (pin 1))
      (node (ref F103) (pin 1)))
    (net (code 12) (name V4)
      (node (ref U101) (pin 12))
      (node (ref U201) (pin 7)))
    (net (code 13) (name V5)
      (node (ref U101) (pin 1))
      (node (ref U601) (pin 8)))
    (net (code 14) (name COM)
      (node (ref U101) (pin 3))
      (node (ref J110) (pin 8)))
    (net (code 15) (name V6)
      (node (ref U601) (pin 14))
      (node (ref U101) (pin 5)))
    (net (code 16) (name C)
      (node (ref J110) (pin 6))
      (node (ref U101) (pin 9)))
    (net (code 17) (name B)
      (node (ref U101) (pin 10))
      (node (ref J110) (pin 4)))
    (net (code 18) (name A)
      (node (ref J110) (pin 2))
      (node (ref U101) (pin 11)))
    (net (code 19) (name ARD_5V)
      (node (ref U201) (pin 4))
      (node (ref U601) (pin 4))
      (node (ref J110) (pin 3))
      (node (ref U101) (pin 16)))
    (net (code 20) (name ARD_GND)
      (node (ref U101) (pin 8))
      (node (ref U101) (pin 6))
      (node (ref J110) (pin 1))
      (node (ref U101) (pin 7))
      (node (ref U601) (pin 11))
      (node (ref U201) (pin 11)))
    (net (code 21) (name /VoltMeter2/+VE)
      (node (ref R401) (pin 1))
      (node (ref R502) (pin 2))
      (node (ref F102) (pin 1))
      (node (ref J107) (pin 1))
      (node (ref U201) (pin 9)))
    (net (code 22) (name /VoltMeter5/+VE)
      (node (ref F105) (pin 1))
      (node (ref U201) (pin 6))
      (node (ref R202) (pin 2))
      (node (ref J115) (pin 1))
      (node (ref R901) (pin 1)))
    (net (code 23) (name /VoltMeter8/-VE)
      (node (ref U601) (pin 6))
      (node (ref R602) (pin 2))
      (node (ref J123) (pin 1)))
    (net (code 24) (name V3)
      (node (ref U101) (pin 15))
      (node (ref U201) (pin 1)))
    (net (code 25) (name V2)
      (node (ref U101) (pin 14))
      (node (ref U201) (pin 14)))
    (net (code 26) (name /VoltMeter1/+VE)
      (node (ref R501) (pin 1))
      (node (ref J106) (pin 1))
      (node (ref F101) (pin 1)))
    (net (code 27) (name V1)
      (node (ref U101) (pin 13))
      (node (ref U201) (pin 8)))
    (net (code 28) (name /VoltMeter8/+VE)
      (node (ref R702) (pin 2))
      (node (ref J118) (pin 1))
      (node (ref U601) (pin 2))
      (node (ref F108) (pin 1))
      (node (ref R601) (pin 1)))
    (net (code 29) (name V8)
      (node (ref U101) (pin 4))
      (node (ref U601) (pin 7)))
    (net (code 30) (name V7)
      (node (ref U101) (pin 2))
      (node (ref U601) (pin 1)))
    (net (code 31) (name "Net-(J110-Pad5)")
      (node (ref J110) (pin 5)))
    (net (code 32) (name "Net-(J110-Pad7)")
      (node (ref J110) (pin 7)))
    (net (code 33) (name "Net-(F101-Pad2)")
      (node (ref J102) (pin 1))
      (node (ref F101) (pin 2)))
    (net (code 34) (name "Net-(R201-Pad2)")
      (node (ref R202) (pin 1))
      (node (ref U201) (pin 5))
      (node (ref R201) (pin 2)))
    (net (code 35) (name "Net-(R301-Pad2)")
      (node (ref R301) (pin 2))
      (node (ref R302) (pin 1))
      (node (ref U201) (pin 3)))
    (net (code 36) (name "Net-(R401-Pad2)")
      (node (ref R401) (pin 2))
      (node (ref U201) (pin 12))
      (node (ref R402) (pin 1)))
    (net (code 37) (name "Net-(R501-Pad2)")
      (node (ref R501) (pin 2))
      (node (ref U201) (pin 10))
      (node (ref R502) (pin 1)))
    (net (code 38) (name "Net-(R601-Pad2)")
      (node (ref U601) (pin 5))
      (node (ref R602) (pin 1))
      (node (ref R601) (pin 2)))
    (net (code 39) (name "Net-(R701-Pad2)")
      (node (ref R701) (pin 2))
      (node (ref U601) (pin 3))
      (node (ref R702) (pin 1)))
    (net (code 40) (name "Net-(R801-Pad2)")
      (node (ref R802) (pin 1))
      (node (ref U601) (pin 12))
      (node (ref R801) (pin 2)))
    (net (code 41) (name "Net-(R901-Pad2)")
      (node (ref U601) (pin 10))
      (node (ref R902) (pin 1))
      (node (ref R901) (pin 2)))))