(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/HBridgePowerModule/HBridgePowerModule.sch)
    (date "14/12/2017 13:52:26")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Rev 3")
        (date 2017-12-06)
        (source HBridgePowerModule.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "For approval by Mansour"))))
    (sheet (number 2) (name "/SinglePowerSwitch 1/") (tstamps /59AEDD49/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AED755))
    (comp (ref J6)
      (value AC_OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AEFF90))
    (comp (ref J7)
      (value AC_OUT)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AFA697))
    (comp (ref J2)
      (value POS_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A28227C))
    (comp (ref J3)
      (value NEG_IN)
      (footprint PartsLibraries:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A28246C))
    (comp (ref IC101)
      (value CAS_50-NP)
      (footprint CAS_NP)
      (datasheet http://www.lem.com/docs/products/lts_15-np.pdf)
      (libsource (lib OAE.Parts) (part CAS_50-NP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A344E30))
    (comp (ref J101)
      (value Conn_01x03)
      (footprint Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A34A7A6))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE014))
    (comp (ref C1)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE01D))
    (comp (ref Q2)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE014))
    (comp (ref C2)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE01D))
    (comp (ref Q3)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE014))
    (comp (ref C3)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE01D))
    (comp (ref Q4)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE014))
    (comp (ref C4)
      (value C)
      (footprint PartsLibraries:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE01D)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part CAS_50-NP)
      (description "LEM Closed Loop Current Sensor, 50A Nominal")
      (docs http://www.lem.com/docs/marketing/LEM%20Leaflet%20CAS%20CASR%20CKSR.pdf)
      (footprints
        (fp CAS_NP))
      (fields
        (field (name Reference) IC)
        (field (name Value) CAS_50-NP)
        (field (name Footprint) CAS_NP)
        (field (name Datasheet) http://www.lem.com/docs/products/lts_15-np.pdf))
      (pins
        (pin (num 1) (name "IN(1)") (type unspc))
        (pin (num 2) (name "IN(2)") (type unspc))
        (pin (num 3) (name "IN(3)") (type unspc))
        (pin (num 8) (name "OUT(3)") (type unspc))
        (pin (num 9) (name "OUT(2)") (type unspc))
        (pin (num 10) (name "OUT(3)") (type unspc))
        (pin (num 11) (name Vout) (type unspc))
        (pin (num 12) (name GND) (type unspc))
        (pin (num 13) (name +5V) (type unspc))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib conn) (part Conn_01x03)
      (description "Generic connector, single row, 01x03")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib OAE.Parts) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name ARD_GND)
      (node (ref IC101) (pin 12))
      (node (ref J101) (pin 2)))
    (net (code 2) (name ARD_CUR)
      (node (ref IC101) (pin 11))
      (node (ref J101) (pin 1)))
    (net (code 3) (name "/SinglePowerSwitch 1/DRAIN")
      (node (ref C1) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref IC101) (pin 10))
      (node (ref C2) (pin 2))
      (node (ref IC101) (pin 9))
      (node (ref Q2) (pin 2))
      (node (ref IC101) (pin 8)))
    (net (code 4) (name "Net-(IC101-Pad1)")
      (node (ref IC101) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref IC101) (pin 3))
      (node (ref IC101) (pin 1)))
    (net (code 5) (name ARD_5V)
      (node (ref IC101) (pin 13))
      (node (ref J101) (pin 3)))
    (net (code 6) (name DRV_GATE_1)
      (node (ref J1) (pin 7))
      (node (ref Q1) (pin 1)))
    (net (code 7) (name DRV_GATE_2)
      (node (ref Q2) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 8) (name GND_ISO_1)
      (node (ref Q1) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref Q3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 5))
      (node (ref J6) (pin 1)))
    (net (code 9) (name DRV_GATE_3)
      (node (ref J1) (pin 3))
      (node (ref Q3) (pin 1)))
    (net (code 10) (name DRV_GATE_4)
      (node (ref J1) (pin 2))
      (node (ref Q4) (pin 1)))
    (net (code 11) (name GND_ISO_3)
      (node (ref J1) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref Q4) (pin 3))
      (node (ref J3) (pin 1))
      (node (ref J1) (pin 4)))
    (net (code 12) (name GND_ISO_2)
      (node (ref C4) (pin 2))
      (node (ref J1) (pin 8))
      (node (ref J7) (pin 1))
      (node (ref Q4) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref C2) (pin 1)))
    (net (code 13) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 14) (name "Net-(Q2-Pad4)")
      (node (ref Q2) (pin 4)))
    (net (code 15) (name "Net-(Q3-Pad4)")
      (node (ref Q3) (pin 4)))
    (net (code 16) (name "Net-(Q4-Pad4)")
      (node (ref Q4) (pin 4)))))