(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/FuseBoard/Fuseboard.sch)
    (date "04/01/2018 14:44:01")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source Fuseboard.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /VoltMeter4/) (tstamps /59C4F642/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /VoltMeter3/) (tstamps /59C51A28/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /VoltMeter2/) (tstamps /59C51FF6/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /VoltMeter1/) (tstamps /59C5216A/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /VoltMeter8/) (tstamps /59C53BAD/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /VoltMeter7/) (tstamps /59C53BBB/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /VoltMeter6/) (tstamps /59C53BC9/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /VoltMeter5/) (tstamps /59C53BD7/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.1a")
        (date 2018-01-04)
        (source VoltMeter.sch)
        (comment (number 1) (value "APPROVED for Prototype"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J110)
      (value RJ45)
      (footprint PartsLibraries:RJ45)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3DA36))
    (comp (ref F101)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A311AB6))
    (comp (ref F102)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314BDF))
    (comp (ref F103)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31508D))
    (comp (ref F104)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A316DCF))
    (comp (ref F105)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A319EA5))
    (comp (ref F106)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B529))
    (comp (ref F107)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B608))
    (comp (ref F108)
      (value Fuse)
      (footprint PartsLibraries:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B6ED))
    (comp (ref J123)
      (value FB_OUT)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3187AF))
    (comp (ref U101)
      (value TC4051BP)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib OAE.Parts) (part TC4051BP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B088))
    (comp (ref J101)
      (value FB_IN)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4D601D))
    (comp (ref U201)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F962))
    (comp (ref R202)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F970))
    (comp (ref R201)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A2FE363))
    (comp (ref C201)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A7FE3))
    (comp (ref R203)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A8016))
    (comp (ref R302)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 59C4F970))
    (comp (ref R301)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A2FE363))
    (comp (ref C301)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A7FE3))
    (comp (ref R303)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A8016))
    (comp (ref R402)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 59C4F970))
    (comp (ref R401)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A2FE363))
    (comp (ref C401)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A7FE3))
    (comp (ref R403)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A8016))
    (comp (ref R502)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 59C4F970))
    (comp (ref R501)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A2FE363))
    (comp (ref C501)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A7FE3))
    (comp (ref R503)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A8016))
    (comp (ref U601)
      (value MCP604)
      (footprint Housings_DIP:DIP-14_W7.62mm)
      (libsource (lib linear) (part MCP604))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 59C4F962))
    (comp (ref R602)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 59C4F970))
    (comp (ref R601)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 5A2FE363))
    (comp (ref C601)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 5A3A7FE3))
    (comp (ref R603)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter8/) (tstamps /59C53BAD/))
      (tstamp 5A3A8016))
    (comp (ref R702)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 59C4F970))
    (comp (ref R701)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 5A2FE363))
    (comp (ref C701)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 5A3A7FE3))
    (comp (ref R703)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter7/) (tstamps /59C53BBB/))
      (tstamp 5A3A8016))
    (comp (ref R802)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 59C4F970))
    (comp (ref R801)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 5A2FE363))
    (comp (ref C801)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 5A3A7FE3))
    (comp (ref R803)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter6/) (tstamps /59C53BC9/))
      (tstamp 5A3A8016))
    (comp (ref R902)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 59C4F970))
    (comp (ref R901)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 5A2FE363))
    (comp (ref C901)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 5A3A7FE3))
    (comp (ref R903)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter5/) (tstamps /59C53BD7/))
      (tstamp 5A3A8016)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib linear) (part LM2902)
      (aliases
        (alias LM324)
        (alias TLC274)
        (alias TLC279)
        (alias TL074)
        (alias LM324A)
        (alias MCP6004)
        (alias TL084)
        (alias TL064)
        (alias LMV324)
        (alias LMC6484)
        (alias MCP604)
        (alias MC33079)
        (alias MC33179)
        (alias OPA4134)
        (alias OPA4340UA)
        (alias OPA4376)
        (alias MCP6L94)
        (alias TSV914)
        (alias ADA4807-4))
      (description "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14")
      (docs http://www.ti.com/lit/ds/symlink/lm2902-n.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*Pitch1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*Pitch0.65mm*)
        (fp SSOP*5.3x6.2mm*Pitch0.65mm*)
        (fp MSOP*3x3mm*Pitch0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2902))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part TC4051BP)
      (description "Analog Multiplexer 8 to 1 lins")
      (fields
        (field (name Reference) U)
        (field (name Value) TC4051BP))
      (pins
        (pin (num 1) (name X4) (type passive))
        (pin (num 2) (name X6) (type passive))
        (pin (num 3) (name X) (type passive))
        (pin (num 4) (name X7) (type passive))
        (pin (num 5) (name X5) (type passive))
        (pin (num 6) (name Inh) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name C) (type input))
        (pin (num 10) (name B) (type input))
        (pin (num 11) (name A) (type input))
        (pin (num 12) (name X3) (type passive))
        (pin (num 13) (name X0) (type passive))
        (pin (num 14) (name X1) (type passive))
        (pin (num 15) (name X2) (type passive))
        (pin (num 16) (name VDD) (type power_in)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical linear)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\linear.lib"))
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name /VoltMeter5/+VE)
      (node (ref F105) (pin 1))
      (node (ref U201) (pin 6))
      (node (ref R202) (pin 2))
      (node (ref R901) (pin 1)))
    (net (code 2) (name /VoltMeter6/+VE)
      (node (ref F106) (pin 1))
      (node (ref R801) (pin 1))
      (node (ref U601) (pin 9))
      (node (ref R902) (pin 2)))
    (net (code 3) (name /VoltMeter7/+VE)
      (node (ref R701) (pin 1))
      (node (ref U601) (pin 13))
      (node (ref F107) (pin 1))
      (node (ref R802) (pin 2)))
    (net (code 4) (name /VoltMeter8/+VE)
      (node (ref F108) (pin 1))
      (node (ref R601) (pin 1))
      (node (ref U601) (pin 2))
      (node (ref R702) (pin 2)))
    (net (code 5) (name /VoltMeter8/-VE)
      (node (ref U601) (pin 6))
      (node (ref R602) (pin 2))
      (node (ref J123) (pin 1)))
    (net (code 6) (name A)
      (node (ref J110) (pin 2))
      (node (ref U101) (pin 11)))
    (net (code 7) (name V5)
      (node (ref C901) (pin 1))
      (node (ref U101) (pin 1))
      (node (ref U601) (pin 8))
      (node (ref R903) (pin 1)))
    (net (code 8) (name ARD_VSS)
      (node (ref U101) (pin 16)))
    (net (code 9) (name V7)
      (node (ref U601) (pin 1))
      (node (ref C701) (pin 1))
      (node (ref R703) (pin 1))
      (node (ref U101) (pin 2)))
    (net (code 10) (name COM)
      (node (ref U101) (pin 3))
      (node (ref J110) (pin 8)))
    (net (code 11) (name V6)
      (node (ref C801) (pin 1))
      (node (ref R803) (pin 1))
      (node (ref U601) (pin 14))
      (node (ref U101) (pin 5)))
    (net (code 12) (name ARD_GND)
      (node (ref C301) (pin 2))
      (node (ref C401) (pin 2))
      (node (ref C701) (pin 2))
      (node (ref R403) (pin 2))
      (node (ref R703) (pin 2))
      (node (ref C601) (pin 2))
      (node (ref U201) (pin 11))
      (node (ref R503) (pin 2))
      (node (ref C501) (pin 2))
      (node (ref R603) (pin 2))
      (node (ref R303) (pin 2))
      (node (ref C801) (pin 2))
      (node (ref R803) (pin 2))
      (node (ref R903) (pin 2))
      (node (ref J110) (pin 1))
      (node (ref U101) (pin 7))
      (node (ref U101) (pin 6))
      (node (ref C901) (pin 2))
      (node (ref U101) (pin 8))
      (node (ref U601) (pin 11))
      (node (ref R203) (pin 2))
      (node (ref C201) (pin 2)))
    (net (code 13) (name C)
      (node (ref U101) (pin 9))
      (node (ref J110) (pin 6)))
    (net (code 14) (name B)
      (node (ref U101) (pin 10))
      (node (ref J110) (pin 4)))
    (net (code 15) (name V4)
      (node (ref U101) (pin 12))
      (node (ref U201) (pin 7))
      (node (ref R203) (pin 1))
      (node (ref C201) (pin 1)))
    (net (code 16) (name V3)
      (node (ref U101) (pin 15))
      (node (ref U201) (pin 1))
      (node (ref R303) (pin 1))
      (node (ref C301) (pin 1)))
    (net (code 17) (name V2)
      (node (ref U101) (pin 14))
      (node (ref C401) (pin 1))
      (node (ref R403) (pin 1))
      (node (ref U201) (pin 14)))
    (net (code 18) (name V1)
      (node (ref R503) (pin 1))
      (node (ref C501) (pin 1))
      (node (ref U101) (pin 13))
      (node (ref U201) (pin 8)))
    (net (code 19) (name V8)
      (node (ref U101) (pin 4))
      (node (ref U601) (pin 7))
      (node (ref R603) (pin 1))
      (node (ref C601) (pin 1)))
    (net (code 20) (name ARD_VDD)
      (node (ref J110) (pin 3))
      (node (ref U201) (pin 4))
      (node (ref U601) (pin 4)))
    (net (code 21) (name "Net-(J110-Pad5)")
      (node (ref J110) (pin 5)))
    (net (code 22) (name "Net-(J110-Pad7)")
      (node (ref J110) (pin 7)))
    (net (code 23) (name /VoltMeter4/+VE)
      (node (ref F104) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref R302) (pin 2))
      (node (ref U201) (pin 2)))
    (net (code 24) (name "Net-(F105-Pad2)")
      (node (ref F105) (pin 2)))
    (net (code 25) (name "Net-(F106-Pad2)")
      (node (ref F106) (pin 2)))
    (net (code 26) (name "Net-(F107-Pad2)")
      (node (ref F107) (pin 2)))
    (net (code 27) (name "Net-(F108-Pad2)")
      (node (ref F108) (pin 2)))
    (net (code 28) (name /VoltMeter3/+VE)
      (node (ref F103) (pin 1))
      (node (ref U201) (pin 13))
      (node (ref R402) (pin 2))
      (node (ref R301) (pin 1)))
    (net (code 29) (name /VoltMeter2/+VE)
      (node (ref R502) (pin 2))
      (node (ref R401) (pin 1))
      (node (ref U201) (pin 9))
      (node (ref F102) (pin 1)))
    (net (code 30) (name /VoltMeter1/+VE)
      (node (ref R501) (pin 1))
      (node (ref J101) (pin 1))
      (node (ref F101) (pin 1)))
    (net (code 31) (name "Net-(F104-Pad2)")
      (node (ref F104) (pin 2)))
    (net (code 32) (name "Net-(F101-Pad2)")
      (node (ref F101) (pin 2)))
    (net (code 33) (name "Net-(F102-Pad2)")
      (node (ref F102) (pin 2)))
    (net (code 34) (name "Net-(F103-Pad2)")
      (node (ref F103) (pin 2)))
    (net (code 35) (name "Net-(R201-Pad2)")
      (node (ref R201) (pin 2))
      (node (ref U201) (pin 5))
      (node (ref R202) (pin 1)))
    (net (code 36) (name "Net-(R301-Pad2)")
      (node (ref R301) (pin 2))
      (node (ref U201) (pin 3))
      (node (ref R302) (pin 1)))
    (net (code 37) (name "Net-(R401-Pad2)")
      (node (ref R401) (pin 2))
      (node (ref U201) (pin 12))
      (node (ref R402) (pin 1)))
    (net (code 38) (name "Net-(R501-Pad2)")
      (node (ref R502) (pin 1))
      (node (ref R501) (pin 2))
      (node (ref U201) (pin 10)))
    (net (code 39) (name "Net-(R601-Pad2)")
      (node (ref R601) (pin 2))
      (node (ref R602) (pin 1))
      (node (ref U601) (pin 5)))
    (net (code 40) (name "Net-(R701-Pad2)")
      (node (ref U601) (pin 3))
      (node (ref R702) (pin 1))
      (node (ref R701) (pin 2)))
    (net (code 41) (name "Net-(R801-Pad2)")
      (node (ref U601) (pin 12))
      (node (ref R801) (pin 2))
      (node (ref R802) (pin 1)))
    (net (code 42) (name "Net-(R901-Pad2)")
      (node (ref R902) (pin 1))
      (node (ref U601) (pin 10))
      (node (ref R901) (pin 2)))))