(export (version D)
  (design
    (source C:\Development\mlihardware\MLI\Modular\PsuSwitchModule\PsuSwitchModule.sch)
    (date "04/02/2020 15:44:09")
    (tool "Eeschema (5.1.2)-2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-03-13)
        (source PsuSwitchModule.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-03-13)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-03-13)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /PsuSwitchModule.Switch.3/) (tstamps /59A71299/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-03-13)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/)
      (title_block
        (title "Power Module (Control Board)")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-03-13)
        (source PsuSwitchModule.Switch.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Monitor)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45) (description "RJ45 connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59526541))
    (comp (ref J2)
      (value "Temperature Probe LM35")
      (footprint Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF2))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 599EAAF9))
    (comp (ref J101)
      (value "Current Sensor")
      (footprint Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3469C9))
    (comp (ref J102)
      (value Earth)
      (footprint OAE_Parts:PowerConnectorRound_M3)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABCCEE9))
    (comp (ref J7)
      (value Control)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45) (description "RJ45 connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59A7EBD8))
    (comp (ref IC1)
      (value TC4421CPA)
      (footprint OAE_Parts:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4421CPA Low Side MOSFET Power Driver, 9A, 4.5 → 18 V, PDIP 8-Pin")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4421CPA)
        (field (name "RS Part Number") 207-0146)
        (field (name Supplier_Name) RS))
      (libsource (lib PsuSwitchModule-rescue) (part TC4422AVPA) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59498139))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5949814D))
    (comp (ref R2)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DA9F))
    (comp (ref U2)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAA6))
    (comp (ref D1)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part D_Zener) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0E59))
    (comp (ref C17)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0ED7))
    (comp (ref R10)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF0FC7))
    (comp (ref R11)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1A58))
    (comp (ref C25)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5A16CD08))
    (comp (ref D201)
      (value D_Zener_x2_KCom_AKA)
      (footprint OAE_Parts:SOT-23_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Zener_x2_ACom_KAK) (description "Dual Zener diode, common anode on pin 2"))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5E39B85D))
    (comp (ref R202)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5E3A5524))
    (comp (ref R201)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5E3A1E35))
    (comp (ref U201)
      (value NME1215DC)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib OAE.Parts) (part NME1215DC) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5E39E16E))
    (comp (ref J201)
      (value Conn_01x03_Male)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03_Male) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 5AA809BD))
    (comp (ref C18)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59EF1DD4))
    (comp (ref R3)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6DAAD))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3E0))
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part CP) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.1/) (tstamps /59498AA5/))
      (tstamp 59A6D3D9))
    (comp (ref IC2)
      (value TC4421CPA)
      (footprint OAE_Parts:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4421CPA Low Side MOSFET Power Driver, 9A, 4.5 → 18 V, PDIP 8-Pin")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4421CPA)
        (field (name "RS Part Number") 207-0146)
        (field (name Supplier_Name) RS))
      (libsource (lib PsuSwitchModule-rescue) (part TC4422AVPA) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59498139))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5949814D))
    (comp (ref R4)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DA9F))
    (comp (ref U4)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAA6))
    (comp (ref D2)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part D_Zener) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0E59))
    (comp (ref C19)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0ED7))
    (comp (ref R12)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF0FC7))
    (comp (ref R13)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1A58))
    (comp (ref C26)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5A16CD08))
    (comp (ref D301)
      (value D_Zener_x2_KCom_AKA)
      (footprint OAE_Parts:SOT-23_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Zener_x2_ACom_KAK) (description "Dual Zener diode, common anode on pin 2"))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5E39B85D))
    (comp (ref R302)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5E3A5524))
    (comp (ref R301)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5E3A1E35))
    (comp (ref U301)
      (value NME1215DC)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib OAE.Parts) (part NME1215DC) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5E39E16E))
    (comp (ref J301)
      (value Conn_01x03_Male)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03_Male) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 5AA809BD))
    (comp (ref C20)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59EF1DD4))
    (comp (ref R5)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6DAAD))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3E0))
    (comp (ref C5)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part CP) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.2/) (tstamps /59A7109E/))
      (tstamp 59A6D3D9))
    (comp (ref IC3)
      (value TC4421CPA)
      (footprint OAE_Parts:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4421CPA Low Side MOSFET Power Driver, 9A, 4.5 → 18 V, PDIP 8-Pin")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4421CPA)
        (field (name "RS Part Number") 207-0146)
        (field (name Supplier_Name) RS))
      (libsource (lib PsuSwitchModule-rescue) (part TC4422AVPA) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59498139))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5949814D))
    (comp (ref R6)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DA9F))
    (comp (ref U6)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAA6))
    (comp (ref D3)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part D_Zener) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0E59))
    (comp (ref C21)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0ED7))
    (comp (ref R14)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF0FC7))
    (comp (ref R15)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1A58))
    (comp (ref C27)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5A16CD08))
    (comp (ref D401)
      (value D_Zener_x2_KCom_AKA)
      (footprint OAE_Parts:SOT-23_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Zener_x2_ACom_KAK) (description "Dual Zener diode, common anode on pin 2"))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5E39B85D))
    (comp (ref R402)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5E3A5524))
    (comp (ref R401)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5E3A1E35))
    (comp (ref U401)
      (value NME1215DC)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib OAE.Parts) (part NME1215DC) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5E39E16E))
    (comp (ref J401)
      (value Conn_01x03_Male)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03_Male) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 5AA809BD))
    (comp (ref C22)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59EF1DD4))
    (comp (ref R7)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6DAAD))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3E0))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part CP) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.3/) (tstamps /59A71299/))
      (tstamp 59A6D3D9))
    (comp (ref IC4)
      (value TC4421CPA)
      (footprint OAE_Parts:TC4422AVPA)
      (fields
        (field (name Description) "Microchip TC4421CPA Low Side MOSFET Power Driver, 9A, 4.5 → 18 V, PDIP 8-Pin")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4421CPA)
        (field (name "RS Part Number") 207-0146)
        (field (name Supplier_Name) RS))
      (libsource (lib PsuSwitchModule-rescue) (part TC4422AVPA) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59498139))
    (comp (ref C15)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5949814D))
    (comp (ref R8)
      (value 180)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DA9F))
    (comp (ref U8)
      (value H11N1M)
      (footprint Housings_DIP:DIP-6_W7.62mm)
      (libsource (lib OAE.Parts) (part H11N1M) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAA6))
    (comp (ref D4)
      (value D_Zener)
      (footprint Diodes_THT:D_T-1_P5.08mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part D_Zener) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0E59))
    (comp (ref C23)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0ED7))
    (comp (ref R16)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF0FC7))
    (comp (ref R17)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1A58))
    (comp (ref C28)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5A16CD08))
    (comp (ref D501)
      (value D_Zener_x2_KCom_AKA)
      (footprint OAE_Parts:SOT-23_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Zener_x2_ACom_KAK) (description "Dual Zener diode, common anode on pin 2"))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5E39B85D))
    (comp (ref R502)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5E3A5524))
    (comp (ref R501)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5E3A1E35))
    (comp (ref U501)
      (value NME1215DC)
      (footprint Housings_DIP:DIP-14_W7.62mm_Socket)
      (libsource (lib OAE.Parts) (part NME1215DC) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5E39E16E))
    (comp (ref J501)
      (value Conn_01x03_Male)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib PsuSwitchModule-rescue) (part Conn_01x03_Male) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 5AA809BD))
    (comp (ref C24)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59EF1DD4))
    (comp (ref R9)
      (value 3K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib PsuSwitchModule-rescue) (part R) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6DAAD))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part C) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3E0))
    (comp (ref C13)
      (value 4.7uF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib PsuSwitchModule-rescue) (part CP) (description ""))
      (sheetpath (names /PsuSwitchModule.Switch.4/) (tstamps /59A712A3/))
      (tstamp 59A6D3D9)))
  (libparts
    (libpart (lib Device) (part D_Zener_x2_ACom_KAK)
      (description "Dual Zener diode, common anode on pin 2")
      (docs ~)
      (footprints
        (fp SOT*)
        (fp SC*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener_x2_ACom_KAK))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))
        (pin (num 3) (name K) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part H11N1M)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) H11N1M)
        (field (name Footprint) Housings_DIP:DIP-6_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1215DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1215DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 3) (name +Vout) (type output))
        (pin (num 8) (name 0V) (type output))
        (pin (num 11) (name -Vout) (type output))
        (pin (num 14) (name +Vin) (type input))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name Earth) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part C)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part Conn_01x01)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part Conn_01x03)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part Conn_01x03_Male)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part D_Zener)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib PsuSwitchModule-rescue) (part TC4422AVPA)
      (fields
        (field (name Reference) IC)
        (field (name Value) TC4422AVPA)
        (field (name Footprint) DIP254P762X432-8)
        (field (name Description) "Microchip TC4422AVPA, MOSFET Power Driver 10A, 4.5  18 V, Non-Inverting, 8-Pin PDIP")
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) TC4422AVPA)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 7747668))
      (pins
        (pin (num 1) (name VDD_2) (type unspc))
        (pin (num 2) (name INPUT) (type unspc))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND_2) (type unspc))
        (pin (num 5) (name GND) (type unspc))
        (pin (num 6) (name ~OUTPUT_2) (type unspc))
        (pin (num 7) (name ~OUTPUT) (type unspc))
        (pin (num 8) (name VDD) (type unspc)))))
  (libraries
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical OAE.Parts)
      (uri C:/Development/mlihardware/oae_parts/OAE.Parts.lib))
    (library (logical PsuSwitchModule-rescue)
      (uri C:\Development\mlihardware\MLI\Modular\PsuSwitchModule/PsuSwitchModule-rescue.lib)))
  (nets
    (net (code 1) (name ARD_GND)
      (node (ref J7) (pin 7))
      (node (ref J7) (pin 5))
      (node (ref J7) (pin 3))
      (node (ref U2) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 8))
      (node (ref J101) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 2) (name ARD_CUR)
      (node (ref J1) (pin 1))
      (node (ref J101) (pin 1)))
    (net (code 3) (name ARD_PWM_A)
      (node (ref J7) (pin 8))
      (node (ref C25) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 4) (name ARD_PWM_B)
      (node (ref R4) (pin 1))
      (node (ref C26) (pin 2))
      (node (ref J7) (pin 6)))
    (net (code 5) (name ARD_PWM_C)
      (node (ref R6) (pin 1))
      (node (ref C27) (pin 2))
      (node (ref J7) (pin 2)))
    (net (code 6) (name Earth)
      (node (ref J501) (pin 1))
      (node (ref J201) (pin 1))
      (node (ref J401) (pin 1))
      (node (ref J1) (pin 9))
      (node (ref J102) (pin 1))
      (node (ref J301) (pin 1))
      (node (ref J7) (pin 9)))
    (net (code 7) (name DC_IN)
      (node (ref U401) (pin 14))
      (node (ref U301) (pin 14))
      (node (ref U501) (pin 14))
      (node (ref U201) (pin 14))
      (node (ref J1) (pin 4)))
    (net (code 8) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref R1) (pin 1)))
    (net (code 9) (name ARD_VCC)
      (node (ref J101) (pin 3))
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 1)))
    (net (code 10) (name ARD_TEMP)
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 6)))
    (net (code 11) (name DC_GND)
      (node (ref U501) (pin 1))
      (node (ref U301) (pin 1))
      (node (ref U401) (pin 1))
      (node (ref J1) (pin 5))
      (node (ref U201) (pin 1)))
    (net (code 12) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 13) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 14) (name ARD_PWM_D)
      (node (ref C28) (pin 2))
      (node (ref J7) (pin 4))
      (node (ref R8) (pin 1)))
    (net (code 15) (name /PsuSwitchModule.Switch.1/-15V)
      (node (ref U201) (pin 11)))
    (net (code 16) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref U201) (pin 8)))
    (net (code 17) (name /PsuSwitchModule.Switch.1/DRV_SIG)
      (node (ref J201) (pin 2)))
    (net (code 18) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref D201) (pin 1)))
    (net (code 19) (name "Net-(D201-Pad2)")
      (node (ref D201) (pin 2)))
    (net (code 20) (name /PsuSwitchModule.Switch.1/-5V)
      (node (ref R202) (pin 1))
      (node (ref R201) (pin 2))
      (node (ref J201) (pin 3)))
    (net (code 21) (name /PsuSwitchModule.Switch.1/-15V)
      (node (ref R202) (pin 2)))
    (net (code 22) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref C1) (pin 2)))
    (net (code 23) (name /PsuSwitchModule.Switch.1/+15V)
      (node (ref C2) (pin 1))
      (node (ref IC1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref U201) (pin 3))
      (node (ref IC1) (pin 8)))
    (net (code 24) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref C2) (pin 2)))
    (net (code 25) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref C18) (pin 2)))
    (net (code 26) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 27) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref C3) (pin 1)))
    (net (code 28) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref IC1) (pin 5)))
    (net (code 29) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref IC1) (pin 4)))
    (net (code 30) (name "Net-(IC1-Pad3)")
      (node (ref IC1) (pin 3)))
    (net (code 31) (name "Net-(C25-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref C25) (pin 1)))
    (net (code 32) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref U2) (pin 5))
      (node (ref D1) (pin 2))
      (node (ref C17) (pin 2)))
    (net (code 33) (name "Net-(C17-Pad1)")
      (node (ref U2) (pin 6))
      (node (ref R10) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 34) (name "Net-(IC1-Pad2)")
      (node (ref IC1) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref R10) (pin 2)))
    (net (code 35) (name /PsuSwitchModule.Switch.1/DRV_SIG)
      (node (ref IC1) (pin 6))
      (node (ref IC1) (pin 7))
      (node (ref C3) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref D201) (pin 3)))
    (net (code 36) (name /PsuSwitchModule.Switch.1/GND_ISO)
      (node (ref R11) (pin 2)))
    (net (code 37) (name /PsuSwitchModule.Switch.2/-15V)
      (node (ref U301) (pin 11)))
    (net (code 38) (name /PsuSwitchModule.Switch.2/DRV_SIG)
      (node (ref J301) (pin 2)))
    (net (code 39) (name /PsuSwitchModule.Switch.2/-15V)
      (node (ref R302) (pin 2)))
    (net (code 40) (name /PsuSwitchModule.Switch.2/-5V)
      (node (ref J301) (pin 3))
      (node (ref R301) (pin 2))
      (node (ref R302) (pin 1)))
    (net (code 41) (name "Net-(D301-Pad2)")
      (node (ref D301) (pin 2)))
    (net (code 42) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref D301) (pin 1)))
    (net (code 43) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref C5) (pin 2)))
    (net (code 44) (name /PsuSwitchModule.Switch.2/+15V)
      (node (ref C5) (pin 1))
      (node (ref IC2) (pin 1))
      (node (ref IC2) (pin 8))
      (node (ref R301) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U301) (pin 3))
      (node (ref C20) (pin 1)))
    (net (code 45) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref U301) (pin 8)))
    (net (code 46) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref C6) (pin 2)))
    (net (code 47) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref C20) (pin 2)))
    (net (code 48) (name "Net-(IC2-Pad3)")
      (node (ref IC2) (pin 3)))
    (net (code 49) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref IC2) (pin 4)))
    (net (code 50) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref IC2) (pin 5)))
    (net (code 51) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref C7) (pin 1)))
    (net (code 52) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 53) (name "Net-(C26-Pad1)")
      (node (ref U4) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 54) (name "Net-(C19-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref C19) (pin 1)))
    (net (code 55) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref C19) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref D2) (pin 2)))
    (net (code 56) (name "Net-(IC2-Pad2)")
      (node (ref U4) (pin 4))
      (node (ref IC2) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 57) (name /PsuSwitchModule.Switch.2/DRV_SIG)
      (node (ref R13) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref D301) (pin 3))
      (node (ref IC2) (pin 7))
      (node (ref IC2) (pin 6)))
    (net (code 58) (name /PsuSwitchModule.Switch.2/GND_ISO)
      (node (ref R13) (pin 2)))
    (net (code 59) (name /PsuSwitchModule.Switch.3/-15V)
      (node (ref U401) (pin 11)))
    (net (code 60) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref U401) (pin 8)))
    (net (code 61) (name /PsuSwitchModule.Switch.3/DRV_SIG)
      (node (ref J401) (pin 2)))
    (net (code 62) (name /PsuSwitchModule.Switch.3/-15V)
      (node (ref R402) (pin 2)))
    (net (code 63) (name /PsuSwitchModule.Switch.3/-5V)
      (node (ref R401) (pin 2))
      (node (ref J401) (pin 3))
      (node (ref R402) (pin 1)))
    (net (code 64) (name "Net-(D401-Pad2)")
      (node (ref D401) (pin 2)))
    (net (code 65) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref D401) (pin 1)))
    (net (code 66) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref C9) (pin 2)))
    (net (code 67) (name /PsuSwitchModule.Switch.3/+15V)
      (node (ref IC3) (pin 8))
      (node (ref IC3) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R401) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U401) (pin 3)))
    (net (code 68) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref C10) (pin 2)))
    (net (code 69) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref C22) (pin 2)))
    (net (code 70) (name "Net-(IC3-Pad3)")
      (node (ref IC3) (pin 3)))
    (net (code 71) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref IC3) (pin 4)))
    (net (code 72) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref IC3) (pin 5)))
    (net (code 73) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref C11) (pin 1)))
    (net (code 74) (name "Net-(U6-Pad3)")
      (node (ref U6) (pin 3)))
    (net (code 75) (name "Net-(C27-Pad1)")
      (node (ref U6) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 76) (name "Net-(C21-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref U6) (pin 6))
      (node (ref C21) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref D3) (pin 1)))
    (net (code 77) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref U6) (pin 5))
      (node (ref D3) (pin 2))
      (node (ref C21) (pin 2)))
    (net (code 78) (name "Net-(IC3-Pad2)")
      (node (ref U6) (pin 4))
      (node (ref R14) (pin 2))
      (node (ref IC3) (pin 2)))
    (net (code 79) (name /PsuSwitchModule.Switch.3/DRV_SIG)
      (node (ref R15) (pin 1))
      (node (ref IC3) (pin 6))
      (node (ref IC3) (pin 7))
      (node (ref D401) (pin 3))
      (node (ref C11) (pin 2)))
    (net (code 80) (name /PsuSwitchModule.Switch.3/GND_ISO)
      (node (ref R15) (pin 2)))
    (net (code 81) (name /PsuSwitchModule.Switch.4/-15V)
      (node (ref U501) (pin 11)))
    (net (code 82) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref U501) (pin 8)))
    (net (code 83) (name /PsuSwitchModule.Switch.4/DRV_SIG)
      (node (ref J501) (pin 2)))
    (net (code 84) (name /PsuSwitchModule.Switch.4/-15V)
      (node (ref R502) (pin 2)))
    (net (code 85) (name /PsuSwitchModule.Switch.4/-5V)
      (node (ref R501) (pin 2))
      (node (ref J501) (pin 3))
      (node (ref R502) (pin 1)))
    (net (code 86) (name "Net-(D501-Pad2)")
      (node (ref D501) (pin 2)))
    (net (code 87) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref D501) (pin 1)))
    (net (code 88) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref C13) (pin 2)))
    (net (code 89) (name /PsuSwitchModule.Switch.4/+15V)
      (node (ref C14) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref R501) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref IC4) (pin 8))
      (node (ref U501) (pin 3))
      (node (ref IC4) (pin 1)))
    (net (code 90) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref C14) (pin 2)))
    (net (code 91) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref C24) (pin 2)))
    (net (code 92) (name "Net-(C23-Pad1)")
      (node (ref C23) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref U8) (pin 6)))
    (net (code 93) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 94) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref C15) (pin 1)))
    (net (code 95) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref IC4) (pin 5)))
    (net (code 96) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref IC4) (pin 4)))
    (net (code 97) (name "Net-(IC4-Pad3)")
      (node (ref IC4) (pin 3)))
    (net (code 98) (name "Net-(IC4-Pad2)")
      (node (ref U8) (pin 4))
      (node (ref IC4) (pin 2))
      (node (ref R16) (pin 2)))
    (net (code 99) (name "Net-(C28-Pad1)")
      (node (ref U8) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 100) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref C23) (pin 2))
      (node (ref U8) (pin 5))
      (node (ref D4) (pin 2)))
    (net (code 101) (name /PsuSwitchModule.Switch.4/DRV_SIG)
      (node (ref R17) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref IC4) (pin 7))
      (node (ref IC4) (pin 6))
      (node (ref D501) (pin 3)))
    (net (code 102) (name /PsuSwitchModule.Switch.4/GND_ISO)
      (node (ref R17) (pin 2)))))