(export (version D)
  (design
    (source C:/Development/MliHardware/MLI/Modular/FuseBoardSub/FuseboardSub.sch)
    (date "06/04/2018 11:47:46")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "SUB Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source FuseboardSub.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /VoltMeter4/) (tstamps /59C4F642/)
      (title_block
        (title "SUB Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /VoltMeter3/) (tstamps /59C51A28/)
      (title_block
        (title "SUB Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /VoltMeter2/) (tstamps /59C51FF6/)
      (title_block
        (title "SUB Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /VoltMeter1/) (tstamps /59C5216A/)
      (title_block
        (title "SUB Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "FOR APPROVAL"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J103)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3DA36))
    (comp (ref F101)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A311AB6))
    (comp (ref F102)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314BDF))
    (comp (ref F103)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31508D))
    (comp (ref F104)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A316DCF))
    (comp (ref J102)
      (value FB_OUT)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3187AF))
    (comp (ref J101)
      (value FB_IN)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4D601D))
    (comp (ref J104)
      (value Earth)
      (footprint OAE_Parts:PowerConnectorRound_M3)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC75BC0))
    (comp (ref R202)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F970))
    (comp (ref R201)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A2FE363))
    (comp (ref C201)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A7FE3))
    (comp (ref R203)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A8016))
    (comp (ref U201)
      (value NKE0303SC)
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A7B1FC2))
    (comp (ref R302)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 59C4F970))
    (comp (ref R301)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A2FE363))
    (comp (ref C301)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A7FE3))
    (comp (ref R303)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A8016))
    (comp (ref U301)
      (value NKE0303SC)
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A7B1FC2))
    (comp (ref R402)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 59C4F970))
    (comp (ref R401)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A2FE363))
    (comp (ref C401)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A7FE3))
    (comp (ref R403)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A8016))
    (comp (ref U401)
      (value NKE0303SC)
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A7B1FC2))
    (comp (ref R502)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 59C4F970))
    (comp (ref R501)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A2FE363))
    (comp (ref C501)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A7FE3))
    (comp (ref R503)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A8016))
    (comp (ref U501)
      (value NKE0303SC)
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A7B1FC2)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name Earth) (type passive)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name /VoltMeter2/+VE)
      (node (ref R401) (pin 1))
      (node (ref U501) (pin 1))
      (node (ref F102) (pin 1))
      (node (ref R502) (pin 2)))
    (net (code 2) (name /VoltMeter4/+VE)
      (node (ref R302) (pin 2))
      (node (ref U301) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref F104) (pin 1)))
    (net (code 3) (name /VoltMeter3/+VE)
      (node (ref R301) (pin 1))
      (node (ref F103) (pin 1))
      (node (ref R402) (pin 2))
      (node (ref U401) (pin 1)))
    (net (code 4) (name /VoltMeter4/-VE)
      (node (ref R202) (pin 2))
      (node (ref U201) (pin 1))
      (node (ref J102) (pin 1)))
    (net (code 5) (name "Net-(F104-Pad2)")
      (node (ref F104) (pin 2)))
    (net (code 6) (name Earth)
      (node (ref J104) (pin 1))
      (node (ref J103) (pin 9)))
    (net (code 7) (name /VoltMeter1/+VE)
      (node (ref F101) (pin 1))
      (node (ref J101) (pin 1))
      (node (ref R501) (pin 1)))
    (net (code 8) (name V8)
      (node (ref J103) (pin 5))
      (node (ref C201) (pin 1))
      (node (ref R203) (pin 1))
      (node (ref U201) (pin 5)))
    (net (code 9) (name "Net-(J103-Pad8)")
      (node (ref J103) (pin 8)))
    (net (code 10) (name "Net-(J103-Pad7)")
      (node (ref J103) (pin 7)))
    (net (code 11) (name "Net-(J103-Pad6)")
      (node (ref J103) (pin 6)))
    (net (code 12) (name V7)
      (node (ref J103) (pin 4))
      (node (ref C301) (pin 1))
      (node (ref U301) (pin 5))
      (node (ref R303) (pin 1)))
    (net (code 13) (name V6)
      (node (ref R403) (pin 1))
      (node (ref C401) (pin 1))
      (node (ref U401) (pin 5))
      (node (ref J103) (pin 3)))
    (net (code 14) (name V5)
      (node (ref J103) (pin 2))
      (node (ref C501) (pin 1))
      (node (ref U501) (pin 5))
      (node (ref R503) (pin 1)))
    (net (code 15) (name ARD_GND)
      (node (ref U501) (pin 7))
      (node (ref R503) (pin 2))
      (node (ref C501) (pin 2))
      (node (ref J103) (pin 1))
      (node (ref R303) (pin 2))
      (node (ref U301) (pin 7))
      (node (ref C301) (pin 2))
      (node (ref U201) (pin 7))
      (node (ref C401) (pin 2))
      (node (ref C201) (pin 2))
      (node (ref R203) (pin 2))
      (node (ref U401) (pin 7))
      (node (ref R403) (pin 2)))
    (net (code 16) (name "Net-(F103-Pad2)")
      (node (ref F103) (pin 2)))
    (net (code 17) (name "Net-(F102-Pad2)")
      (node (ref F102) (pin 2)))
    (net (code 18) (name "Net-(F101-Pad2)")
      (node (ref F101) (pin 2)))
    (net (code 19) (name "Net-(R201-Pad2)")
      (node (ref U201) (pin 4))
      (node (ref R202) (pin 1))
      (node (ref R201) (pin 2)))
    (net (code 20) (name "Net-(R301-Pad2)")
      (node (ref R301) (pin 2))
      (node (ref R302) (pin 1))
      (node (ref U301) (pin 4)))
    (net (code 21) (name "Net-(R401-Pad2)")
      (node (ref R402) (pin 1))
      (node (ref R401) (pin 2))
      (node (ref U401) (pin 4)))
    (net (code 22) (name "Net-(R501-Pad2)")
      (node (ref U501) (pin 4))
      (node (ref R501) (pin 2))
      (node (ref R502) (pin 1)))))