(export (version D)
  (design
    (source C:/Development/MliHardware/MLI/Modular/FuseBoard/Fuseboard.sch)
    (date "06/04/2018 11:41:23")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source Fuseboard.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /VoltMeter4/) (tstamps /59C4F642/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /VoltMeter3/) (tstamps /59C51A28/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /VoltMeter2/) (tstamps /59C51FF6/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /VoltMeter1/) (tstamps /59C5216A/)
      (title_block
        (title "Fuseboard with Voltage metering")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source VoltMeter.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J103)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 59C3DA36))
    (comp (ref F101)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A311AB6))
    (comp (ref F102)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A314BDF))
    (comp (ref F103)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31508D))
    (comp (ref F104)
      (value Fuse)
      (footprint OAE_Parts:Fuse_NITD32)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A316DCF))
    (comp (ref J102)
      (value FB_OUT)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A3187AF))
    (comp (ref U101)
      (value TC4051BP)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib Fuseboard-cache) (part TC4051BP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A31B088))
    (comp (ref J101)
      (value FB_IN)
      (footprint Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A4D601D))
    (comp (ref J104)
      (value RJ45)
      (footprint OAE_Parts:RJ45-shielded-Molex)
      (libsource (lib OAE.Parts) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A7DB627))
    (comp (ref J105)
      (value Earth)
      (footprint OAE_Parts:PowerConnectorRound_M3)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC63C39))
    (comp (ref R202)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 59C4F970))
    (comp (ref R201)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A2FE363))
    (comp (ref C201)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A7FE3))
    (comp (ref R203)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A3A8016))
    (comp (ref U201)
      (value " NKE0303SC")
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter4/) (tstamps /59C4F642/))
      (tstamp 5A7B1FC2))
    (comp (ref R302)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 59C4F970))
    (comp (ref R301)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A2FE363))
    (comp (ref C301)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A7FE3))
    (comp (ref R303)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A3A8016))
    (comp (ref U301)
      (value " NKE0303SC")
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter3/) (tstamps /59C51A28/))
      (tstamp 5A7B1FC2))
    (comp (ref R402)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 59C4F970))
    (comp (ref R401)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A2FE363))
    (comp (ref C401)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A7FE3))
    (comp (ref R403)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A3A8016))
    (comp (ref U401)
      (value " NKE0303SC")
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter2/) (tstamps /59C51FF6/))
      (tstamp 5A7B1FC2))
    (comp (ref R502)
      (value 10M)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 59C4F970))
    (comp (ref R501)
      (value 10K)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A2FE363))
    (comp (ref C501)
      (value C)
      (footprint Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A7FE3))
    (comp (ref R503)
      (value R)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A3A8016))
    (comp (ref U501)
      (value " NKE0303SC")
      (footprint OAE_Parts:NKE0303SC)
      (libsource (lib OAE.Parts) (part NME1212DC))
      (sheetpath (names /VoltMeter1/) (tstamps /59C5216A/))
      (tstamp 5A7B1FC2)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part NME1212DC)
      (fields
        (field (name Reference) U)
        (field (name Value) NME1212DC))
      (pins
        (pin (num 1) (name -Vin) (type input))
        (pin (num 4) (name +Vin) (type input))
        (pin (num 5) (name +Vout) (type output))
        (pin (num 7) (name -Vout) (type output))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part RJ45)
      (description "RJ45 connector")
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name Earth) (type passive))))
    (libpart (lib Fuseboard-cache) (part TC4051BP)
      (fields
        (field (name Reference) U)
        (field (name Value) TC4051BP))
      (pins
        (pin (num 1) (name X4) (type passive))
        (pin (num 2) (name X6) (type passive))
        (pin (num 3) (name X) (type passive))
        (pin (num 4) (name X7) (type passive))
        (pin (num 5) (name X5) (type passive))
        (pin (num 6) (name Inh) (type input))
        (pin (num 7) (name VEE) (type power_in))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name C) (type input))
        (pin (num 10) (name B) (type input))
        (pin (num 11) (name A) (type input))
        (pin (num 12) (name X3) (type passive))
        (pin (num 13) (name X0) (type passive))
        (pin (num 14) (name X1) (type passive))
        (pin (num 15) (name X2) (type passive))
        (pin (num 16) (name VDD) (type power_in)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\MliHardware\oae_parts\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical Fuseboard-cache)
      (uri C:\Development\MliHardware\MLI\Modular\FuseBoard\Fuseboard-cache.lib)))
  (nets
    (net (code 1) (name ARD_GND)
      (node (ref J104) (pin 1))
      (node (ref R503) (pin 2))
      (node (ref C501) (pin 2))
      (node (ref C401) (pin 2))
      (node (ref J103) (pin 1))
      (node (ref U401) (pin 7))
      (node (ref R403) (pin 2))
      (node (ref C301) (pin 2))
      (node (ref R203) (pin 2))
      (node (ref U301) (pin 7))
      (node (ref U201) (pin 7))
      (node (ref R303) (pin 2))
      (node (ref C201) (pin 2))
      (node (ref U501) (pin 7))
      (node (ref U101) (pin 7))
      (node (ref U101) (pin 6))
      (node (ref U101) (pin 8)))
    (net (code 2) (name V1)
      (node (ref U501) (pin 5))
      (node (ref R503) (pin 1))
      (node (ref C501) (pin 1))
      (node (ref U101) (pin 13)))
    (net (code 3) (name ARD_VSS)
      (node (ref U101) (pin 16)))
    (net (code 4) (name "Net-(J104-Pad8)")
      (node (ref J104) (pin 8)))
    (net (code 5) (name Earth)
      (node (ref J105) (pin 1))
      (node (ref J103) (pin 9))
      (node (ref J104) (pin 9)))
    (net (code 6) (name "Net-(J104-Pad7)")
      (node (ref J104) (pin 7)))
    (net (code 7) (name "Net-(J104-Pad6)")
      (node (ref J104) (pin 6)))
    (net (code 8) (name V8)
      (node (ref J104) (pin 5))
      (node (ref U101) (pin 4)))
    (net (code 9) (name V7)
      (node (ref U101) (pin 2))
      (node (ref J104) (pin 4)))
    (net (code 10) (name V6)
      (node (ref U101) (pin 5))
      (node (ref J104) (pin 3)))
    (net (code 11) (name V5)
      (node (ref U101) (pin 1))
      (node (ref J104) (pin 2)))
    (net (code 12) (name /VoltMeter1/+VE)
      (node (ref J101) (pin 1))
      (node (ref F101) (pin 1))
      (node (ref R501) (pin 1)))
    (net (code 13) (name "Net-(J103-Pad7)")
      (node (ref J103) (pin 7)))
    (net (code 14) (name V2)
      (node (ref C401) (pin 1))
      (node (ref R403) (pin 1))
      (node (ref U101) (pin 14))
      (node (ref U401) (pin 5)))
    (net (code 15) (name /VoltMeter3/+VE)
      (node (ref R301) (pin 1))
      (node (ref F103) (pin 1))
      (node (ref U401) (pin 1))
      (node (ref R402) (pin 2)))
    (net (code 16) (name V3)
      (node (ref R303) (pin 1))
      (node (ref U101) (pin 15))
      (node (ref U301) (pin 5))
      (node (ref C301) (pin 1)))
    (net (code 17) (name V4)
      (node (ref U101) (pin 12))
      (node (ref R203) (pin 1))
      (node (ref U201) (pin 5))
      (node (ref C201) (pin 1)))
    (net (code 18) (name /VoltMeter4/-VE)
      (node (ref U201) (pin 1))
      (node (ref J102) (pin 1))
      (node (ref R202) (pin 2)))
    (net (code 19) (name COM)
      (node (ref J103) (pin 8))
      (node (ref U101) (pin 3)))
    (net (code 20) (name /VoltMeter2/+VE)
      (node (ref R502) (pin 2))
      (node (ref R401) (pin 1))
      (node (ref U501) (pin 1))
      (node (ref F102) (pin 1)))
    (net (code 21) (name C)
      (node (ref U101) (pin 9))
      (node (ref J103) (pin 6)))
    (net (code 22) (name "Net-(J103-Pad5)")
      (node (ref J103) (pin 5)))
    (net (code 23) (name B)
      (node (ref U101) (pin 10))
      (node (ref J103) (pin 4)))
    (net (code 24) (name ARD_VDD)
      (node (ref J103) (pin 3)))
    (net (code 25) (name A)
      (node (ref J103) (pin 2))
      (node (ref U101) (pin 11)))
    (net (code 26) (name /VoltMeter4/+VE)
      (node (ref U301) (pin 1))
      (node (ref R302) (pin 2))
      (node (ref F104) (pin 1))
      (node (ref R201) (pin 1)))
    (net (code 27) (name "Net-(F101-Pad2)")
      (node (ref F101) (pin 2)))
    (net (code 28) (name "Net-(F102-Pad2)")
      (node (ref F102) (pin 2)))
    (net (code 29) (name "Net-(F103-Pad2)")
      (node (ref F103) (pin 2)))
    (net (code 30) (name "Net-(F104-Pad2)")
      (node (ref F104) (pin 2)))
    (net (code 31) (name "Net-(R201-Pad2)")
      (node (ref R202) (pin 1))
      (node (ref U201) (pin 4))
      (node (ref R201) (pin 2)))
    (net (code 32) (name "Net-(R301-Pad2)")
      (node (ref U301) (pin 4))
      (node (ref R302) (pin 1))
      (node (ref R301) (pin 2)))
    (net (code 33) (name "Net-(R401-Pad2)")
      (node (ref U401) (pin 4))
      (node (ref R401) (pin 2))
      (node (ref R402) (pin 1)))
    (net (code 34) (name "Net-(R501-Pad2)")
      (node (ref U501) (pin 4))
      (node (ref R501) (pin 2))
      (node (ref R502) (pin 1)))))