(export (version D)
  (design
    (source C:/Development/mlihardware/MLI/Modular/HBridgePowerModule/HBridgePowerModule.sch)
    (date "10/04/2018 13:02:44")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source HBridgePowerModule.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/SinglePowerSwitch 1/") (tstamps /59AEDD49/)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/)
      (title_block
        (title "MLI HBridge Power Board")
        (company "Enertechnos Ltd")
        (rev "Release 0.2")
        (date 2018-04-05)
        (source SinglePowerSwitch.sch)
        (comment (number 1) (value "For Approval"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J6)
      (value AC_OUT)
      (footprint OAE_Parts:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AEFF90))
    (comp (ref J7)
      (value AC_OUT)
      (footprint OAE_Parts:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AFA697))
    (comp (ref J2)
      (value POS_IN)
      (footprint OAE_Parts:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A28227C))
    (comp (ref J3)
      (value NEG_IN)
      (footprint OAE_Parts:PowerConnectorRound)
      (libsource (lib conn) (part Conn_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A28246C))
    (comp (ref IC101)
      (value CAS_50-NP)
      (footprint CAS_NP)
      (datasheet http://www.lem.com/docs/products/lts_15-np.pdf)
      (libsource (lib OAE.Parts) (part CAS_50-NP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A344E30))
    (comp (ref J101)
      (value Conn_01x03)
      (footprint Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A34A7A6))
    (comp (ref Q1)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE014))
    (comp (ref C1)
      (value C)
      (footprint OAE_Parts:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 59AEE01D))
    (comp (ref J201)
      (value Conn_01x03)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names "/SinglePowerSwitch 1/") (tstamps /59AEDD49/))
      (tstamp 5AC4E93A))
    (comp (ref Q2)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE014))
    (comp (ref C2)
      (value C)
      (footprint OAE_Parts:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 59AEE01D))
    (comp (ref J301)
      (value Conn_01x03)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names "/SinglePowerSwitch 2/") (tstamps /59AEEDCB/))
      (tstamp 5AC4E93A))
    (comp (ref Q3)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE014))
    (comp (ref C3)
      (value C)
      (footprint OAE_Parts:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 59AEE01D))
    (comp (ref J401)
      (value Conn_01x03)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names "/SinglePowerSwitch 3/") (tstamps /59AEEFC6/))
      (tstamp 5AC4E93A))
    (comp (ref Q4)
      (value RFP12N10L)
      (footprint TO_SOT_Packages_THT:TO-247_TO-3P_Vertical)
      (datasheet https://componentsearchengine.com/Datasheets/2/RFP12N10L.pdf)
      (fields
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (libsource (lib OAE.Parts) (part RFP12N10L))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE014))
    (comp (ref C4)
      (value C)
      (footprint OAE_Parts:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib device) (part C))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 59AEE01D))
    (comp (ref J501)
      (value Conn_01x03)
      (footprint OAE_Parts:TerminalBlock_Altech_AK300-3_P5.00mm)
      (libsource (lib conn) (part Conn_01x03))
      (sheetpath (names "/SinglePowerSwitch 4/") (tstamps /59AEEFCD/))
      (tstamp 5AC4E93A)))
  (libparts
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib OAE.Parts) (part CAS_50-NP)
      (description "LEM Closed Loop Current Sensor, 50A Nominal")
      (docs http://www.lem.com/docs/marketing/LEM%20Leaflet%20CAS%20CASR%20CKSR.pdf)
      (footprints
        (fp CAS_NP))
      (fields
        (field (name Reference) IC)
        (field (name Value) CAS_50-NP)
        (field (name Footprint) CAS_NP)
        (field (name Datasheet) http://www.lem.com/docs/products/lts_15-np.pdf))
      (pins
        (pin (num 1) (name "IN(1)") (type unspc))
        (pin (num 2) (name "IN(2)") (type unspc))
        (pin (num 3) (name "IN(3)") (type unspc))
        (pin (num 8) (name "OUT(3)") (type unspc))
        (pin (num 9) (name "OUT(2)") (type unspc))
        (pin (num 10) (name "OUT(3)") (type unspc))
        (pin (num 11) (name Vout) (type unspc))
        (pin (num 12) (name GND) (type unspc))
        (pin (num 13) (name +5V) (type unspc))))
    (libpart (lib conn) (part Conn_01x01)
      (description "Generic connector, single row, 01x01")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib conn) (part Conn_01x03)
      (description "Generic connector, single row, 01x03")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib OAE.Parts) (part RFP12N10L)
      (fields
        (field (name Reference) Q)
        (field (name Value) RFP12N10L)
        (field (name Footprint) TO254P470X1016X2167-3P)
        (field (name Datasheet) https://www.fairchildsemi.com/datasheets/RF/RFP12N10L.pdf)
        (field (name Description) "N-channel logicFET,RFP12N10L 12A 100V")
        (field (name Manufacturer_Name) "Fairchild Semiconductor")
        (field (name Manufacturer_Part_Number) RFP12N10L)
        (field (name Supplier_Name) RS)
        (field (name "RS Part Number") 0295703)
        (field (name Height) 4.7))
      (pins
        (pin (num 1) (name G) (type unspc))
        (pin (num 2) (name D) (type unspc))
        (pin (num 3) (name S) (type unspc))
        (pin (num 4) (name "D__(TAB)") (type unspc)))))
  (libraries
    (library (logical OAE.Parts)
      (uri C:\Development\multilevelinverter\Hardware\PartsLibraries\OAE.Parts.lib))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name ARD_5V)
      (node (ref IC101) (pin 13))
      (node (ref J101) (pin 3)))
    (net (code 2) (name ARD_CUR)
      (node (ref J101) (pin 1))
      (node (ref IC101) (pin 11)))
    (net (code 3) (name "/SinglePowerSwitch 1/DRAIN")
      (node (ref Q2) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref IC101) (pin 8))
      (node (ref IC101) (pin 9))
      (node (ref IC101) (pin 10)))
    (net (code 4) (name "Net-(IC101-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref IC101) (pin 1))
      (node (ref IC101) (pin 2))
      (node (ref IC101) (pin 3)))
    (net (code 5) (name DRV_GATE_1)
      (node (ref Q1) (pin 1))
      (node (ref J201) (pin 2)))
    (net (code 6) (name ARD_GND)
      (node (ref IC101) (pin 12))
      (node (ref J101) (pin 2)))
    (net (code 7) (name GND_ISO_3)
      (node (ref J501) (pin 3))
      (node (ref J401) (pin 3))
      (node (ref Q3) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref Q4) (pin 3)))
    (net (code 8) (name DRV_GATE_3)
      (node (ref J401) (pin 2))
      (node (ref Q3) (pin 1)))
    (net (code 9) (name GND_ISO_2)
      (node (ref Q4) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref Q2) (pin 3))
      (node (ref C4) (pin 2))
      (node (ref J301) (pin 3)))
    (net (code 10) (name DRV_GATE_2)
      (node (ref J301) (pin 2))
      (node (ref Q2) (pin 1)))
    (net (code 11) (name GND_ISO_1)
      (node (ref Q3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref J201) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref C1) (pin 1)))
    (net (code 12) (name DRV_GATE_4)
      (node (ref Q4) (pin 1))
      (node (ref J501) (pin 2)))
    (net (code 13) (name "Net-(J201-Pad1)")
      (node (ref J201) (pin 1)))
    (net (code 14) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4)))
    (net (code 15) (name "Net-(J301-Pad1)")
      (node (ref J301) (pin 1)))
    (net (code 16) (name "Net-(Q2-Pad4)")
      (node (ref Q2) (pin 4)))
    (net (code 17) (name "Net-(J401-Pad1)")
      (node (ref J401) (pin 1)))
    (net (code 18) (name "Net-(Q3-Pad4)")
      (node (ref Q3) (pin 4)))
    (net (code 19) (name "Net-(J501-Pad1)")
      (node (ref J501) (pin 1)))
    (net (code 20) (name "Net-(Q4-Pad4)")
      (node (ref Q4) (pin 4)))))